;; For ITS network stuff, the following parameters are defined:
;
; NETP - General network code (net independent, both CHAOS, NCP, TCP, etc)
; INETP - Internet Protocol code.  Must have IMPP or some other device.
; NCPP - Include NCP code (IMPP must be on)
; TCPP - Include TCP code (INETP must be on)

; CHAOSP - Include CHAOS net code
; - other CHAOS stuff, all independent of internet stuff.

NE%UNT==:<1_32.>	; Escape bit indicating non-Internet address
NW$BYT==:301400		; Byte pointer to network number (approx!)	
NE%STR==:<1_33.>	; Escape bit indicating string-type address

DEFINE HOSTN A,B,C,D
.RADIX 10.,<<<<<A_8>+B>_8>+C>_8>+D,!TERMIN

; HOSTS3 full word network # values for certain networks

NW%CHS==:<NE%UNT+<7_24.>>
NW%ARP==:<12_24.>
NW%LCS==:<22_24.>
NW%AI==:HOSTN 128,52,0,0

DEFINE GETNET AC,(ADDR)		; Macro to extract net number
IFNB [ADDR] MOVE AC,ADDR
	TLNN AC,(17_32.)	; Check for non-Internet type addrs
	 TLNN AC,(1_31.)	;  Internet address, see if class A net
	  TDZA AC,[77,,-1]	;   Unternet or class A, zap low 3 octets
	TLNN AC,(1_30.)		; Class B or C, see which.
	 TRZA AC,177777		;  Class B network, zap low 2 octets
	  TRZ AC,377		;   Class C net, only zap 1 low octet
TERMIN

;;; Misc defs
CALL==<PUSHJ P,>
RET==<POPJ P,>
CALRET==<JRST>

	OVHMTR NET

IFN IMPP,[	; ARPAnet IMP interface code
IFN KAIMP,[
$INSRT IMPOLD
]
IFN KSIMP,[
$INSRT IMP
]
]

	OVHMTR NET

IFN NCPP,[	; Old Arpanet NCP protocol code
$INSRT NCP
]
	OVHMTR NET

IFN INETP,[	; Internet Protocol code
$INSRT INET
]

	OVHMTR NET

IFN TCPP,[	; Transmission Control Protocol code
$INSRT TCP
]

	OVHMTR UUO

IFN CHAOSP,[	; CHAOSnet interface and protocol code
$INSRT CHAOS
]
	OVHMTR UUO

SUBTTL	General Network System Calls

; .CALL NETRFC - Get a pending Request For Connection for a specific network
;	Arg 1 - SIXBIT name of network
;	Arg 2 - optional network-dependent arg
;		(for CHAOS, points to packet buffer)
;	Val 1 - network-dependent value
;		For TCP and ARPNCP, this is <id>,,<port/socket #>
; Control bits:
	%NQREF==:1	; Arg 2 is previously returned identifier,
			; refuse connection and flush from queue.

NETRFC:	MOVE C,CTLBTS(U)	; Set up control bits in C
IFN TCPP,[
	CAMN A,[SIXBIT /TCP/]
	 JRST TCPRQ
]
IFN CHAOSP,[
	CAMN A,[SIXBIT /CHAOS/]
	 JRST [	TRNE C,%NQREF	; If refusing conn,
		 JRST OPNL12	; Ignore, can't handle yet.  "Mode not avail"
		CAIGE W,2	; Must have a 2nd arg
		 JRST OPNL30	; "Too few args"
		MOVE A,B	; Fake out old CHAOSQ call
		JRST CHAOSQ]
]
IFN NCPP,[	; NOP for now
;	CAMN A,[SIXBIT /ARPNCP/]
;	 JRST IMPRQ
]
	JRST OPNL33		; No match, say "meaningless args".

; .CALL NETBLK	- Wait for net channel state to change, or time out.
;	Arg 1 - Channel (comes in R)
;	Arg 2 - Undesired state
;	Arg 3 - Optional timeout (as in .SLEEP), written back unless immediate
;	Val 1 - New state
;	Val 2 - Time left

NETBLK:	HRRZ T,(R)		; Get IOCHNM RH = device index
	HLRZ I,(R)		; Get LH = often connection index
IFN NCPP,[
	CAIL T,NETDUI
	 CAILE T,NETDBO
	  CAIA
	   JRST [MOVE T,[HRRZ A,IMSOC4]
		JRST NETBLI]
] ;NCPP
IFN CHAOSP,[
	CAIE T,CHAIDN
	 CAIN T,CHAODN
	  JRST [MOVE T,[HRRZ A,CHSSTA]
		JRST NETBLI]
] ;CHAOSP
IFN TCPP,[
	CAIN T,TCPDUI
	 JRST [	MOVE T,[HLRZ A,XBSTAU]
		JRST NETBLI]
	CAIN T,TCPDUO
	 JRST [	MOVE T,[HRRZ A,XBSTAU]
		JRST NETBLI]
] ;TCP
	JRST OPNL34	; Not a net chan, say "Wrong Type Device".


; T/ Instruction to XCT (not indexed) to get state in A
; Entry at NETBLI adds (I) to the instruction.

NETBLI:	ADDI T,(I)		; Provide "index" for instruction.
NETBL0:	CAIGE W,3
	 JRST [	HRLOI D,377777	; No time given, use infinity
		JRST NETBL4 ]
	TLNE C,1000		; Skip if pointer rather than immediate
	 JRST [	HRRZ D,C	; Get immediate time
		ADD D,TIME
		JRST NETBL4 ]
	XCTR XRW,[MOVES D,(C)]	; Get time, check writeability
	JUMPGE D,[ MOVNS D	; Relative time, make negative absolute
		   SUB D,TIME
		   JRST .+1 ]
	UMOVEM D,(C)		; Store back absolute time
	MOVNS D			; Make positive
NETBL4:	MOVEM D,AC0S+D(U)	; Save absolute time to wait until
	MOVEM B,AC0S+B(U)	; Save undesired state
	PUSHJ P,NETBL2		; Skip if state change or timeout
	 PUSHJ P,UFLS
	MOVE B,D
	SUB B,TIME		; How much used?
	XCT T			; Return new state
	JRST POPJ1

NETBL2:	XCT T			; Get current state
	CAME A,AC0S+B(U)	; Skip if still match
	 JRST POPJ1
	MOVE A,AC0S+D(U)	; Timeout time
	CAMG A,TIME
	 AOS (P)
	POPJ P,

SUBTTL Utilities - CVTH2A, CVTH3A


; CVH2NA - Convert network host address in A to HOSTS2 format.
;	A/ net address (any format)
; Returns A

CVH2NA:	PUSH P,B
	LDB B,[301400,,A]	; Get high 12 bits of net address
	CAIGE B,70		; If less than lowest HOSTS2-fmt value
	 JUMPN B,CVH2N3		; then must be HOSTS3, go convert.
	CAIL B,1000		; If any of high 3 bits set,
	 JRST CVH2N3		;  then it's a HOSTS3 strange-fmt number.
	JUMPN B,CVH2N2
	CAILE A,377		; Zero network, so must be ARPA net
	 JRST CVH2N1		; Not just 8 bits, just add net number.

	; Old-style 8-bit Arpanet host number
	LSHC A,-6.
	ROT B,6.
	DPB B,[112000,,A]
CVH2N1:	TLO A,(12_33)
	JRST POPBJ

	; Probably HOSTS2 format number
CVH2N2:	JRST POPBJ		; For now, that's good enough.

	; HOSTS3 format number, convert it.
CVH2N3:	CAIN B,12		; Arpa net?
	 JRST [	LSHC A,-16.
		ANDI A,377
		ROT B,16.
		DPB B,[112000,,A]
		TLO A,(12_33)
		JRST POPBJ]
	CAIN B,7+<NE%UNT_-24.>	; Chaos net?
	 JRST [	ANDI A,177777	; Yup, fix it up.
		TLO A,(7_33)
		JRST POPBJ]
	CAIN B,22		; LCS net?
	 JRST [	LSHC A,-8.
		ANDI A,-1
		LSH A,2
		LSHC A,8.
		TLO A,(22_33)
		JRST POPBJ]

	; Not a known net, but try to do something plausible.
	ANDCM A,[-1_24.]	; Preserve low 24 bits
	DPB B,[331100,,A]	; put net # into HOSTS2 field.
	POP P,B
	RET

; CVH3NA - Convert network host address in A to HOSTS3 (Internet) format.
;	A/ net address (any format)
; Returns A

CVH3NA:	PUSH P,B
	LDB B,[301400,,A]	; Get high 12 bits of net address
	CAIGE B,70		; If less than lowest HOSTS2 value,
	 JUMPN B,CVH3N3		; it's already HOSTS3 format!  (unless zero)
	CAIL B,1000		; If any of high 3 bits were set,
	 JRST CVH3N3		;  it must be a HOSTS3 strange-fmt addr.
	JUMPN B,CVH3N2		; If not zero, then must assume HOSTS2 fmt.

	; Old-format 8-bit Arpanet host number, or HOSTS2 with zero net.
	CAILE A,377
	 JRST CVH3N6	; If greater than 8 bits, assume HOSTS2, zero net.
	LSHC A,-6	; Put 10 bits spacing between host/imp #s.
	LSH B,-<2+8.>
	LSHC A,<2+8.+6>
	TLO A,(12_24.)	; and add ARPA network number.
	JRST CVH3N3

	; HOSTS2 format number
CVH3N2:	TRZE B,7	; Zap low 3 bits to ensure correct comparison
	 JRST CVH3N5	; If any were set, can't be Chaosnet.
	CAIN B,7_3		; Chaos net?
	 JRST [	ANDI A,177777		; Yes, kill all but bottom 16 bits
		TLO A,(NE%UNT+<7_24.>)	; Add Chaos net #
		JRST CVH3N3]
CVH3N5:	CAIN B,12_3		; Arpa net?
CVH3N6:	 JRST [	LSHC A,-9.
		ANDI A,177777
		ROT B,9.
		DPB B,[201000,,A]
		TLO A,(12_24.)
		JRST CVH3N3]
	CAIN B,22_3		; LCS net?
	 JRST [	LSHC A,-8.
		LSH A,-2
		ANDI A,377
		LSHC A,-8.
		TLO A,(22_24.)
		JRST CVH3N3]

	; No match, assume it's HOSTS3.

CVH3N3:	POP P,B
	RET

;.CALL STYNET
;ARG 1 - STY CHANNEL
;ARG 2 - NET INPUT CHANNEL TO CONNECT STY OUTPUT TO, OR -1 TO DISCONNECT
;ARG 3 - NET OUTPUT CHANNEL TO CONNECT STY INPUT TO
;ARG 4 - CHARS TO SEND WHEN OUTPUT .RESET HAPPENS ON STY'S TTY
;	   UP TO 3 8-BIT CHARACTERS, LEFT JUSTIFIED.

NSTYNT:	TLNN R,%CLSST
	 JRST OPNL34		;1ST ARG NOT A STY CHANNEL.
	HLRZ I,(R)		;GET TTY # OF STY
	HRRES B			;ALLOW IMMEDIATE -1
	JUMPGE B,NSTYN2		;JUMP IF CONNECTING.
	PUSHJ P,NSTYN0		;DISCONNECT
	 JRST OPNL41		;WASN'T CONNECTED
	JRST POPJ1

;VARIOUS ROUTINES CALL HERE WITH THE TTY# OF A STY IN I, TO DISCONNECT THE
; STY FROM THE NETWORK.  NOTE THIS ROUTINE MUST NOT CHANGE U AND MUST NOT
; LSWCLR, SINCE IT COULD BE CALLED FROM IODCL VIA STYCLS OR NETCLS.

NSTYN0:	MOVSI B,%SSNET		;DISCONNECTING BOTH SIDES.
	CONO PI,NETOFF
	TDNN B,STYSTS-NFSTTY(I)
	 POPJ P,			;THIS STY NOT CONNECTED?
	ANDCAB B,STYSTS-NFSTTY(I)	;MARK AS NO LONGER CONNECTED
	MOVE C,STYNTL-NFSTTY(I)		;REMOVE THIS STY FROM ACTIVATION LIST
	MOVEI D,STYNTA-STYNTL+NFSTTY
NSTYN1:	CAMN I,STYNTL-NFSTTY(D)		;FIND THE STY THAT POINTS TO THIS ONE,
	 MOVEM C,STYNTL-NFSTTY(D)	;AND PATCH US OUT OF THE LIST.
	SKIPE D,STYNTL-NFSTTY(D) 	;SEARCH WHOLE LIST TILL FIND WHO POINTS TO US.
	 JRST NSTYN1
	SETOB C,STYNTL-NFSTTY(I)
	EXCH C,STYNTI-NFSTTY(I)	;MARK THIS STY AS HAVING NO CONNECTION, GET SOCKET INDICES
IFN CHAOSP,[
	TLNE B,%SSCHA
	 JRST [	MOVSI B,%SSCHA	;DISCONNECT FROM CHAOS NET
		ANDCAM B,STYSTS-NFSTTY(I)
		MOVSI B,%CFSTY
		TDNN B,CHSSTA(C)
		 JRST 4,.	;CHAOS DOESN'T THINK IT WAS CONNECTED?
		ANDCAM B,CHSSTA(C)
		JRST NETOJ1 ]
];CHAOSP
IFN TCPP,[
	TLNE B,%SSTCP
	 JRST [	MOVSI B,%SSTCP		; Disconnect from TCP connection
		ANDCAM B,STYSTS-NFSTTY(I)	; Flush STY's "connect" bit
		MOVSI B,(XB%STY)
		TDNN B,XBUSER(C)	; Make sure TCP thinks connected
		 BUG			; It isn't??
		ANDCAM B,XBUSER(C)
		JRST NETOJ1]
] ;TCPP
IFN NCPP,[
	MOVE B,[40000,,777]
	TDNN B,IMSOC5(C)
	 JRST 4,.		;SOCKET DOESN'T THINK IT WAS CONNECTED?
	ANDCAM B,IMSOC5(C)	;AND MARK SOCKETS WE WERE CONNECTED TO AS DISCONNECTED
	MOVSS C
	TDNN B,IMSOC5(C)
	 JRST 4,.		;SOCKET DOESN'T THINK IT WAS CONNECTED?
	ANDCAM B,IMSOC5(C)
	JRST NETOJ1
] ;NCPP
.ELSE	BUG

; Here to set up STY connection.

NSTYN2:	MOVE Q,I		;SAVE TTY # OF STY
	MOVEI E,1
	MOVE A,B		;DECODE THE NETWORK INPUT CHANNEL
	JSP T,CHNDCD
	HRRZ A,(R)
IFN CHAOSP,[
	CAIE A,CHAIDN
	 CAIN A,CHAODN
	  JRST [ HLRZ I,(R)	;CONNECT TO CHAOS NET
		 CONO PI,NETOFF
		 MOVSI B,%CFSTY
		 TDNE B,CHSSTA(I)
		  JRST OPNL23	;ALREADY CONNECTED, FILE LOCKED
		 MOVSI C,%SSNET+%SSCHA
		 TDNE C,STYSTS-NFSTTY(Q)
		  JRST OPNL23	;ALREADY CONNECTED, FILE LOCKED
		 IORM B,CHSSTA(I)	;OK, HOOK UP
		 DPB Q,[$CFTTN,,CHSSTA(I)]
		 JRST NSTYN3 ]
];CHAOSP
IFN TCPP,[
	CAIE A,TCPDUI
	 CAIN A,TCPDUO
	  JRST [HLRZ I,(R)	; Connect to TCP, get TCB index
		CONO PI,NETOFF
		MOVSI B,(XB%STY)
		TDNE B,XBUSER(I)
		 JRST OPNL23	; TCB Already connected, say "File Locked"
		MOVSI C,%SSNET+%SSTCP
		TDNE C,STYSTS-NFSTTY(Q)
		 JRST OPNL23	; STY already connected, say "File Locked"
		DPB Q,[XB$STY (I)]	; Store TTY # to connect TCB.
		JRST NSTYN3]
] ;TCPP
IFN NCPP,[
	JSP T,NETCHK	;TEST LEGALITY;  OPNL IF LOSES
	TDNE E,IMSOC2(I)
	 JRST OPNL2		;WRONG DIRECTION IF IT'S AN OUTPUT CHANNEL
	MOVE B,I		;SAVE INPUT IMSOC INDEX
	MOVE A,C		;DECODE OUTPUT CHANNEL
	JSP T,CHNDCD
	JSP T,NETCHK
	TDNN E,IMSOC2(I)
	 JRST OPNL2		;WRONG DIRECTION IF INPUT SOCKET
	CONO PI,NETOFF
	MOVE E,[40000,,777]
	TDNN E,IMSOC5(B)	;ERROR IF EITHER CHANNEL ALREADY CONNECTED
	 TDNE E,IMSOC5(I)
	  JRST OPNL23		;"FILE LOCKED"
	MOVSI C,%SSNET
	TDNE C,STYSTS-NFSTTY(Q)
	 JRST OPNL23		;SIMILAR ERROR IF STY ALREADY CONNECTED
	HRR E,Q			;GET 40000,,TTY #
	IORM E,IMSOC5(I)
	IORM E,IMSOC5(B)	;MARK SOCKETS AS CONNECTED
] ;NCPP

NSTYN3:	SKIPGE STYNTL-NFSTTY(Q)	;HALT IF STY'S VARS ARE NOT CORRECT FOR A 
	 SKIPL STYNTI-NFSTTY(Q)	;NON-CONNECTED STY.
	  JRST 4,.
	IORM C,STYSTS-NFSTTY(Q)	;ALL ERROR CAUGHT, SO MARK STY CONNECTED.
	HRL B,I			;PUT INPUT IMSOC IDX,, OUTPUT IMSOC IDX
	MOVSM B,STYNTI-NFSTTY(Q) ;INTO THE STY
	TRZ D,7777		;STORE THE OUTPUT RESET CHARACTERS - AT MOST 3
	MOVEM D,STYORC-NFSTTY(Q)

	;ACTIVATE IN CASE HAS UNREAD INPUT
IFN NCPP,[
	TLNN C,%SSCHA+%SSTCP
	 PUSHJ P,IMPUIN
] ;NCPP
IFN CHAOSP,[
	TLNE C,%SSCHA
	 PUSHJ P,CHINTI
];CHAOSP
IFN TCPP,[
	TLNE C,%SSTCP
	 PUSHJ P,TCPUII
] ;TCPP
	JRST NETOJ1

SUBTTL	Clock interrupt level code

; NETCLK - Slow net clock.  Called at clock level every 1/2 sec.
;	Can clobber all ACs

NETCLK:
IFN CHAOSP, PUSHJ P,CHACLK	; Run Chaos net 1/2-second clock
IFN TCPP, PUSHJ P,TCPCLK	; Run TCP 1/2-sec clock
	SETCMB A,NETCL1		; Flip the 1 sec switch
	JUMPE A,CPOPJ		; Return unless time for 1-sec clock
IFN INETP,CALL IPFCLK		; Run IP reassembly timeout every 1 sec
	RET
EBLK
NETCL1:	0		; Flip-flop to get 1-sec ticks
BBLK

; STYNTC - Called at clock level every 1/60 sec to process all
;	necessary transfers of data between STYs and associated
;	net connections

STYNTC:	CONO PI,NETOFF
	SKIPN I,STYNTA		;GET HEAD OF ACTIVATE LIST
	 JRST NETONJ		;EMPTY
	SETZM STYNTA		;COPY LIST IN CASE A STY IS PUT BACK ON
	CONO PI,NETON
STYNT7:	MOVE A,STYNTL-NFSTTY(I)	;GET NEXT ON LIST
	MOVEM A,STYNTB		;SAVE FOR NEXT TIME AROUND LOOP
	SETOM STYNTL-NFSTTY(I)	;THIS ONE IS NO LONGER ON ACTIVATE LIST
	MOVE A,STYSTS-NFSTTY(I)
	TLNN A,%SSNET
	 JRST 4,.		;STY CLAIMS NOT TO BE CONNECTED??
	MOVE R,I		;SAVE TTY #

IFN CHAOSP,[
	TLNE A,%SSCHA
	 JRST STYCHA		;CONNECTED TO CHAOS NET
];CHAOSP
IFN TCPP,[
	TLNE A,%SSTCP
	 JRST STYTCP
] ;TCPP
IFN NCPP,[
	JRST STYNCP
];NCPP

STYNT8:	SKIPE I,STYNTB		;GET NEXT STY FROM COPIED ACTIVATION LIST
	 JRST STYNT7
	POPJ P,

;SUBROUTINE TO STANDARDIZE HOST NUMBER, OPNL25 IF NO GOOD
;PROCESSES HOST NUMBER IN T, MUNGS H, CALLED BY JSP J,STDHST
STDHST:
IFN 1,[
	EXCH A,T
	CALL CVH3NA		; Convert # to HOSTS3 fmt
	EXCH A,T
	LDB H,[301400,,T]	; Get high 12 bits (net #)
	CAIE H,12		; Should be ARPA net
	 JRST OPNL25
	TDZ T,[NW%ARP+<377_8.>]	; Flush the net # and logical host field
	JRST (J)
] ;IFN 1
IFN 0,[
	LDB H,[331000,,T]	;GET NETWORK-NUMBER FIELD
	CAIE H,12		;ONLY 12 OR 0 IS ACCEPTABLE
	 JUMPN H,OPNL25
	TDNE T,[400600,,400]	;MAKE SURE OTHER RANDOM BITS AREN'T ON
	 JRST OPNL25
	TLZ T,777000		;CLEAR NETWORK NUMBER
	JUMPE T,OPNL25		;0 IS NOT ACCEPTABLE
	CAIL T,400		;SKIP IF OLD-STYLE HOST NUMBER
	 JRST (J)
	LDB H,[060200,,T]	;GET HOST FIELD
	ANDI T,77		;GET IMP FIELD
	EXCH H,T
	DPB H,[112000,,T]	;RECOMBINE
	JRST (J)
] ;IFN 0
