(footprint "R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal_OverLapping"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
	(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
	(property "Reference" "R16"
		(at 5.08 0.029 0)
		(layer "F.SilkS")
		(uuid "0544b029-1f5c-45e9-9d02-52b7f2b9fd71")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "10K"
		(at 5.10884 -2.496 0)
		(layer "F.Fab")
		(uuid "cee98caa-4334-4fe9-b297-b86fbb068a43")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e7251269-2859-4a52-9676-b09f5d69e6ad")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c1afcfd9-b5de-47a9-8f4e-f192e96a507e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "bb0f12eb-0c3b-45c2-8e36-474f771a8f58")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.05 -1.5)
		(end -1.05 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "62485945-317b-4a3d-a4c8-7629b09180dc")
	)
	(fp_line
		(start -1.05 1.5)
		(end 11.21 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3d788273-20b3-4916-9e14-3741a6808229")
	)
	(fp_line
		(start 1.04 0)
		(end 1.81 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b54750a9-6d45-4658-a0e2-1a52cbd1f53a")
	)
	(fp_line
		(start 1.81 -1.37)
		(end 1.81 1.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "420e7532-8c87-4562-883c-4891ccc2f724")
	)
	(fp_line
		(start 1.81 1.37)
		(end 8.35 1.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "db00b380-7fc0-4f56-894b-262dfe118c8e")
	)
	(fp_line
		(start 8.35 -1.37)
		(end 1.81 -1.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "210b3e73-d5c6-4cfc-ae20-7954fe8478bf")
	)
	(fp_line
		(start 8.35 1.37)
		(end 8.35 -1.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5c8217a2-c06b-4fb9-bf96-945ac1024e7c")
	)
	(fp_line
		(start 9.12 0)
		(end 8.35 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0a828455-583f-4ff1-822f-ec74b76970e1")
	)
	(fp_line
		(start 11.21 -1.5)
		(end -1.05 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9761cd0b-bf27-4358-bbf3-1fc82c427c2b")
	)
	(fp_line
		(start 11.21 1.5)
		(end 11.21 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5ae8c3fb-2be7-40bc-82e4-394ce7c9bd5f")
	)
	(fp_line
		(start 0 0)
		(end 1.93 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "04437735-a0f4-42f0-bacd-a3b4790f26df")
	)
	(fp_line
		(start 1.93 -1.25)
		(end 1.93 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "be6fbd5e-ef29-4c22-a854-3f19a045028d")
	)
	(fp_line
		(start 1.93 1.25)
		(end 8.23 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1819160e-80be-4066-8b5c-d6a93f828052")
	)
	(fp_line
		(start 8.23 -1.25)
		(end 1.93 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0c6d6df1-edca-4ceb-a220-b915c44f75f6")
	)
	(fp_line
		(start 8.23 1.25)
		(end 8.23 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6ac4d9cb-2850-4d71-8762-5a15f1887aa2")
	)
	(fp_line
		(start 10.16 0)
		(end 8.23 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "083d617c-7085-46d8-a3dd-4cdf8840f008")
	)
	(fp_text user "${REFERENCE}"
		(at 5.08 0 0)
		(layer "F.Fab")
		(uuid "d5ee6142-652f-40ab-b4f6-2e44fc32eadf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d0ebc173-57c0-465e-84f4-f3ad903debb7")
	)
	(model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
