(module EXP_Header (layer F.Cu) (tedit 60FDFAB4)
  (fp_text reference P2 (at -1 11) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value EXP-Connector (at -2.733 -3.875) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 1 (at -3 7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 48 (at -3 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 24 (at 61 7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 25 (at 61 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 69.52 9.5) (end 69.52 -3) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.1 9.49) (end -11.1 -3.01) (layer F.SilkS) (width 0.12))
  (fp_line (start -11.1 -3.01) (end 69.52 -3) (layer F.SilkS) (width 0.12))
  (fp_line (start 69.52 9.5) (end -11.1 9.49) (layer F.SilkS) (width 0.12))
  (fp_poly (pts (xy 69.52 -3) (xy 66.52 -3) (xy 69.52 0)) (layer F.SilkS) (width 0.1))
  (fp_poly (pts (xy -11.1 -3.01) (xy -11.1 -0.01) (xy -8.1 -3.01)) (layer F.SilkS) (width 0.1))
  (pad 48 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 47 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 46 thru_hole circle (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 45 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 44 thru_hole circle (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 43 thru_hole circle (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 42 thru_hole circle (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 41 thru_hole circle (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 40 thru_hole circle (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 39 thru_hole circle (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 38 thru_hole circle (at 25.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 37 thru_hole circle (at 27.94 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 36 thru_hole circle (at 30.48 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 35 thru_hole circle (at 33.02 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 34 thru_hole circle (at 35.56 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 33 thru_hole circle (at 38.1 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 32 thru_hole circle (at 40.64 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 31 thru_hole circle (at 43.18 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 45.72 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 48.26 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 50.8 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 53.34 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 55.88 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 58.42 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.54 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5.08 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 7.62 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 10.16 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 12.7 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 15.24 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 17.78 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 20.32 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 22.86 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 25.4 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 27.94 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 30.48 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 33.02 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 35.56 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 38.1 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 40.64 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 43.18 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 45.72 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 48.26 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 50.8 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 53.34 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 55.88 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 58.42 6.5) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at -3.5 3.25) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 61.72 3.25) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
)
