(module VariCap (layer F.Cu) (tedit 5CD8948C)
  (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
  (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
  (fp_text reference C403 (at 0.018999 4.884999) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 47P (at 2.5 6.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 2.5 0) (end 7.5 0) (layer F.Fab) (width 0.1))
  (fp_circle (center 2.5 0) (end 7.75 0) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.788861 -2.1875) (end -0.788861 -2.1875) (layer F.Fab) (width 0.1))
  (fp_line (start -1.288861 -2.6875) (end -1.288861 -1.6875) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 2.5 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.508 -2.032) (end -0.508 2.032) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 2.032) (end 2.54 3.048) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 -2.032) (end 2.54 -3.048) (layer F.SilkS) (width 0.15))
  (fp_arc (start 2.54 0) (end 2.54 3.048) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_circle (center 2.54 0) (end 1.016 0.762) (layer F.SilkS) (width 0.15))
  (fp_circle (center 2.54 0) (end 1.397 0.508) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.159 -1.143) (end 2.159 1.143) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.921 -1.143) (end 2.921 1.143) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
)
