(module DS215+DIN8_COMBO (layer F.Cu) (tedit 5E9ACC76)
  (fp_text reference REF** (at 0 11) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DS215+DIN8_COMBO (at 0 11) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 10.6 -9.5) (end -9.1 -9.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -9 -7) (end -9 9.5) (layer F.SilkS) (width 0.381))
  (fp_line (start -9 9.5) (end 9 9.5) (layer F.SilkS) (width 0.381))
  (fp_line (start 9 9.5) (end 9 -7) (layer F.SilkS) (width 0.381))
  (fp_text user "Comments layer lists pins used by the original Amiga Power Connector" (at 0 -10.9) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SH1 (at -11 3) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user -12V (at 0 0.5) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user +12V (at -11.5 8) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 11 8) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user +5V (at 2 5.5) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SH2 (at 0 -8.75) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9 -7) (end -9 -7) (layer F.SilkS) (width 0.381))
  (fp_line (start -9.1 -9.5) (end -9.1 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.6 -8.5) (end -9.1 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.85 -7.5) (end 9.1 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.1 -7.5) (end 9.1 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.6 -8.5) (end 9.1 -8.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.6 -8.5) (end 10.6 -9.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.6 -8.5) (end -10.6 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -10.6 -7.5) (end -7.85 -7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.85 -7.5) (end -7.85 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.85 -7.5) (end 7.85 -7) (layer F.SilkS) (width 0.15))
  (fp_poly (pts (xy 10.6 -8.5) (xy 9.1 -8.5) (xy 9.1 -7.5) (xy 7.85 -7.5)
    (xy 7.85 -7) (xy -7.85 -7) (xy -7.85 -7.5) (xy -10.6 -7.5)
    (xy -10.6 -8.5) (xy -9.1 -8.5) (xy -9.1 -9.5) (xy 10.6 -9.5)) (layer F.SilkS) (width 0.1))
  (pad 6 thru_hole circle (at 5 -7) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -5 -7) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 3) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 7.5 3) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -7.5 3) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 7.5 8) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 8) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -7.5 8) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -5 5.5) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 5 5.5) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 -7) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -2.5 -7) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.5 -7) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 -4.5) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -2.5 -4.5) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.5 -4.5) (size 2 2) (drill 1.4) (layers *.Cu *.Mask))
)
