(module EMI_Filter_Long (layer F.Cu) (tedit 5CD35E39)
  (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x03 2.54mm single row")
  (fp_text reference E416 (at -11.557 -1.778) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 470p (at 0 7.41) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.81 1.27) (end -9.144 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.81 -1.27) (end -9.144 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.175 1.905) (end -0.635 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 1.27) (end -0.635 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 1.27) (end 0.635 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.175 -1.905) (end -0.635 -1.912) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.175 -1.905) (end -3.81 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.81 1.27) (end -3.175 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.635 -1.905) (end 0 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.635 -1.905) (end 0 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.175 -1.905) (end 3.81 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.81 1.27) (end 3.175 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.635 1.905) (end 3.175 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start 0.635 -1.905) (end 3.175 -1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start -9.144 1.27) (end -9.144 -1.27) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0 2.54 270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
)
