(module LineFilter (layer F.Cu) (tedit 5CD6C272)
  (descr "Through hole straight pin header, 2x04, 1.00mm pitch, double rows")
  (tags "Through hole pin header THT 2x04 1.00mm double row")
  (fp_text reference LF1 (at 0 0 270) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value L (at 0.5 4.56 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6 10.16) (end 6 10.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 -10.16) (end -6 10.16) (layer F.SilkS) (width 0.12))
  (fp_line (start 6 -10.16) (end 6 10.16) (layer F.SilkS) (width 0.12))
  (fp_line (start -6 -10.16) (end 6 -10.16) (layer F.SilkS) (width 0.12))
  (fp_text user %R (at 0.5 1.5 270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -3.5 -7.62) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -3.5 -2.54) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -3.5 2.54) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -3.5 7.62) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 3.5 7.62) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 3.5 2.54) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 3.5 -2.54) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 3.5 -7.62) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask))
)
