(module EMI_Filter_Short (layer F.Cu) (tedit 5CD35AD8)
  (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x03 2.54mm single row")
  (fp_text reference E511 (at -3.048 2.54 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 100p (at 0 7.41) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 2.54 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 6.85) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 6.85) (end 1.8 6.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 -1.8) (end -1.8 6.85) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.27 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.905 3.175) (end 1.905 5.715) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.905 3.175) (end -1.905 5.715) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 6.35) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 6.35) (end -1.27 6.35) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 -1.27) (end 1.27 6.35) (layer F.Fab) (width 0.1))
  (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 6.35) (end -1.905 5.715) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.905 5.715) (end 1.27 6.35) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.905 3.175) (end 1.27 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.905 1.905) (end 1.27 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 -1.27) (end -1.905 -0.635) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.905 -0.635) (end 1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.905 -0.635) (end 1.912 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 2.54) (end -1.905 3.175) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 2.54) (end -1.905 1.905) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.905 -0.635) (end -1.905 1.905) (layer F.SilkS) (width 0.12))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
)
