(module Jumper2-Open (layer F.Cu) (tedit 5CBF752B)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference JP7B1 (at 2.5654 -2.1336) (layer F.SilkS)
    (effects (font (size 1.6 1.6) (thickness 0.3)))
  )
  (fp_text value Jumper_3_Bridged12 (at 0 1.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 1 (at -1.584 0) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.905 1.143) (end -1.905 -1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start 2.032 1.143) (end -1.905 1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start 2.032 -1.143) (end 2.032 1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start -1.905 -1.143) (end 2.032 -1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.159 -1.27) (end 2.286 -1.27) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.159 -1.27) (end -2.159 1.23) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.286 1.27) (end 2.286 -1.27) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.286 1.27) (end -2.159 1.27) (layer F.CrtYd) (width 0.05))
  (pad 2 smd rect (at 1.016 0) (size 1.5 1.5) (layers F.Cu F.Mask))
  (pad 1 smd rect (at -0.889 0) (size 1.5 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
)
