(module Jumper3-Bridged23 (layer F.Cu) (tedit 5EA1EF99)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference JP2 (at -4.4 -2.3 -270) (layer F.SilkS)
    (effects (font (size 1.6 1.6) (thickness 0.3)))
  )
  (fp_text value Jumper_3_Bridged23 (at 0 1.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.3 1.25) (end -2.3 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 1.25) (end 2.3 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 -1.25) (end -2.3 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 -1.25) (end 2.3 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.921 -1.143) (end 2.921 -1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start 2.921 -1.143) (end 2.921 1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start 2.921 1.143) (end -2.921 1.143) (layer F.SilkS) (width 0.2))
  (fp_line (start -2.921 1.143) (end -2.921 -1.143) (layer F.SilkS) (width 0.2))
  (fp_text user 1 (at -2.6 0) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 3 (at 2.6 0) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_poly (pts (xy 0.454 -0.3) (xy 1.451 -0.3) (xy 1.451 0.3) (xy 0.454 0.3)) (layer F.Cu) (width 0))
  (pad 1 smd rect (at -1.905 0) (size 1.5 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
  (pad 2 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask))
  (pad 3 smd rect (at 1.905 0) (size 1.5 1.5) (layers F.Cu F.Mask)
    (zone_connect 0))
)
