(module Battery_Holder_Coin_2032_BS-7 (layer F.Cu) (tedit 5E921D87)
  (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
  (fp_text reference BT1 (at 8.128 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CR2032 (at 7.4676 13.56) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.9624 11.43) (end 21.5138 11.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.9624 -11.43) (end 21.5138 -11.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start 21.5138 -11.43) (end 21.5138 11.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.9624 -11.43) (end -3.9624 11.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start 20.7772 3.9116) (end 20.7772 1.0668) (layer F.SilkS) (width 0.1))
  (fp_line (start 20.7772 -3.9116) (end 20.7772 -1.0668) (layer F.SilkS) (width 0.1))
  (fp_line (start 18.034 3.9116) (end 20.7772 3.9116) (layer F.SilkS) (width 0.1))
  (fp_line (start 18.034 -3.9116) (end 20.7772 -3.9116) (layer F.SilkS) (width 0.1))
  (fp_line (start 20.6756 -3.81) (end 20.6756 3.81) (layer F.Fab) (width 0.1))
  (fp_line (start 17.9832 3.81) (end 20.6756 3.81) (layer F.Fab) (width 0.1))
  (fp_line (start 17.9832 -3.81) (end 20.6756 -3.81) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 7.4676 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 7.4676 0) (end -3.7592 0) (layer F.SilkS) (width 0.1))
  (fp_circle (center 7.4676 0) (end -3.7084 0) (layer F.Fab) (width 0.1))
  (pad 2 thru_hole rect (at 0 0) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 20 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/3dModels/BS-7.STEP
    (offset (xyz 7.5 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -90))
  )
)
