
### SAMPLE Data:
> **[2017-09-12 23.18.43.731 - Received 41 (0x29) bytes]**

> 7E A0 27 01 02 01 10 5A  87 E6 E7 00 0F 40 00 00  00 09 0C 07 E1 09 0C 02
> 17 12 2A FF 80 00 00 02  01 06 00 00 05 28 B8 0C  7E


### Breakdown:
Data	|	Explaination
--------|-------------
7E 	|	Frame Start flag
A	|	4 bits, A = Frame Format Type 3 (0b1010)
0 27	|	11 bits, Frame size: 0x27 (39 bytes, excluding start/end flags)
01	|	Destination Address (Address can be 1-4 bytes. Terminated by LSB=1)
02 01	|	Source Address (Address can be 1-4 bytes. Terminated by LSB=1)
10	|	Control Field
5A 87	|	Header check sequence (HCS) (Check sum calculated from the address bytes, according to RFC 1662)
**Begin Data**|	LLC PDU Format (GB, 8.3 Fig 19)||
E6	|	Destination LSAP
E7	|	Source LSAP
00	|	LLC Quality
0F 	|	Information, n*8 bits?
40	|	(UNCERTAIN) Push setup, class_id=40
00	|	(UNCERTAIN) version=0
00 00 09 0C | 	(UNKNOWN, 2316?)
07 E1	|	2017 (year)
09	|	09 (sep)
0C	|	12 (date)
02	|	tuesday 
17	|	23 (hour)
12	|	18 (min)
2A	|	42 (sec)
FF 	|	(fff not specified)
80 	|	(deviation not specified)
00 00 	|	(clock_status)
02 	|	(UNKNOWN)
01 06 	|	(UNCERTAIN. 0106=List1, 0D09=List2, 1209=List3)
00 	|	(UNKNOWN)
00 	|	(UNKNOWN)
05 28	|	1320 Watt
**End Data**|
B8 0C	|	Frame check sequence (FCS) (Check sum calculated from full frame, excluding flags and FCS, according to RFC 1662)
7E	|	Frame End flag
