## arty-100t board
set_property PACKAGE_PIN E3  [get_ports clk]
set_property PACKAGE_PIN D9  [get_ports rst]
set_property PACKAGE_PIN H5  [get_ports io_led[4]]
set_property PACKAGE_PIN J5  [get_ports io_led[5]]
set_property PACKAGE_PIN T9  [get_ports io_led[6]]
set_property PACKAGE_PIN T10 [get_ports io_led[7]]

set_property IOSTANDARD LVCMOS33 [get_ports clk]
set_property IOSTANDARD LVCMOS33 [get_ports rst]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[4]]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[5]]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[6]]
set_property IOSTANDARD LVCMOS33 [get_ports io_led[7]]
