(module TestPoint_Pad_2x12_D1.0mm (layer F.Cu) (tedit 5F9F0FA0)
  (descr "Through hole straight pin header, 2x12, 2.54mm pitch, double rows")
  (tags "Through hole pin header THT 2x12 2.54mm double row")
  (fp_text reference REF** (at 1.27 -2.33) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TestPoint_Pad_2x12_D1.0mm (at 1.27 30.27) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.35 29.75) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 29.75) (end 4.35 29.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 -1.8) (end -1.8 29.75) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 1.27 13.97 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 0 0.7) (layer F.SilkS) (width 0.12))
  (fp_circle (center 2.54 0) (end 3.54 0) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 0) (end 1 0) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 2.54) (end 1 2.54) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 2.54) (end 3.54 2.54) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 5.08) (end 3.54 5.08) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 5.08) (end 1 5.08) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 10.16) (end 1 10.16) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 10.16) (end 3.54 10.16) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 7.62) (end 1 7.62) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 7.62) (end 3.54 7.62) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 15.24) (end 1 15.24) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 15.24) (end 3.54 15.24) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 12.7) (end 1 12.7) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 12.7) (end 3.54 12.7) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 20.32) (end 1 20.32) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 20.32) (end 3.54 20.32) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 17.78) (end 1 17.78) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 17.78) (end 3.54 17.78) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 22.86) (end 3.54 22.86) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 25.4) (end 3.54 25.4) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 22.86) (end 1 22.86) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 25.4) (end 1 25.4) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 2.54 27.94) (end 3.54 27.94) (layer F.CrtYd) (width 0.05))
  (fp_circle (center 0 27.94) (end 1 27.94) (layer F.CrtYd) (width 0.05))
  (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask))
  (pad 2 smd circle (at 2.54 0) (size 1 1) (layers F.Cu F.Mask))
  (pad 3 smd circle (at 0 2.54) (size 1 1) (layers F.Cu F.Mask))
  (pad 4 smd circle (at 2.54 2.54) (size 1 1) (layers F.Cu F.Mask))
  (pad 6 smd circle (at 2.54 5.08) (size 1 1) (layers F.Cu F.Mask))
  (pad 5 smd circle (at 0 5.08) (size 1 1) (layers F.Cu F.Mask))
  (pad 7 smd circle (at 0 7.62) (size 1 1) (layers F.Cu F.Mask))
  (pad 9 smd circle (at 0 10.16) (size 1 1) (layers F.Cu F.Mask))
  (pad 8 smd circle (at 2.54 7.62) (size 1 1) (layers F.Cu F.Mask))
  (pad 10 smd circle (at 2.54 10.16) (size 1 1) (layers F.Cu F.Mask))
  (pad 11 smd circle (at 0 12.7) (size 1 1) (layers F.Cu F.Mask))
  (pad 13 smd circle (at 0 15.24) (size 1 1) (layers F.Cu F.Mask))
  (pad 12 smd circle (at 2.54 12.7) (size 1 1) (layers F.Cu F.Mask))
  (pad 14 smd circle (at 2.54 15.24) (size 1 1) (layers F.Cu F.Mask))
  (pad 15 smd circle (at 0 17.78) (size 1 1) (layers F.Cu F.Mask))
  (pad 17 smd circle (at 0 20.32) (size 1 1) (layers F.Cu F.Mask))
  (pad 16 smd circle (at 2.54 17.78) (size 1 1) (layers F.Cu F.Mask))
  (pad 18 smd circle (at 2.54 20.32) (size 1 1) (layers F.Cu F.Mask))
  (pad 19 smd circle (at 0 22.86) (size 1 1) (layers F.Cu F.Mask))
  (pad 21 smd circle (at 0 25.4) (size 1 1) (layers F.Cu F.Mask))
  (pad 20 smd circle (at 2.54 22.86) (size 1 1) (layers F.Cu F.Mask))
  (pad 22 smd circle (at 2.54 25.4) (size 1 1) (layers F.Cu F.Mask))
  (pad 23 smd circle (at 0 27.94) (size 1 1) (layers F.Cu F.Mask))
  (pad 24 smd circle (at 2.54 27.94) (size 1 1) (layers F.Cu F.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x12_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
