CPU						status		writeup		sources

24315	Memory reference group			passed		in 21MX CE	no
	- LOAD diagnostic
	- RUN 100
	- HLT 77, PC = 3353

24316	Alter/skip group			passed		in 21MX CE	no
	- LOAD diagnostic
	- RUN 100
	- HLT 77, PC = 633 

24317	Shift/rotate group			passed		in 21MX CE	no
	- LOAD diagnostic
	- RUN 100
	- HLT 77, PC = 1726

24296	Diagnostic configurator			passed		in 21MX CE	no
	- LOAD configurator
	- SET CPU 21MX
	- ATTACH PTR binary image of
	  diagnostic to be configured
	- D S XXYY, where XX = device number
	  of PTR, YY = device number of TTY
	- RUN 2
	- HLT 77, PC = 77237 (for 32K mem)

24319	Extended arithmetic group		passed		in 21MX CE	no
	- load diagnostic via configurator
	- D S 0
	- RUN 100
	- prints diagnostic name
	- prints END OF PASS 1 and halts

13206	IOP for 2100 group			passed		13206 manual	no

24320	Floating point				passed		in 21MX CE	no
	- load diagnostic via configurator
	- D S 0
	- RUN 100
	- prints diagnostic name
	- prints PASS 000001 and halts

12943-1	Extended instruction group, part 1	passed		12943 manual	no
	- load diagnostic via configurator
	- D S 0
	- RUN 100
	- prints diagnostic name
	- prints PASS 000001 and halts

12943-2	Extended instruction group, part 2	passed		12943 manual	no
	- load diagnostic via configurator
	- D S XX, where XX = device number
	  of TTY
	- RUN 100
	- HLT 74, PC = 2406
	- D S 0
	- CONTINUE
	- prints diagnostic name
	- prints PASS 000001 and halts

24322	Dual channel port controller		passed		in 21MX CE	no
	- load diagnostic via configurator
	- SET LPS ENA
	- SET LPS DIAG
	- D S XX, where XX = device number
	  of LPS
	- RUN 100
	- HALT 74, PC = 1541
	- D S 0
	- CONTINUE
	- prints diagnostic name
	- prints H324 PRESS PRESET AND RUN
	- HLT 24, PC = 2312
	- RESET ALL
	- CONTINUE
	- prints PASS 000001 and halts

12892	Memory protect-parity error		passed		in 21MX CE	no
	- load diagnostic via configurator
	- disable all I/O devices except
	  PTR, TTY, clock
	- D S 1400XX, where XX = device number
	  of PTR
	- RUN 100
	- HLT 74, PC = 2444
	- D S 1000 (test select mode)
	- CONTINUE
	- prints diagnostic name
	- HLT 75, PC = 2026
	- D S 0
	- D A 31777 (tests 10-11 can't be run)
	- Rings bell and prints
	  H314 PRESS HALT,PRESET AND RUN WITHIN 30 SECONDS
	- WRU (CTRL+E) to interrupt simulation
	- RESET ALL
	- CONTINUE
	- prints PASS 000001 and halts

12929	Memory expansion unit (DMS)		passed		in 21MX CE	no
	- load diagnostic via configurator
	- SET CPU 64K
	- SET LPS ENA
	- SET LPS DIAG
	- D S XX, where XX = device number
	  of LPS
	- RUN 100
	- HLT 74, PC = 2435
	- D S 0
	- CONTINUE
	- Prints H115 PRESS HALT-PRESET-RUN IN LESS THAN 10 SECONDS
	- WRU (CTRL+E) to interrupt simulation
	- RESET ALL
	- CONTINUE
	- Prints H117 PRESET TEST COMPLETE
	- Prints PASS 000001 and halts
	- Test 23 won't run at >256K mem
	  (real 21MX limited to 304K)

Peripherals

12531	TTY test				passed		in 21MX CE	no
	- set TTY TTIME to 100
	- run with test select = 173
	- remaining tests can't be run
12539	time base generator			passed		in 21MX CE	no
	- runs with CLK in diag mode
12597	reader/punch				passed		in 21MX CE	no
	- set PTP TIME to 100
	- run with test select a=4017
	- remaining tests can't be run
12984	2767 line printer			passed		in 21MX CE	no
	- set LPS PTIME, CTIME to 100
	- run with test select a = 15
	- remaining tests can't be run
12960	7900/7901 disk				passed		in 21MX CE	no
12965	2883/2884 disk				passed		12965 manual	no
12559	3030 magtape				not run		no documentation
13181	7970B magtape				partial		in 21MX CE	no
	- set MSC CTIME to 180000
	- do not change MSC XTIME
	- attach scratch tapes to units 0,1
	- set s = 2000 (suppress CRC/LRC)
	- run with test select a = 37737, b = 7767
	- tests 4, 14, 15 are timing dependent
	- test 19 uses non-supported read rev
13183	7970E magtape				not run		in 21MX CE	no
12920	multiplexor				not run		in 21MX CE	no
