(module USB_A_Molex_67643_Horizontal (layer F.Cu) (tedit 5EA03975)
  (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
  (tags "USB_A Female Connector receptacle")
  (fp_text reference REF** (at 3.5 -3.19) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_A_Molex_67643_Horizontal (at 3.5 14.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 3.5 3.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.05 -2.27) (end 10.05 -2.27) (layer F.Fab) (width 0.1))
  (fp_line (start 10.05 -2.27) (end 10.05 12.69) (layer F.Fab) (width 0.1))
  (fp_line (start -3.16 12.58) (end -3.16 4.47) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.16 12.58) (end -3.81 12.58) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.7 12.69) (end -3.7 12.99) (layer F.Fab) (width 0.1))
  (fp_line (start -3.7 12.99) (end 10.7 12.99) (layer F.Fab) (width 0.1))
  (fp_line (start 10.7 12.99) (end 10.7 12.69) (layer F.Fab) (width 0.1))
  (fp_line (start 10.7 12.69) (end 10.05 12.69) (layer F.Fab) (width 0.1))
  (fp_line (start -3.05 9.27) (end 10.05 9.27) (layer F.Fab) (width 0.1))
  (fp_line (start -3.55 -2.77) (end 10.55 -2.77) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.55 -2.77) (end 10.55 0.76) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.55 -2.77) (end -3.55 0.76) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.2 13.49) (end 11.2 13.49) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.2 13.49) (end 11.2 12.19) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.2 12.19) (end 10.55 12.19) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.55 12.19) (end 10.55 4.66) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.2 13.49) (end -4.2 12.19) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.2 12.19) (end -3.55 12.19) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.55 12.19) (end -3.55 4.66) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -3.07 2.71) (end -3.55 0.76) (angle -152.3426981) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 10.07 2.71) (end 10.55 4.66) (angle -152.3426981) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.16 -2.38) (end 10.16 -2.38) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.16 -2.38) (end -3.16 0.95) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.16 -2.38) (end 10.16 0.95) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.05 12.69) (end -3.05 -2.27) (layer F.Fab) (width 0.1))
  (fp_line (start 10.81 13.1) (end 10.81 12.58) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.81 13.1) (end 10.81 13.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.16 4.47) (end 10.16 12.58) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.81 12.58) (end -3.81 13.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.81 12.58) (end 10.16 12.58) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.05 12.69) (end -3.7 12.69) (layer F.Fab) (width 0.1))
  (fp_line (start -0.9 -2.6) (end 0.9 -2.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -1 -2.27) (end 0 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 0 -1.27) (end 1 -2.27) (layer F.Fab) (width 0.1))
  (pad 5 thru_hole circle (at -3.07 2.71) (size 3 3) (drill 2.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 10.07 2.71) (size 3 3) (drill 2.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.6 1.5) (drill 0.95) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 4.5 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 7 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
