	.STITL	DISC BLOCKS, NODE SPACE AND TEST LINES
	VERN==VERN+%FNAM2

	.MACR NODE A,B
	.XLIST
$.==$$+1
	A
	B
$$==$$+1
	.LIST
.ENDM

VERNF==VERN
SALTL:	LTL
LTL:	L1
	L2
	L3
	L4
	L5
	L6
	0	;L7
	0	;L8
	0	;L9
	0	;L10
	0	;L11
	0	;L12
	0	;L13
	0	;L14
	0

.EVEN
SLOT1:
MSLTLN==LUVBLK+PPDLL+SPDLL+DBUFL+DDIRL+<4*4096.>	;ALL YOU COULD POSSIBLY WANT
UVSAV:	.=.+LUVBLK
	.=.+PPDLL
	IP=.
PDLINK:	.=.+4	;LINK TO PREVIOUS DISK BLOCK
	.=.+SPDLL
	IS=.
SDLINK:	.=.+4
HCC==67.	;HASH CODE CONSTANT - A PRIME
UHCT:	.=UHCT+<2*16.>
	$OB3
	$OB4
	$OB5
	.=UHCT+<2*23.>
	$OB2
	.=UHCT+<2*60.>
	$OB1
	.=UHCT+<2*HCC>
DBUF:	.=.+DBUFL
DDIR:	.=.+DDIRL
	0
	0

.IF2
	PAD ^\ START OF NODESP\,\.
.ENDC

NODESP:	0	;NODE 0
	0
	.=NODESP+80.
	TRUE=140000+20.
	SSTR+21.	;20
	"TR
	SSTR+0	;21
	"UE
	FALSE=140000+22.
	SSTR+23.	;22
	"FA
	SSTR+24.	;23
	"LS
	SSTR+0		;24
	'E
	.=NODESP+404.
	L1=101.			;PRINT "ABCD"
	SFUN+102.	;NODE 101
	$PRINT
	LSTR+0		;102
	LSTR+103.
	SSTR+104.	;103
	"AB
	SSTR	;104
	"CD
	L2=105.			;"123"
	LSTR+0	;105
	LSTR+106.
	SSTR+107.	;106
	"12
	SSTR	;107
	'3
	SFUN	;108
	0
	SFUN		;109
	0
	L3=110.			;(PRINT "AXBYJ" "1Q" "FOOBAR")
	SFUN+111.	;110
	$LPAR
	SFUN+112.	;111
	$PRINT
	LSTR+117.	;112
	LSTR+114.
	SSTR+0		;113
	"1Q
	SSTR+115.	;114
	"AX
	SSTR+116.	;115
	"BY
	SSTR+0		;116
	'J
	LSTR+118.	;117
	LSTR+113.
	ATOM+119.	;118
	ATOM+122.
	SFUN+0	;119
	$RPAR
	SFUN+0		;120
	0
$OB1=121.
	0		;121 = START OF UOB BUCKET 60.
	$FOO
	$FOO=122.
	ATOM+125.		;122 - HEADER OF FIRST UOE
	LSTR+123.
	SSTR+124.	;123
	"FO
	SSTR+0		;124
	'O
	VBIND+$FOOF		;125 - VARIABLE BINDING OF 1ST UOE
	LSTR+126.
	SSTR+127.	;126
	"FO
	SSTR+128.	;127
	"OB
	SSTR+0		;128
	"AR
	0		;129
	0
	L4=130.		;IF "TRUE" THEN PRINT "TRUE" ELSE PRINT "FALSE"
	SFUN+131.	;130
	$IF
	LSTR+134.	;131
	LSTR+132.
	SSTR+133.	;132
	"TR
	SSTR+0		;133
	"UE
	SFUN+135.	;134
	$THEN
	SFUN+136.	;135
	$PRINT
	LSTR+137.	;136
	LSTR+132.
	SFUN+138.	;137
	$ELSE
	SFUN+139.	;138
	$PRINT
	LSTR+0	;139
	LSTR+140.
	SSTR+141.	;140
	"FA
	SSTR+142.	;141
	"LS
	SSTR+0		;142
	'E
	SFUN+0		;143
	0
	$$=144.
L5=$$	;MAKE "BAR" "AB1C"
	NODE SFUN+$.,$MAKE
	NODE ATOM+$.,ATOM+$BAR
	NODE LSTR,LSTR+$.
	NODE SSTR+$.,"AB
	NODE SSTR,"1C
L6=$$	;PRINT :BAR
	NODE SFUN+$.,$PRINT
	NODE UVAR,UVAR+$BAR
$OB2=$$
	NODE 0,$BAR	;START OF UOB BUCKET 23.
$BAR=$$
	NODE ATOM,LSTR+$.
	NODE SSTR+$.,"BA
	NODE SSTR,'R
L7==$$	;FOO :BAR "GRINCH"
	NODE UFUN+$.,$FOO
	NODE UVAR+$.,UVAR+$BAR
	NODE LSTR,LSTR+$.
	NODE SSTR+$.,"GR
	NODE SSTR+$.,"IN
	NODE SSTR,"CH
$FOOF=$$
	NODE FBIND+$.,LIST+$FLLP
	NODE SFBIND,LIST+$FSFB
$FLLP=$$
	NODE LIST+$.,LIST+$FL0
	NODE LIST+$.,LIST+$FL1
	NODE LIST,LIST+$FL2
$FL0=$$
	NODE SNUM+$.,2
	NODE SNUM+$.,$A
	NODE SNUM,$B
$FL1=$$
	NODE SNUM+$.,10.
	NODE SFUN+$.,$PRINT
	NODE UVAR,UVAR+$A
$FL2=$$
	NODE SNUM+$.,20.
	NODE SFUN+$.,$PRINT
	NODE UVAR,UVAR+$B
$FSFB=$$
	NODE SNUM+$.,2	;NO. ARGS
	NODE SNUM+$.,0	;PROCD SWAP NO.
	NODE SNUM+$.,0	;NO. NODES
	NODE SNUM+$.,0	;NO. FLUSHABLE NODES
	NODE SNUM+$.,0	;DISC ADDR 1
	NODE SNUM+$.,0	; "     "     2
	NODE SNUM+$.,0	;# WORDS ON DISC
$OB3=$$
	NODE 0,$A	;START OF UOB BUCKET 16.
$OB4=$$
	NODE 0,$B	;START OF UOB BUCKET 17.
$OB5=$$
	NODE 0,$C	;START OF UOB BUCKET 18.
$A=$$
	NODE ATOM,LSTR+$.
	NODE SSTR,'A
$B=$$
	NODE ATOM+$BVB,LSTR+$.
	NODE SSTR,'B
$BVB=$$
	NODE VBIND,LSTR+$.
	NODE SSTR+$.,"B.
	NODE SSTR+$.,"HA
	NODE SSTR+$.,"S.
	NODE SSTR+$.,"LO
	NODE SSTR,"TS
$C==$$
	NODE ATOM+$CVB,LSTR+$.
	NODE SSTR,'C
$CVB==$$
	NODE VBIND,LNUM+$.
	NODE SNUM,100.
L8=$$	;MAKE "BLIP" 13
	NODE SFUN+$.,$MAKE
	NODE LSTR+$.,LSTR+$BLIP
	NODE LNUM,LNUM+$.
	NODE SNUM,13
L9=$$	;PRINT : "BLIP"
	NODE SFUN+$.,$PRINT
	NODE SFUN+$.,$DOTS
	NODE LSTR,LSTR+$BLIP
L10=$$	;MAKE "BLIP" "XX"
	NODE SFUN+$.,$MAKE
	NODE LSTR+$.,LSTR+$BLIP
	NODE LSTR,LSTR+$.
	NODE SSTR,"XX
L11=$$	;PRINT :"BLIP"
	NODE SFUN+$.,$PRINT
	NODE SFUN+$.,$DOTS
	NODE LSTR,LSTR+$BLIP
L12=$$	;MAKE "BLAP" "YY"
	NODE SFUN+$.,$MAKE
	NODE LSTR+$.,LSTR+$BLAP
	NODE LSTR,LSTR+$.
	NODE SSTR,"YY
L13==$$	;PRINT :"BLAP"
	NODE SFUN+$.,$PRINT
	NODE SFUN+$.,$DOTS
	NODE LSTR,LSTR+$BLAP
L14==$$	;STARTDISPLAY
	NODE SFUN,$START
L15==$$	;FORWARD :C
	NODE SFUN+$.,$FORWA
	NODE UVAR,UVAR+$C
$BLAP==$$	;"BLAP"
	NODE SSTR+$.,"BL
	NODE SSTR,"AP
$BLIP==$$	;"BLIP"
	NODE SSTR+$.,"BL
	NODE SSTR,"IP
	NNN=$$	;NEXT NODE NO.
SOFN=NNN	;START OF FREE NODES
ASOFN=.
LOGEND=.


;IN THE EVENT THAT THE SYSTEM OBLIST
;HAS BEEN INCORRECTLY SET UP, AND THE MACRO TRIED TO WRITE OVER
;PARTS OF IT, THIS LITTLE .IFLE WILL PRINT OUT A MESSAGE
	.IFLE OBX0
	********
	YOU ARE OVERWRITING THE SYSTEM OBLIST
	********
	.XLIST
	.ENDC
	.END
