# Attach to a server.  If the remote port isn't telnet, append ;notelnet.
attach tty 12345,connect=localhost:23
# Configure a bootstrap ROM; some programs require this.
set rom type=stty
# Load SSV version 22.
load -s ssv22.iml
# Reset and run.
reset
go
