# configure tb_nexsy4 with sys_tst_rlink_n4 target;
# use vhdl configure file (tb_tst_rlink_n4.vhd) to allow
# that all configurations will co-exist in work library
# configure
nexys4_aif = ../sys_tst_rlink_n4.vbom
sys_conf = sys_conf_sim.vhd
# design
../../../../bplib/nexys4/tb/tb_nexys4.vbom
tb_tst_rlink_n4.vhd
