# configure tb_nx_cram_memctl with tbd_nx_cram_memctl_as target;
# use vhdl configure file (tb_nx_cram_memctl_as.vhd) to allow
# that all configurations will co-exist in work library
# configure
uut = tbd_nx_cram_memctl_as.vbom
tb_nx_cram_memctl.vbom
# design
tb_nx_cram_memctl_as.vhd
