# $Id: sys_tst_rlink_cuff_ic_n3.imfset 769 2016-05-28 11:36:22Z mueller $
#
# ----------------------------------------------------------------------------
[xst]
Case statement is complete. others clause is never selected
Using initial value '0' for reset since it is never assigned
Using initial value '0' for fx2_tx2ena_l since it is never assigned

Net <FX2_TX2BUSY> does not have a driver.

Output port <LOCKED> of the instance <DCM> is unconnected
Output port <RXAEMPTY> of the instance <FX2_CNTL_IC.CNTL> is unconnected
Output port <TXAFULL> of the instance <FX2_CNTL_IC.CNTL> is unconnected
Output port <FX2_TX2DATA> of the instance <TST> is unconnected
Output port <FX2_TX2ENA> of the instance <TST> is unconnected
Output port <SIZER> of the instance <TXFIFO> is unconnected
Output port <DOA> of the instance <RAM> is unconnected
Output port <RL_MONI_eop> of the instance <RLCORE> is unconnected
Output port <RL_MONI_attn> of the instance <RLCORE> is unconnected
Output port <RL_MONI_lamp> of the instance <RLCORE> is unconnected
Output port <MONI_rxerr> of the instance <SERPORT> is unconnected
Output port <MONI_rxovr> of the instance <SERPORT> is unconnected
Output port <MONI_abdone> of the instance <SERPORT> is unconnected
Output port <SIZE> of the instance <TXFIFO> is unconnected or connected
Output port <SIZE> of the instance <FIFO> is unconnected or connected
Output port <DOB> of the instance <BRAM> is unconnected

Signal <FX2_TX2DATA> is used but never assigned

Signal 'FX2_TX2BUSY', unconnected in block 'sys_tst_rlink_cuff_n3'

Node <FX2_CNTL_IC.CNTL/R_MONI_[CS]_.*> of sequential type is unconnected
Node <FX2_CNTL_IC.CNTL/R_REGS_moni_ep6_sel> of sequential type is unconnected
Node <FX2_CNTL_IC.CNTL/R_REGS_moni_ep6_pf> of sequential type is unconnected
Node <FX2_CNTL_IC.CNTL/R_REGS_moni_ep4_pf> of sequential type is unconnected
ode <FX2_CNTL_IC.CNTL/R_REGS_moni_ep4_sel> of sequential type is unconnected
Node <IOB_FX2_FLAG/R_DI_3> of sequential type is unconnected
Node <HIO/R_REGS_swieff_[3-7]> of sequential type is unconnected
Node <HIO/R_REGS_btn_[0-4]> of sequential type is unconnected
Node <HIO/R_REGS_swi_[3-7]> of sequential type is unconnected
Node <HIO/R_REGS_btneff_[0-4]> of sequential type is unconnected
Node <FX2_CNTL_IC.CNTL/[RT]XFIFO/R_REG[RW]_size[rw]_\d> of sequential type is unconnected
Node <TST/RLCORE/RL/R_REGS_monattn> of sequential type is unconnected
Node <TST/RLCORE/RL/R_REGS_monlamp> of sequential type is unconnected
Node <TST/RLCORE/RL/R_REGS_moneop> of sequential type is unconnected
Node <TST/SERPORT/XONRX/R_REGS_rxovr> of sequential type is unconnected

Input <RB_MREQ_init> is never used
Input <RB_MREQ_din<15:10>> is never used
Input <I_MEM_WAIT> is never used
Input <SWI<7:3>> is never used
Input <SWI<0:0>> is never used
Input <BTN<3:0>> is never used
Input <FX2_MONI_fifo_ep4> is never used
Input <FX2_MONI_fifo_ep6> is never used
Input <FX2_MONI_fifo_ep8> is never used
Input <FX2_MONI_flag_ep4_empty> is never used
Input <FX2_MONI_flag_ep4_almost> is never used
Input <FX2_MONI_flag_ep6_full> is never used
Input <FX2_MONI_flag_ep6_almost> is never used
Input <FX2_MONI_flag_ep8_full> is never used
Input <FX2_MONI_flag_ep8_almost> is never used
Input <FX2_MONI_slrd> is never used
Input <FX2_MONI_slwr> is never used
Input <FX2_MONI_pktend> is never used

FF/Latch <R_MONI_[CS]_.*> has a constant value of 0
FF/Latch <TX2ENA_PSTR/R_REGS_busy_1> has a constant value
FF/Latch <TX2ENA_PSTR/R_REGS_busy_0> has a constant value

of type RAMB16_S18 has been replaced by RAMB16BWER
of type RAMB16_S36 has been replaced by RAMB16BWER
of type RAMB16_S36_S36 has been replaced by RAMB16BWER

FF/Latch <HIO/R_REGS_ledin_[2-6]> has a constant value of 0
FF/Latch <FX2_CNTL_IC.CNTL/[RT]XFIFO/R_REG[RW]_rst.*> has a constant value

The FF/Latch <R_REGS_rbre> .* is equivalent
The FF/Latch <HIO/HIO/HIO/DEB.DEB_SWI/R_REGS_cecnt_[01]> .* is equivalent
The FF/Latch <HIO/HIO/DRV/R_REGS_cdiv_0> .* is the opposite

#
# ----------------------------------------------------------------------------
[tra]

#
# ----------------------------------------------------------------------------
[map]
INFO:.*

#
# ----------------------------------------------------------------------------
[par]
The signal I_MEM_WAIT_IBUF has no load
The signal I_FX2_FLAG<3>_IBUF has no load
There are 2 loadless signals in this design

#
# ----------------------------------------------------------------------------
[bgn]
