## $Id: sys_tst_sram_n3.ucf_cpp 435 2011-12-04 20:15:25Z mueller $
##
## Revision History: 
## Date         Rev Version  Comment
## 2011-12-03   435   1.1    use also pmb0_rs232
## 2011-11-27   433   1.0    Initial version
##

NET "I_CLK100" TNM_NET = "I_CLK100";
TIMESPEC "TS_I_CLK100" = PERIOD "I_CLK100" 10.0 ns HIGH 50 %;
OFFSET =  IN 10 ns BEFORE "I_CLK100";
OFFSET = OUT 20 ns  AFTER "I_CLK100";

## std board
##
#include "bplib/nexys3/nexys3_pins.ucf"
##
## Pmod B0 - RS232 
##
#include "bplib/nexys3/nexys3_pins_pmb0_rs232.ucf"
