# $Id: sys_w11a_n3.imfset 776 2016-06-18 17:22:51Z mueller $
#
# ----------------------------------------------------------------------------
[xst]
INFO:.*Case statement is complete. others clause is never selected
INFO:.*The small RAM <.*> will be implemented on LUTs

Output port <LOCKED> of the instance <GEN_CLKSYS> is unconnected
Output port <FX2_MONI_.*> of the instance <RLINK> is unconnected
Output port <BTN> of the instance <HIO> is unconnected
Output port <RL_MONI_.*> of the instance <RLINK> is unconnected
#
Input <CP_STAT_.*> is never used
Input <MONI_.*> is never used
Input <SER_MONI_.*> is never used
Input <IB_MREQ_.*> is never used
Input <RB_MREQ_.*> is never used
Input <RB_SRES_.*> is never used
Input <DM_STAT_(DP|VM|CO|SE)_.*> is never used
#
INFO:.*Instance.*has been replaced by RAMB16BWER
#
# ----------------------------------------------------------------------------
[tra]
INFO:.*TNM 'I_CLK100'.*was traced into DCM_SP
INFO:.*Setting CLKIN_PERIOD attribute associated with DCM instance
#
# ----------------------------------------------------------------------------
[map]
WARNING:.*has the attribute CLK_FEEDBACK set to NONE
WARNING:.*The signal <I_MEM_WAIT_IBUF> is incomplete
WARNING:.*to use input parity pin.*dangling output for parity pin
INFO:.*
#
# ----------------------------------------------------------------------------
[par]
WARNING:.*has the attribute CLK_FEEDBACK set to NONE
WARNING:.*The signal I_MEM_WAIT_IBUF has no load
WARNING:.*There are 1 loadless signals in this design
#
# ----------------------------------------------------------------------------
[bgn]
WARNING:.*The signal <I_MEM_WAIT_IBUF> is incomplete
WARNING:.*to use input parity pin.*dangling output for parity pin
INFO:.*To achieve optimal frequency synthesis performance
