# configure tb_nexsy2 with sys_tst_sram_n2 target;
# use vhdl configure file (tb_tst_sram_n2.vhd) to allow
# that all configurations will co-exist in work library
# configure
nexys2_aif = ../sys_tst_sram_n2.vbom
sys_conf = sys_conf_sim.vbom
# design
../../../../bplib/nexys2/tb/tb_nexys2.vbom
tb_tst_sram_n2.vhd
