# configure tb_nexsy4d_dram with sys_tst_sram_n4d target;
# use vhdl configure file (tb_tst_sram_n4d.vhd) to allow
# that all configurations will co-exist in work library
# configure
nexys4d_dram_aif = ../sys_tst_sram_n4d.vbom
sys_conf = sys_conf_sim.vhd
# design
../../../../bplib/nexys4d/tb/tb_nexys4d_dram.vbom
tb_tst_sram_n4d.vhd
