# Not meant for direct top level usage. Used with 
# tb_nx_cram_memctl_(....)[_ssim].vbom and config
# lines to generate the different cases.
#
# libs
../../../vlib/slvtypes.vhd
../../../vlib/simlib/simlib.vhd
# components
../../../vlib/simlib/simclk.vbom
../../../vlib/simlib/simclkcnt.vbom
../../micron/mt45w8mw16b.vbom
${uut := tbd_nx_cram_memctl_as.vbom}  -UUT
# design
tb_nx_cram_memctl.vhd
@top:tb_nx_cram_memctl
