## $Id: sys_tst_sram_n2.ucf_cpp 336 2010-11-06 18:28:27Z mueller $
##
## Revision History: 
## Date         Rev Version  Comment
## 2010-11-06   336   1.0.1  rename input pin CLK -> I_CLK50
## 2010-05-23   294   1.0    Initial version
##

NET "I_CLK50" TNM_NET = "I_CLK50";
TIMESPEC "TS_I_CLK50" = PERIOD "I_CLK50" 20 ns HIGH 50 %;
OFFSET =  IN 10 ns BEFORE "I_CLK50";
OFFSET = OUT 20 ns  AFTER "I_CLK50";

#include "bplib/nexys2/nexys2_pins.ucf"
