## $Id: sys_tst_snhumanio_n2.ucf_cpp 410 2011-09-18 11:23:09Z mueller $
##
## Revision History: 
## Date         Rev Version  Comment
## 2011-09-17   410   1.0    Initial version
##

NET "I_CLK50" TNM_NET = "I_CLK50";
TIMESPEC "TS_I_CLK50" = PERIOD "I_CLK50" 20.0 ns HIGH 50 %;
OFFSET =  IN 10 ns BEFORE "I_CLK50";
OFFSET = OUT 20 ns  AFTER "I_CLK50";

## std board
##
#include "bplib/nexys2/nexys2_pins.ucf"
