# configure tb_nexys2_fusp_cuff with sys_w11a_n2 target;
# use vhdl configure file (tb_w11a_n2.vhd) to allow
# that all configurations will co-exist in work library
# configure
nexys2_fusp_cuff_aif = ../sys_w11a_n2.vbom
sys_conf = sys_conf_sim.vbom
# design
../../../../bplib/nexys2/tb/tb_nexys2_fusp_cuff.vbom
tb_w11a_n2.vhd
