## $Id: sys_tst_serloop_s3.ucf_cpp 441 2011-12-20 17:01:16Z mueller $
##
## Revision History: 
## Date         Rev Version  Comment
## 2011-10-25   419   1.0    Initial version
##

NET "I_CLK50" TNM_NET = "I_CLK50";
TIMESPEC "TS_I_CLK50" = PERIOD "I_CLK50" 20 ns HIGH 50 %;
OFFSET =  IN 10 ns BEFORE "I_CLK50";
OFFSET = OUT 20 ns  AFTER "I_CLK50";

## std board
##
#include "bplib/s3board/s3board_pins.ucf"
##
## Pmod1-RS232 on A2 connector
##
#include "bplib/s3board/s3board_a2_pm1_rs232.ucf"
