(export (version D)
  (design
    (source /home/sukko/Documents/kicad/Raemixx500/Raemixx500.sch)
    (date "sab 2 mag 2020, 16:06:37")
    (tool "Eeschema 5.1.5")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-11)
        (source Raemixx500.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 2) (name /CPU+Agnus/) (tstamps /5CAE5331/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-04-11)
        (source cpu.sch)
        (comment (number 1) (value "PROCESSOR AND OTHER USEFUL COMPONENTS"))
        (comment (number 2) (value "Derived from Commodore Schematic #312813, Rev. 1 - Sheet 2 of 10"))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 3) (name /RAM/) (tstamps /5EA8075B/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-04)
        (source ram.sch)
        (comment (number 1) (value "MEMORY AND...WELL, I USED TO REMEMBER"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 4) (name "/Denise & Video Stuff/") (tstamps /5CBA5669/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-05)
        (source video.sch)
        (comment (number 1) (value "DENISE IS PRETTY MUCH INTO VIDEO..."))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 5) (name "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-04)
        (source audio.sch)
        (comment (number 1) (value "PAULA PREFERS THE TRADITIONAL MODES"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 6) (name "/Parallel & Serial/") (tstamps /5E7E9EC4/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-05)
        (source cias.sch)
        (comment (number 1) (value "RS232 AND PARALLEL PORT"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 7) (name "/Floppy Drives/") (tstamps /6072A453/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-06-23)
        (source floppy.sch)
        (comment (number 1) (value "FLOPPY STUFF"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 8) (name "/Termination & Pullups/") (tstamps /5D6D5EBE/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-04-20)
        (source terminators.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 9) (name "/Kickstart ROM/") (tstamps /5D86DD46/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-04-20)
        (source rom.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 10) (name "/Clock Distribution/") (tstamps /5D88EC26/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-04-20)
        (source clockdist.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 11) (name "/Expansion Bus/") (tstamps /5E813DC5/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-06-23)
        (source expansion.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 12) (name "/Power & Decoupling/") (tstamps /5E9E4C57/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-04)
        (source power.sch)
        (comment (number 1) (value "POWER AND DECOUPLING"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 13) (name "/Real-Time Clock/") (tstamps /5CF615AB/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2019-04-23)
        (source rtc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2"))))
    (sheet (number 14) (name "/Trapdoor Expansion/") (tstamps /5D00C589/)
      (title_block
        (title Rämixx500)
        (company SukkoPera)
        (rev 1)
        (date 2020-04-05)
        (source trapdoor.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "Licensed under CERN OHL v.1.2")))))
  (components
    (comp (ref V0)
      (value OSHW_LOGO)
      (footprint Symbol:OSHW-Logo2_14.6x12mm_SilkScreen)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib void) (part Void) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED3E7FB))
    (comp (ref V1)
      (value KICAD_LOGO)
      (footprint Symbol:KiCad-Logo2_8mm_SilkScreen)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib void) (part Void) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED79790))
    (comp (ref V2)
      (value PROJ_LOGO)
      (footprint Raemixx500:Logo)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib void) (part Void) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EB0B2BE))
    (comp (ref R114)
      (value 68)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CAEA43A))
    (comp (ref U2)
      (value FAT_AGNUS_8375)
      (footprint Package_LCC:PLCC-84_THT-Socket)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CUSTOM))
      (libsource (lib FAT_AGNUS_8375) (part FAT_AGNUS_8375) (description ""))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CAEC18D))
    (comp (ref R103)
      (value 47)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CAF1F56))
    (comp (ref R104)
      (value 47)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CAF26DB))
    (comp (ref R105)
      (value 47)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CAF27C4))
    (comp (ref U37)
      (value 74LS32)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS32)
      (fields
        (field (name Cost) 0.442)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS32N)
        (field (name Optional) PARALLEL/FLOPPY/KEYBOARD))
      (libsource (lib 74xx) (part 74LS32) (description "Quad 2-input OR"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CB489DB))
    (comp (ref JP2)
      (value Jumper_3_Bridged23)
      (footprint Raemixx500:Jumper3-Bridged23)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper_3_Bridged23) (part Jumper_3_Bridged23) (description "Jumper, 3-pole, pins 1+2 closed/bridged"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CB6FAD7))
    (comp (ref R106)
      (value 47)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CCACD78))
    (comp (ref R107)
      (value 47)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CCBE5F9))
    (comp (ref C99)
      (value 100n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.035)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA115C104KAR))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CCD0386))
    (comp (ref R101)
      (value 27)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CD17492))
    (comp (ref R102)
      (value 27)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CD4EF32))
    (comp (ref U1)
      (value 68000D)
      (footprint Package_DIP:DIP-64_W22.86mm_Socket_LongPads)
      (datasheet https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf)
      (fields
        (field (name Optional) CPU))
      (libsource (lib 68000D) (part 68000D) (description "16/32-bit Microprocessor"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CDC0BF7))
    (comp (ref U13)
      (value 74LS373)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS373)
      (fields
        (field (name Cost) 0.68)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS373N)
        (field (name Optional) MEMORY))
      (libsource (lib 74ls373) (part 74LS373) (description "8-bit Latch, 3-state outputs"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CFCEC13))
    (comp (ref U11)
      (value 74LS373)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS373)
      (fields
        (field (name Cost) 0.68)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS373N)
        (field (name Optional) MEMORY))
      (libsource (lib 74ls373) (part 74LS373) (description "8-bit Latch, 3-state outputs"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CFF7EAA))
    (comp (ref R113)
      (value 47)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D0A2B83))
    (comp (ref R112)
      (value 68)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D0A2CB9))
    (comp (ref R111)
      (value 68)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D0A2D42))
    (comp (ref U10)
      (value 74LS244)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS244)
      (fields
        (field (name Cost) 0.62)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS244N)
        (field (name Optional) MEMORY))
      (libsource (lib 74ls244) (part 74LS244) (description "8-bit Bus Buffer 3-State outputs"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D116EA8))
    (comp (ref U12)
      (value 74LS244)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS244)
      (fields
        (field (name Cost) 0.62)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS244N)
        (field (name Optional) MEMORY))
      (libsource (lib 74ls244) (part 74LS244) (description "8-bit Bus Buffer 3-State outputs"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D188F20))
    (comp (ref U5)
      (value GARY_5719)
      (footprint Package_DIP:DIP-48_W15.24mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CUSTOM))
      (libsource (lib GARY) (part GARY_5719) (description ""))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 607A12E7))
    (comp (ref U33)
      (value 74LS258)
      (footprint Package_DIP:DIP-16_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS258)
      (fields
        (field (name "MFG Name") N/A)
        (field (name Optional) CLOCK))
      (libsource (lib 74ls258) (part 74LS258) (description "Quad 2 to 1 Multiplexer, inverting"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CBE9A78))
    (comp (ref E666)
      (value 22p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.141)
        (field (name EMI_FILTER_TYPE) C)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA102A220JARC)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5CC5EA40))
    (comp (ref X1)
      (value XTAL)
      (footprint Oscillator:Oscillator_DIP-14)
      (datasheet http://www.txccorp.com/download/products/osc/7C_o.pdf)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib xtal) (part XTAL) (description "Crystal Clock Oscillator"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D05A737))
    (comp (ref FB101)
      (value 68)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D645153))
    (comp (ref FB102)
      (value 150)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names /CPU+Agnus/) (tstamps /5CAE5331/))
      (tstamp 5D8302E3))
    (comp (ref U34)
      (value 74LS373)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS373)
      (fields
        (field (name Cost) 0.68)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS373N)
        (field (name Optional) MEMORY))
      (libsource (lib 74ls373) (part 74LS373) (description "8-bit Latch, 3-state outputs"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5EB19726))
    (comp (ref U35)
      (value 74LS244)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS244)
      (fields
        (field (name Cost) 0.62)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS244N)
        (field (name Optional) MEMORY))
      (libsource (lib 74ls244) (part 74LS244) (description "8-bit Bus Buffer 3-State outputs"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5EB9A376))
    (comp (ref RP201)
      (value 68)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R_Pack05_SIP) (description "5 resistor network, parallel topology, SIP package"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5EF1C367))
    (comp (ref RP202)
      (value 68)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R_Pack05_SIP) (description "5 resistor network, parallel topology, SIP package"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5EF1C6CE))
    (comp (ref RP203)
      (value 68)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R_Pack05_SIP) (description "5 resistor network, parallel topology, SIP package"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5F5CC2F4))
    (comp (ref U32)
      (value 74LS139)
      (footprint Package_DIP:DIP-16_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS139)
      (fields
        (field (name Cost) 0.615)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS139AN)
        (field (name Optional) MEMORY))
      (libsource (lib 74xx) (part 74LS139) (description "Dual Decoder 1 of 4, Active low outputs"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5CF5939E))
    (comp (ref JP3A1)
      (value Jumper_2_Bridged)
      (footprint Raemixx500:Jumper2-Bridged)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_2_Bridged) (description "Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D453E68))
    (comp (ref JP3B1)
      (value Jumper_2_Bridged)
      (footprint Raemixx500:Jumper2-Bridged)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_2_Bridged) (description "Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D4540CC))
    (comp (ref R201)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D708549))
    (comp (ref R202)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D708798))
    (comp (ref U16)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D1C956E))
    (comp (ref U17)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D4117A6))
    (comp (ref U18)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D42DBCB))
    (comp (ref U19)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D42DBD1))
    (comp (ref U20)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D805FD5))
    (comp (ref U21)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D805FDB))
    (comp (ref U22)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D805FE1))
    (comp (ref U23)
      (value XX4256)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) MEMORY))
      (libsource (lib XX4256) (part XX4256) (description ""))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5D805FE7))
    (comp (ref JP4A1)
      (value Jumper_3_Open)
      (footprint Raemixx500:Jumper3-Open)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_3_Open) (description "Jumper, 3-pole, both open"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5DCD8A02))
    (comp (ref JP4B1)
      (value Jumper_3_Open)
      (footprint Raemixx500:Jumper3-Open)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_3_Open) (description "Jumper, 3-pole, both open"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5E08E93D))
    (comp (ref C16)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5CCC91AE))
    (comp (ref C17)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5CD19B3E))
    (comp (ref C20)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5CD69C13))
    (comp (ref C18)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5CF36D58))
    (comp (ref C19)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /RAM/) (tstamps /5EA8075B/))
      (tstamp 5CF36D6A))
    (comp (ref U4)
      (value DENISE)
      (footprint Package_DIP:DIP-48_W15.24mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CUSTOM))
      (libsource (lib DENISE) (part DENISE) (description ""))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CBA56DB))
    (comp (ref C403)
      (value 47p)
      (footprint Raemixx500:VariCap)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP))
      (libsource (lib Device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CBE4324))
    (comp (ref U40)
      (value 74LS245)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS245)
      (fields
        (field (name Cost) 0.311)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") CD74ACT245E)
        (field (name Optional) VIDEO))
      (libsource (lib 74ls245) (part 74LS245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CBE8812))
    (comp (ref U41)
      (value 74LS245)
      (footprint Package_DIP:DIP-20_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS245)
      (fields
        (field (name Cost) 0.311)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") CD74ACT245E)
        (field (name Optional) VIDEO))
      (libsource (lib 74ls245) (part 74LS245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CBF1E4C))
    (comp (ref HY1)
      (value VIDIOT)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x22_P2.54mm_Vertical)
      (datasheet DOCUMENTATION)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) VID))
      (libsource (lib VIDIOT) (part VIDIOT) (description "Video DAC"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CC01A68))
    (comp (ref RP402)
      (value 47)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet ~)
      (libsource (lib r_pack05) (part R_Pack05) (description "5 resistor network, parallel topology, DIP package"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CD1046C))
    (comp (ref RP403)
      (value 47)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet ~)
      (libsource (lib r_pack05) (part R_Pack05) (description "5 resistor network, parallel topology, DIP package"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CD10554))
    (comp (ref CN9)
      (value VIDEO_DB23M)
      (footprint Raemixx500:DB_23M)
      (datasheet " ~")
      (fields
        (field (name Optional) VIDEO))
      (libsource (lib db23_male_mountingholes) (part DB23_Male_MountingHoles) (description "25-pin male D-SUB connector, Mounting Hole"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CE70E09))
    (comp (ref E405)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CE8B2B2))
    (comp (ref E403)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CF24BA0))
    (comp (ref E404)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5CF24C8A))
    (comp (ref E402)
      (value 150p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.238)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") "DSS1NB32A151Q91A ")
        (field (name Optional) VIDEO))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D034FA1))
    (comp (ref E434)
      (value 150p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.238)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") "DSS1NB32A151Q91A ")
        (field (name Optional) VIDEO))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D0EFA81))
    (comp (ref R402)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D1737A4))
    (comp (ref R403)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D17FD6E))
    (comp (ref R404)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D17FFDB))
    (comp (ref E406)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D176766))
    (comp (ref C4)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) VIDEO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D1BC11B))
    (comp (ref R406)
      (value 4.7)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D2C11FC))
    (comp (ref C402)
      (value 1000u)
      (footprint Capacitor_THT:CP_Radial_D12.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.343)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1C102))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D34A65C))
    (comp (ref C40)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) VIDEO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D38ACBD))
    (comp (ref C41)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) VIDEO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D39B62F))
    (comp (ref C401)
      (value 1000u)
      (footprint Capacitor_THT:CP_Radial_D12.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.343)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1C102))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D43E808))
    (comp (ref R405)
      (value 0.47)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D4670F1))
    (comp (ref JP11)
      (value Jumper_3_Bridged12)
      (footprint Raemixx500:Jumper3-Bridged12)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_3_Bridged12) (description "Jumper, 3-pole, pins 1+2 closed/bridged"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D80F9A3))
    (comp (ref R409)
      (value 150)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5DA05B94))
    (comp (ref HY2)
      (value COLOR_ANNEX)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet https://github.com/SukkoPera/OpenAmigaVideoHybrid)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) VID))
      (libsource (lib VIDIOT) (part VIDIOT_ANNEX) (description "Video DAC Color Annex"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5D5227DD))
    (comp (ref E433)
      (value FERR)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.129)
        (field (name EMI_FILTER_TYPE) FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") BL02RN2R1M2B)
        (field (name Optional) VIDEO))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5DD342FD))
    (comp (ref E431)
      (value FERR)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.129)
        (field (name EMI_FILTER_TYPE) FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") BL02RN2R1M2B)
        (field (name Optional) VIDEO))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5DD4BEEC))
    (comp (ref E432)
      (value FERR)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.129)
        (field (name EMI_FILTER_TYPE) FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") BL02RN2R1M2B)
        (field (name Optional) VIDEO))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5DD7EF86))
    (comp (ref E435)
      (value FERR)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.129)
        (field (name EMI_FILTER_TYPE) FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") BL02RN2R1M2B)
        (field (name Optional) VIDEO))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5DF6B27A))
    (comp (ref CN10)
      (value COMPOSITE)
      (footprint Raemixx500:SWITCHCRAFT_PJRAN1X1U01X)
      (datasheet A)
      (fields
        (field (name Field4) Switchcraft)
        (field (name Field5) 13mm)
        (field (name Field6) "Manufacturer Recommendations")
        (field (name Optional) VIDEO))
      (libsource (lib PJRAN1X1U01X) (part PJRAN1X1U01X) (description ""))
      (sheetpath (names "/Denise & Video Stuff/") (tstamps /5CBA5669/))
      (tstamp 5FB5AA2B))
    (comp (ref U3)
      (value PAULA)
      (footprint Package_DIP:DIP-48_W15.24mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CUSTOM))
      (libsource (lib PAULA) (part PAULA) (description ""))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D2DD129))
    (comp (ref FB802)
      (value Ferrite_Bead_Small)
      (footprint Raemixx500:Ferrite_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) FERRITE))
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D2F2A18))
    (comp (ref CN1)
      (value LEFT_JOY)
      (footprint Raemixx500:DB_9M)
      (datasheet " ~")
      (fields
        (field (name Optional) JOYSTICK))
      (libsource (lib db9_male_mountingholes) (part DB9_Male_MountingHoles) (description "9-pin male D-SUB connector, Mounting Hole"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D2FF5E8))
    (comp (ref C411)
      (value 1000p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.083)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA101C102KAR))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D30478C))
    (comp (ref C413)
      (value 1000p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.083)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA101C102KAR))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D3068BD))
    (comp (ref C412)
      (value 1000p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.083)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA101C102KAR))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D306919))
    (comp (ref E416)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D321710))
    (comp (ref E417)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D32E41F))
    (comp (ref R401)
      (value 4.7)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D349E96))
    (comp (ref JP8)
      (value Jumper_3_Bridged23)
      (footprint Raemixx500:Jumper3-Bridged23)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper_3_Bridged23) (part Jumper_3_Bridged23) (description "Jumper, 3-pole, pins 1+2 closed/bridged"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D355FA7))
    (comp (ref CN2)
      (value RIGHT_JOY)
      (footprint Raemixx500:DB_9M)
      (datasheet " ~")
      (fields
        (field (name Optional) JOYSTICK))
      (libsource (lib db9_male_mountingholes) (part DB9_Male_MountingHoles) (description "9-pin male D-SUB connector, Mounting Hole"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC00))
    (comp (ref C421)
      (value 1000p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.083)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA101C102KAR))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC07))
    (comp (ref C423)
      (value 1000p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.083)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA101C102KAR))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC0D))
    (comp (ref C422)
      (value 1000p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.083)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA101C102KAR))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC13))
    (comp (ref E425)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC19))
    (comp (ref E427)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC3A))
    (comp (ref R408)
      (value 4.7)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC4A))
    (comp (ref E411)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D3C0092))
    (comp (ref E412)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D3C0098))
    (comp (ref E413)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D3C009E))
    (comp (ref U15)
      (value 74LS157)
      (footprint Package_DIP:DIP-16_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS157)
      (fields
        (field (name Cost) 0.236)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74HCT157NE4)
        (field (name Optional) JOYSTICK))
      (libsource (lib 74ls157) (part 74LS157) (description "Quad 2 to 1 line Multiplexer"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D4839EA))
    (comp (ref E421)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D4B014E))
    (comp (ref E422)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D4B0154))
    (comp (ref E424)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D4B0160))
    (comp (ref E441)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D569D5D))
    (comp (ref E443)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D569D63))
    (comp (ref E444)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D569D69))
    (comp (ref E442)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D569D6F))
    (comp (ref RP401)
      (value 4.7K)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D5E405F))
    (comp (ref C312)
      (value 47n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.284)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C473M5U5TA))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D717C7F))
    (comp (ref C311)
      (value 47n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.284)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C473M5U5TA))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D717C85))
    (comp (ref C314)
      (value 47n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.284)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C473M5U5TA))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D717C8B))
    (comp (ref C313)
      (value 47n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.284)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C473M5U5TA))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D774DDD))
    (comp (ref U14)
      (value LF347)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/ds/symlink/tl081.pdf)
      (fields
        (field (name Cost) 0.58)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") "LF347N ???")
        (field (name Optional) AUDIO))
      (libsource (lib Amplifier_Operational) (part TL084) (description "Quad JFET-Input Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D83683C))
    (comp (ref E305)
      (value 270p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A271Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D84A977))
    (comp (ref E306)
      (value 270p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A271Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D84AEBD))
    (comp (ref R321)
      (value 360)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D86E35E))
    (comp (ref C321)
      (value 100n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.035)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA115C104KAR))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D86E851))
    (comp (ref R322)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D904F4A))
    (comp (ref R323)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D9182BF))
    (comp (ref C322)
      (value 6800p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C430C682J5G5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D953C8A))
    (comp (ref C325)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D9E475D))
    (comp (ref C324)
      (value 22u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.118)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H220))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D9E4B3B))
    (comp (ref R324)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DA8E858))
    (comp (ref R325)
      (value 390)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DABA92A))
    (comp (ref E302)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DABAC82))
    (comp (ref Q321)
      (value MPF102)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet ~)
      (libsource (lib Device) (part Q_NJFET_DSG) (description "N-JFET transistor, drain/source/gate"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD1A1D0))
    (comp (ref R326)
      (value 470k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD32AED))
    (comp (ref R331)
      (value 360)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A170))
    (comp (ref C331)
      (value 100n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.035)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA115C104KAR))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A176))
    (comp (ref R332)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A18B))
    (comp (ref R333)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A191))
    (comp (ref C332)
      (value 6800p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C430C682J5G5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A198))
    (comp (ref C335)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A1AB))
    (comp (ref C334)
      (value 22u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.118)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H220))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A1B1))
    (comp (ref R334)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A1C2))
    (comp (ref R335)
      (value 390)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A1C8))
    (comp (ref E303)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A1CE))
    (comp (ref Q331)
      (value MPF102)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet ~)
      (libsource (lib Device) (part Q_NJFET_DSG) (description "N-JFET transistor, drain/source/gate"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A206))
    (comp (ref R336)
      (value 470k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DD9A20C))
    (comp (ref C323)
      (value 3900p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name "MFG Name") N/A))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DE6979A))
    (comp (ref C333)
      (value 3900p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name "MFG Name") N/A))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DEF165B))
    (comp (ref C308)
      (value 10n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DFE684E))
    (comp (ref Q301)
      (value 2N3906)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet ~)
      (libsource (lib Device) (part Q_PNP_EBC) (description "PNP transistor, emitter/base/collector"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E02E0E4))
    (comp (ref R308)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E0778F5))
    (comp (ref R306)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E0EAE10))
    (comp (ref R305)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E111042))
    (comp (ref U38)
      (value MC1488)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Cost) 0.615)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") MC1488N)
        (field (name Optional) SERIAL))
      (libsource (lib MC1488) (part MC1488) (description "Quad Line EIA-232D Driver"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E3403B1))
    (comp (ref R307)
      (value 2.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E52C868))
    (comp (ref JP10B1)
      (value Jumper_2_Bridged)
      (footprint Raemixx500:Jumper2-Bridged)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_2_Bridged) (description "Jumper, 2-pole, closed/bridged"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E55F219))
    (comp (ref JP10A1)
      (value Jumper_2_Bridged)
      (footprint Raemixx500:Jumper2-Bridged)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_2_Bridged) (description "Jumper, 2-pole, closed/bridged"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E5BD1DB))
    (comp (ref R339)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5E5EC393))
    (comp (ref R309)
      (value 10)
      (footprint Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D5A8497))
    (comp (ref C3)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D66BD3B))
    (comp (ref R303)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D66BD4F))
    (comp (ref C307)
      (value 1000u)
      (footprint Capacitor_THT:CP_Radial_D12.5mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.343)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1C102))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D66BD59))
    (comp (ref R304)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D9BBA0A))
    (comp (ref C305)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DA271C0))
    (comp (ref C306)
      (value 10u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.196)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H100))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DA271CB))
    (comp (ref R301)
      (value 10)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DB48BB9))
    (comp (ref R302)
      (value 10)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DBF49FE))
    (comp (ref C301)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DCA385C))
    (comp (ref C303)
      (value 22u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.118)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H220))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DCA3862))
    (comp (ref C302)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DCDDA3D))
    (comp (ref C304)
      (value 22u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.118)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H220))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5DCDDA43))
    (comp (ref C15)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5EC8858D))
    (comp (ref E414)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D3C00A6))
    (comp (ref E423)
      (value 6800p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A682Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D4B015A))
    (comp (ref E408)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC1F))
    (comp (ref E401)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A)
        (field (name Optional) JOYSTICK))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D3215BB))
    (comp (ref E426)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D36BC25))
    (comp (ref E415)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5D32038D))
    (comp (ref CN3)
      (value RIGHT)
      (footprint Raemixx500:SWITCHCRAFT_PJRAN1X1U01X)
      (datasheet A)
      (fields
        (field (name Field4) Switchcraft)
        (field (name Field5) 13mm)
        (field (name Field6) "Manufacturer Recommendations")
        (field (name Optional) AUDIO))
      (libsource (lib PJRAN1X1U01X) (part PJRAN1X1U01X) (description ""))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5F7C1CDB))
    (comp (ref CN4)
      (value LEFT)
      (footprint Raemixx500:SWITCHCRAFT_PJRAN1X1U01X)
      (datasheet A)
      (fields
        (field (name Field4) Switchcraft)
        (field (name Field5) 13mm)
        (field (name Field6) "Manufacturer Recommendations")
        (field (name Optional) AUDIO))
      (libsource (lib PJRAN1X1U01X) (part PJRAN1X1U01X) (description ""))
      (sheetpath (names "/Paula & Audio Stuff/") (tstamps /5D2DC3A1/))
      (tstamp 5FA7359A))
    (comp (ref U7)
      (value VIA_8520)
      (footprint Package_DIP:DIP-40_W15.24mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CUSTOM))
      (libsource (lib VIA_8520) (part VIA_8520) (description ""))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E7EC434))
    (comp (ref U8)
      (value VIA_8520)
      (footprint Package_DIP:DIP-40_W15.24mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CUSTOM))
      (libsource (lib VIA_8520) (part VIA_8520) (description ""))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E7EF4F3))
    (comp (ref CN7)
      (value PARALLEL_DB25F)
      (footprint Raemixx500:DB_25F)
      (datasheet " ~")
      (fields
        (field (name Optional) PARALLEL))
      (libsource (lib db25_female_mountingholes) (part DB25_Female_MountingHoles) (description "25-pin female D-SUB connector, Mounting Hole"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8537DA))
    (comp (ref E520)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) PARALLEL))
      (libsource (lib Device) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E87A0B8))
    (comp (ref E511)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8B3D41))
    (comp (ref E512)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8B3DEE))
    (comp (ref E513)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8BE123))
    (comp (ref E514)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8BE129))
    (comp (ref E515)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C3235))
    (comp (ref E516)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C323B))
    (comp (ref E517)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C3243))
    (comp (ref E518)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C3249))
    (comp (ref E519)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C665E))
    (comp (ref E521)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C6664))
    (comp (ref E522)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C666C))
    (comp (ref E523)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C6672))
    (comp (ref E524)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8C667A))
    (comp (ref RP501)
      (value 10k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (fields
        (field (name Optional) KEYBOARD/FLOPPY/PARALLEL/MEMORY))
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E9781E7))
    (comp (ref CN6)
      (value SERIAL_DB25M)
      (footprint Raemixx500:DB_25M)
      (datasheet " ~")
      (fields
        (field (name Optional) SERIAL))
      (libsource (lib db25_male_mountingholes) (part DB25_Male_MountingHoles) (description "25-pin male D-SUB connector, Mounting Hole"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EBF2D7E))
    (comp (ref E532)
      (value 150p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.238)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") "DSS1NB32A151Q91A ")
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EC70ADB))
    (comp (ref E534)
      (value 150p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.238)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") "DSS1NB32A151Q91A ")
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EC70AE1))
    (comp (ref E533)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EC70AE9))
    (comp (ref E535)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EC70AEF))
    (comp (ref E537)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EC70B04))
    (comp (ref C501)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) SERIAL))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EE8C5DF))
    (comp (ref C502)
      (value 330n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) SERIAL))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EEC226F))
    (comp (ref E531)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F003110))
    (comp (ref E538)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F05121C))
    (comp (ref R109)
      (value 68)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) PARALLEL/SERIAL/FLOPPY))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F08C983))
    (comp (ref Q501)
      (value 2N3904)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (fields
        (field (name Optional) SERIAL))
      (libsource (lib Transistor_BJT) (part 2N3904) (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F0CC7D2))
    (comp (ref R502)
      (value 2.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) SERIAL))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F0F6026))
    (comp (ref D501)
      (value 1N4148)
      (footprint Diode_THT:D_DO-35_SOD27_P12.70mm_Horizontal)
      (datasheet http://www.nxp.com/documents/data_sheet/1N4148_1N4448.pdf)
      (fields
        (field (name Optional) SERIAL))
      (libsource (lib Diode) (part 1N4148) (description "100V 0.15A standard switching diode, DO-35"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F134D2F))
    (comp (ref R501)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) SERIAL))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F149CBE))
    (comp (ref U39)
      (value MC1489)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Cost) 0.668)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") MC1489N)
        (field (name Optional) SERIAL))
      (libsource (lib mc1489) (part MC1489) (description "Quad Line EIA-232D Receivers"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F30DED7))
    (comp (ref C39)
      (value 10n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F6A3A58))
    (comp (ref R504)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F8814B9))
    (comp (ref R506)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F8818E1))
    (comp (ref Q503)
      (value 2N3906)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Transistor_BJT) (part 2N3906) (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F8DE53A))
    (comp (ref CN13)
      (value KEYBOARD)
      (footprint Raemixx500:Keyboard_Connector)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib conn) (part CONN_8) (description "Symbole general de connecteur"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5F93CF11))
    (comp (ref R503)
      (value 4.7k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FA8F09B))
    (comp (ref R505)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FA8F0A1))
    (comp (ref Q502)
      (value 2N3906)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Transistor_BJT) (part 2N3906) (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FA8F0B2))
    (comp (ref R507)
      (value 100)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) KEYBOARD))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FBBDEB1))
    (comp (ref E632)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) KEYBOARD))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FC0C8A2))
    (comp (ref E631)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)")
        (field (name Optional) KEYBOARD))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FD0A3D9))
    (comp (ref U42)
      (value NE555)
      (footprint Package_DIP:DIP-8_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/ds/symlink/ne555.pdf)
      (fields
        (field (name Cost) 0.315)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") NE555P)
        (field (name Optional) POR))
      (libsource (lib ne555) (part NE555) (description "Timer, DIP-8/SOIC-8/SSOP-8"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FF90A64))
    (comp (ref R712)
      (value 47K)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) POR))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FFFE029))
    (comp (ref R711)
      (value 1M)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) POR))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5FFFE3DD))
    (comp (ref C713)
      (value 10n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO)
        (field (name Optional) POR))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 6020FC2F))
    (comp (ref Q711)
      (value 2N3904)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (fields
        (field (name Optional) POR))
      (libsource (lib Transistor_BJT) (part 2N3904) (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 602F87A0))
    (comp (ref JP1)
      (value Jumper_2_Bridged)
      (footprint Raemixx500:Jumper2-Bridged)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_2_Bridged) (description "Jumper, 2-pole, closed/bridged"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 6034771D))
    (comp (ref C42)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) POR))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 6050811F))
    (comp (ref C7)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EA2573B))
    (comp (ref C8)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EA25E9D))
    (comp (ref R713)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) POR))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5CFD0A7C))
    (comp (ref E536)
      (value 470p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A471Q91A)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EC70AF7))
    (comp (ref E502)
      (value "47 1/2W")
      (footprint Raemixx500:EMI_Filter_Longer)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E0EA71F))
    (comp (ref E503)
      (value "47 1/2W")
      (footprint Raemixx500:EMI_Filter_Longer)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) SERIAL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E0EA729))
    (comp (ref E501)
      (value "47 1/2W")
      (footprint Raemixx500:EMI_Filter_Longer)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) PARALLEL))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E3D78DB))
    (comp (ref JP7B1)
      (value Jumper_3_Bridged23)
      (footprint Raemixx500:Jumper3-Bridged23)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper_3_Bridged23) (part Jumper_3_Bridged23) (description "Jumper, 3-pole, pins 1+2 closed/bridged"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5E8A9D97))
    (comp (ref C712)
      (value 10u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.196)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H100)
        (field (name Optional) POR))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EBE40E3))
    (comp (ref C711)
      (value 100n)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.035)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA115C104KAR)
        (field (name Optional) POR))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EBE45B6))
    (comp (ref J90)
      (value DRIVE_SWITCHER)
      (footprint Raemixx500:DriveSwitchHeader)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x03_Odd_Even) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/Parallel & Serial/") (tstamps /5E7E9EC4/))
      (tstamp 5EFAA487))
    (comp (ref U36)
      (value 74LS05)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (datasheet http://www.ti.com/lit/gpn/sn74LS05)
      (fields
        (field (name Cost) 0.668)
        (field (name "MFG Name") TI)
        (field (name "MFG Part Num") SN74LS05N)
        (field (name Optional) FLOPPY/RTC))
      (libsource (lib 74xx) (part 74LS05) (description "Inverter Open Collect"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 607A3EC8))
    (comp (ref CN12)
      (value FLOPPY_POWER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (fields
        (field (name Optional) FLOPPY))
      (libsource (lib conn) (part CONN_4) (description "Symbole general de connecteur"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 607A922B))
    (comp (ref CN11)
      (value INTERNAL_FLOPPY)
      (footprint Connector_IDC:IDC-Header_2x17_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name Optional) FLOPPY))
      (libsource (lib Connector_Generic) (part Conn_02x17_Odd_Even) (description "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5CB7C0D7))
    (comp (ref CN5)
      (value EXTFLOPPY_DB23F)
      (footprint Raemixx500:DB_23F)
      (datasheet " ~")
      (fields
        (field (name Optional) FLOPPY))
      (libsource (lib db23_mountingholes_2sides) (part DB23_MountingHoles_2sides) (description "25-pin male D-SUB connector, Mounting Hole"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D5C4F68))
    (comp (ref E613)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6431F2))
    (comp (ref E614)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6431F9))
    (comp (ref E615)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D643201))
    (comp (ref E616)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D643208))
    (comp (ref E601)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D643210))
    (comp (ref E611)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D693C4F))
    (comp (ref E612)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D693C55))
    (comp (ref E617)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6A84E5))
    (comp (ref E618)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6A84EB))
    (comp (ref E619)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6A84F2))
    (comp (ref E620)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6A84F8))
    (comp (ref E621)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6CA78C))
    (comp (ref E622)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6CA792))
    (comp (ref E623)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6CA799))
    (comp (ref E624)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6CA79F))
    (comp (ref E625)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6D1FA1))
    (comp (ref E626)
      (value 100p)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.233)
        (field (name EMI_FILTER_TYPE) NORMAL)
        (field (name "MFG Part Num") "DSS1NB32A101Q91A (has ferrite)"))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6D1FA7))
    (comp (ref E602)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D6D1FAE))
    (comp (ref CN15)
      (value IDE_I/F)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP))
      (libsource (lib conn) (part CONN_4) (description "Symbole general de connecteur"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D746087))
    (comp (ref CN14)
      (value IDE_POWER)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP))
      (libsource (lib conn) (part CONN_4) (description "Symbole general de connecteur"))
      (sheetpath (names "/Floppy Drives/") (tstamps /6072A453/))
      (tstamp 5D7501AC))
    (comp (ref RP107)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6D64EB))
    (comp (ref RP106)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6D7AD8))
    (comp (ref RP105)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6DB666))
    (comp (ref RP108)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6E5956))
    (comp (ref RP110)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6E5AC0))
    (comp (ref RP109)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6F5285))
    (comp (ref RP111)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D6F528B))
    (comp (ref RP102)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D7152A6))
    (comp (ref R192)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D73ED8F))
    (comp (ref R191)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D749EFE))
    (comp (ref RP101)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D756FA0))
    (comp (ref RP104)
      (value 4.7k)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet http://www.vishay.com/docs/31509/csc.pdf)
      (libsource (lib Device) (part R_Network09) (description "9 resistor network, star topology, bussed resistors, small symbol"))
      (sheetpath (names "/Termination & Pullups/") (tstamps /5D6D5EBE/))
      (tstamp 5D756FA6))
    (comp (ref U6)
      (value ROM)
      (footprint Package_DIP:DIP-42_W15.24mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) ROM))
      (libsource (lib AMIGA_ROM) (part AMIGA_ROM) (description ""))
      (sheetpath (names "/Kickstart ROM/") (tstamps /5D86DD46/))
      (tstamp 5D8766E5))
    (comp (ref C6)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Kickstart ROM/") (tstamps /5D86DD46/))
      (tstamp 5E9EA8DA))
    (comp (ref J91)
      (value Dispatcher_3to1)
      (footprint Raemixx500:Dispatcher_3to1)
      (datasheet ~)
      (libsource (lib Dispatcher) (part Dispatcher_3to1) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/Kickstart ROM/") (tstamps /5D86DD46/))
      (tstamp 5F631089))
    (comp (ref J92)
      (value Dispatcher_3to1)
      (footprint Raemixx500:Dispatcher_3to1)
      (datasheet ~)
      (libsource (lib Dispatcher) (part Dispatcher_3to1) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/Kickstart ROM/") (tstamps /5D86DD46/))
      (tstamp 5F63D7FD))
    (comp (ref J93)
      (value Dispatcher_3to1)
      (footprint Raemixx500:Dispatcher_3to1)
      (datasheet ~)
      (libsource (lib Dispatcher) (part Dispatcher_3to1) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/Kickstart ROM/") (tstamps /5D86DD46/))
      (tstamp 5F64035F))
    (comp (ref RP103)
      (value 39)
      (footprint Resistor_THT:R_Array_SIP10)
      (datasheet ~)
      (fields
        (field (name Optional) CLOCK))
      (libsource (lib r_pack05) (part R_Pack05) (description "5 resistor network, parallel topology, DIP package"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5D89736C))
    (comp (ref C33)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5EFD7963))
    (comp (ref E793)
      (value 47p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEDC355))
    (comp (ref E792)
      (value 47p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEDC35C))
    (comp (ref E791)
      (value 47p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEDC363))
    (comp (ref E109)
      (value 47p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEDC36A))
    (comp (ref E102)
      (value 47p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEDC371))
    (comp (ref E106)
      (value 47p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEEB0AC))
    (comp (ref E107)
      (value 47p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEEB0B2))
    (comp (ref E108)
      (value 47p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CEEB0B8))
    (comp (ref E794)
      (value 47p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CF1A8D8))
    (comp (ref E103)
      (value 47p)
      (footprint Raemixx500:C_Axial_L9.0mm_D3.2mm_P12.70mm)
      (datasheet ~)
      (fields
        (field (name EMI_FILTER_TYPE) C)
        (field (name Optional) CLOCK))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5CF1A8DE))
    (comp (ref E407)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A)
        (field (name Optional) CLOCK))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5EFD7951))
    (comp (ref E105)
      (value 68)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) CLOCK))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5D5D787F))
    (comp (ref E104)
      (value 68)
      (footprint Raemixx500:EMI_Filter_Long)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name EMI_FILTER_TYPE) R)
        (field (name Optional) CLOCK))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Clock Distribution/") (tstamps /5D88EC26/))
      (tstamp 5D5EAC36))
    (comp (ref P1)
      (value "EXPANSION BUS")
      (footprint Raemixx500:A2000_COPRO_SLOT)
      (datasheet DOCUMENTATION)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) CONN))
      (libsource (lib BUSEXP) (part BUSEXP) (description ""))
      (sheetpath (names "/Expansion Bus/") (tstamps /5E813DC5/))
      (tstamp 5E8156AA))
    (comp (ref E702)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Expansion Bus/") (tstamps /5E813DC5/))
      (tstamp 5E90E8D4))
    (comp (ref E703)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Expansion Bus/") (tstamps /5E813DC5/))
      (tstamp 5E93673B))
    (comp (ref E704)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Expansion Bus/") (tstamps /5E813DC5/))
      (tstamp 5E953633))
    (comp (ref C14)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EE9C954))
    (comp (ref C1)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) CPU))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EE9C9F2))
    (comp (ref E101)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EE9CBC5))
    (comp (ref C2)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EE9CD5A))
    (comp (ref E110)
      (value 10n)
      (footprint Raemixx500:EMI_Filter_Short)
      (datasheet http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (fields
        (field (name Cost) 0.234)
        (field (name EMI_FILTER_TYPE) W/FERRITE)
        (field (name "MFG Name") MURATA)
        (field (name "MFG Part Num") DSS1NB32A103Q91A))
      (libsource (lib emi_filter_lcl_small) (part EMI_Filter_LCL) (description "EMI T-filter (LCL)"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EE9D7A0))
    (comp (ref C701)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EE9D8C8))
    (comp (ref C5)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EEA6467))
    (comp (ref C11)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EED266B))
    (comp (ref C13)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EED4AB7))
    (comp (ref C10)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EED4BCE))
    (comp (ref C12)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EED4C9E))
    (comp (ref C32)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EF06334))
    (comp (ref C34)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EF1227E))
    (comp (ref C35)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO)
        (field (name Optional) MEMORY))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EF1ED46))
    (comp (ref C36)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EF234DA))
    (comp (ref C37)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5EF27F5A))
    (comp (ref CN8)
      (value POWER)
      (footprint Raemixx500:DS215+DIN8_COMBO)
      (datasheet ~)
      (fields
        (field (name Optional) POWER))
      (libsource (lib amipower) (part Amiga_Power_Conn) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CC1E93B))
    (comp (ref LF1)
      (value L)
      (footprint Raemixx500:LineFilter)
      (datasheet ~)
      (fields
        (field (name Optional) POWER))
      (libsource (lib linefilter) (part L) (description "Line Filter"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CC2D6BF))
    (comp (ref C802)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CC97A36))
    (comp (ref C821)
      (value 47u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.137)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H470))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CCACA7E))
    (comp (ref C803)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CCB3CDE))
    (comp (ref C822)
      (value 47u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.137)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H470))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CCC257D))
    (comp (ref C801)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD42F0C))
    (comp (ref C804)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD81FFE))
    (comp (ref C811)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.265)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H101))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD822B9))
    (comp (ref C812)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.265)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H101))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD82551))
    (comp (ref C813)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.265)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H101))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD82607))
    (comp (ref C814)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.265)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H101))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD8AD69))
    (comp (ref C815)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.265)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H101))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD8AD6F))
    (comp (ref C816)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.265)
        (field (name "MFG Name") PANASONIC)
        (field (name "MFG Part Num") EEUFR1H101))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CD8AD75))
    (comp (ref MT1)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_4mm_Pad)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CDEC3BD))
    (comp (ref MT2)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_4mm_Pad)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CDEC70A))
    (comp (ref MT4)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_4mm_Pad)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CDECB1F))
    (comp (ref MT5)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_4mm_Pad)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CDECB25))
    (comp (ref MT6)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_4mm_Pad)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CDF7576))
    (comp (ref MT7)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_4mm_Pad)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) SKIP))
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5CDF757C))
    (comp (ref C800)
      (value 10n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.071)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C410C103K1H5TAAUTO))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/Power & Decoupling/") (tstamps /5E9E4C57/))
      (tstamp 5D4BE8BA))
    (comp (ref U9)
      (value MSM6242B)
      (footprint Package_DIP:DIP-18_W7.62mm_Socket_LongPads)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) RTC))
      (libsource (lib MSM6242B) (part MSM6242B) (description ""))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF6500A))
    (comp (ref R915)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF75B36))
    (comp (ref R914)
      (value 10k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF763B4))
    (comp (ref R916)
      (value 1k)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF7CC89))
    (comp (ref JP9)
      (value Jumper_2_Open)
      (footprint Raemixx500:Jumper2-Open)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper) (part Jumper_2_Open) (description "Jumper, 2-pole, open"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF7DF20))
    (comp (ref TC9)
      (value 6.8-45p)
      (footprint Raemixx500:VariCap)
      (datasheet ~)
      (fields
        (field (name Optional) RTC))
      (libsource (lib Device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF819AD))
    (comp (ref C911)
      (value 22p)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.141)
        (field (name "MFG Name") AVX)
        (field (name "MFG Part Num") SA102A220JARC))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF81C27))
    (comp (ref Y9)
      (value "32768 Hz")
      (footprint Raemixx500:Crystal_RTC)
      (datasheet ~)
      (fields
        (field (name Optional) RTC))
      (libsource (lib Device) (part Crystal_GND2) (description "Three pin crystal, GND on pin 2"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF90547))
    (comp (ref BT9)
      (value CR2032)
      (footprint Raemixx500:Battery_Holder_Coin_2032_BS-7)
      (datasheet ~)
      (fields
        (field (name Optional) RTC))
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF9EAEA))
    (comp (ref C913)
      (value 4.7u)
      (footprint Capacitor_THT:CP_Radial_D8.0mm_P5.00mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.41)
        (field (name "MFG Name") "RS PRO")
        (field (name "MFG Part Num") 181-4685)
        (field (name Optional) RTC))
      (libsource (lib Device) (part CP1) (description "Polarized capacitor, US symbol"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CF9EEAC))
    (comp (ref C9)
      (value 330n)
      (footprint Raemixx500:C_Axial_L6.3mm_D2.5mm_P10.16mm)
      (datasheet ~)
      (fields
        (field (name Cost) 0.078)
        (field (name "MFG Name") KEMET)
        (field (name "MFG Part Num") C412C334M5U5TA)
        (field (name Optional) RTC))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CFA11A8))
    (comp (ref D912)
      (value 1n4148)
      (footprint Diode_THT:D_DO-35_SOD27_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) RTC))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CFAA713))
    (comp (ref D911)
      (value 1n4148)
      (footprint Diode_THT:D_DO-35_SOD27_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) RTC))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CFABB51))
    (comp (ref R911)
      (value 470)
      (footprint Raemixx500:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CFABC9A))
    (comp (ref D913)
      (value 1n4148)
      (footprint Diode_THT:D_DO-35_SOD27_P12.70mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Optional) RTC))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names "/Real-Time Clock/") (tstamps /5CF615AB/))
      (tstamp 5CFBBF2C))
    (comp (ref P9)
      (value TRAPDOOR)
      (footprint Raemixx500:Trapdoor)
      (datasheet DOCUMENTATION)
      (fields
        (field (name Optional) CONN))
      (libsource (lib TRAPDOOR) (part TRAPDOOR) (description ""))
      (sheetpath (names "/Trapdoor Expansion/") (tstamps /5D00C589/))
      (tstamp 5D00E3F8))
    (comp (ref JP7A1)
      (value Jumper_3_Open)
      (footprint Raemixx500:Jumper3-Open)
      (datasheet ~)
      (fields
        (field (name "MFG Name") SKIP)
        (field (name "MFG Part Num") SKIP)
        (field (name Optional) JMP))
      (libsource (lib Jumper_3_Bridged23) (part Jumper_3_Open) (description "Jumper, 3-pole, both open"))
      (sheetpath (names "/Trapdoor Expansion/") (tstamps /5D00C589/))
      (tstamp 5E92560D)))
  (libparts
    (libpart (lib 68000D) (part 68000D)
      (description "16/32-bit Microprocessor")
      (docs https://www.nxp.com/docs/en/reference-manual/MC68000UM.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 68000D))
      (pins
        (pin (num 1) (name D4) (type BiDi))
        (pin (num 2) (name D3) (type BiDi))
        (pin (num 3) (name D2) (type BiDi))
        (pin (num 4) (name D1) (type BiDi))
        (pin (num 5) (name D0) (type BiDi))
        (pin (num 6) (name AS) (type output))
        (pin (num 7) (name UDS) (type output))
        (pin (num 8) (name LDS) (type output))
        (pin (num 9) (name R/W) (type output))
        (pin (num 10) (name DTACK) (type input))
        (pin (num 11) (name BG) (type output))
        (pin (num 12) (name BGACK) (type input))
        (pin (num 13) (name BR) (type input))
        (pin (num 14) (name VCC) (type power_in))
        (pin (num 15) (name CLK) (type input))
        (pin (num 16) (name GND) (type power_in))
        (pin (num 17) (name HALT) (type BiDi))
        (pin (num 18) (name RESET) (type BiDi))
        (pin (num 19) (name VMA) (type output))
        (pin (num 20) (name E) (type output))
        (pin (num 21) (name VPA) (type input))
        (pin (num 22) (name BERR) (type input))
        (pin (num 23) (name IPL2) (type input))
        (pin (num 24) (name IPL1) (type input))
        (pin (num 25) (name IPL0) (type input))
        (pin (num 26) (name FC2) (type output))
        (pin (num 27) (name FC1) (type output))
        (pin (num 28) (name FC0) (type output))
        (pin (num 29) (name A1) (type output))
        (pin (num 30) (name A2) (type output))
        (pin (num 31) (name A3) (type output))
        (pin (num 32) (name A4) (type output))
        (pin (num 33) (name A5) (type output))
        (pin (num 34) (name A6) (type output))
        (pin (num 35) (name A7) (type output))
        (pin (num 36) (name A8) (type output))
        (pin (num 37) (name A9) (type output))
        (pin (num 38) (name A10) (type output))
        (pin (num 39) (name A11) (type output))
        (pin (num 40) (name A12) (type output))
        (pin (num 41) (name A13) (type output))
        (pin (num 42) (name A14) (type output))
        (pin (num 43) (name A15) (type output))
        (pin (num 44) (name A16) (type output))
        (pin (num 45) (name A17) (type output))
        (pin (num 46) (name A18) (type output))
        (pin (num 47) (name A19) (type output))
        (pin (num 48) (name A20) (type output))
        (pin (num 49) (name VCC) (type power_in))
        (pin (num 50) (name A21) (type output))
        (pin (num 51) (name A22) (type output))
        (pin (num 52) (name A23) (type output))
        (pin (num 53) (name GND) (type power_in))
        (pin (num 54) (name D15) (type BiDi))
        (pin (num 55) (name D14) (type BiDi))
        (pin (num 56) (name D13) (type BiDi))
        (pin (num 57) (name D12) (type BiDi))
        (pin (num 58) (name D11) (type BiDi))
        (pin (num 59) (name D10) (type BiDi))
        (pin (num 60) (name D9) (type BiDi))
        (pin (num 61) (name D8) (type BiDi))
        (pin (num 62) (name D7) (type BiDi))
        (pin (num 63) (name D6) (type BiDi))
        (pin (num 64) (name D5) (type BiDi))))
    (libpart (lib 74ls157) (part 74LS157)
      (description "Quad 2 to 1 line Multiplexer")
      (docs http://www.ti.com/lit/gpn/sn74LS157)
      (footprints
        (fp DIP?16*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS157))
      (pins
        (pin (num 1) (name S) (type input))
        (pin (num 2) (name I0a) (type input))
        (pin (num 3) (name I1a) (type input))
        (pin (num 4) (name Za) (type output))
        (pin (num 5) (name I0b) (type input))
        (pin (num 6) (name I1b) (type input))
        (pin (num 7) (name Zb) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name Zd) (type output))
        (pin (num 10) (name I1d) (type input))
        (pin (num 11) (name I0d) (type input))
        (pin (num 12) (name Zc) (type output))
        (pin (num 13) (name I1c) (type input))
        (pin (num 14) (name I0c) (type input))
        (pin (num 15) (name E) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib 74ls244) (part 74LS244)
      (description "8-bit Bus Buffer 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS244)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS244))
      (pins
        (pin (num 1) (name OEa) (type input))
        (pin (num 2) (name I0a) (type input))
        (pin (num 3) (name O3b) (type 3state))
        (pin (num 4) (name I1a) (type input))
        (pin (num 5) (name O2b) (type 3state))
        (pin (num 6) (name I2a) (type input))
        (pin (num 7) (name O1b) (type 3state))
        (pin (num 8) (name I3a) (type input))
        (pin (num 9) (name O0b) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name I0b) (type input))
        (pin (num 12) (name O3a) (type 3state))
        (pin (num 13) (name I1b) (type input))
        (pin (num 14) (name O2a) (type 3state))
        (pin (num 15) (name I2b) (type input))
        (pin (num 16) (name O1a) (type 3state))
        (pin (num 17) (name I3b) (type input))
        (pin (num 18) (name O0a) (type 3state))
        (pin (num 19) (name OEb) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 74ls245) (part 74LS245)
      (description "Octal BUS Transceivers, 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS245)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 74ls258) (part 74LS258)
      (description "Quad 2 to 1 Multiplexer, inverting")
      (docs http://www.ti.com/lit/gpn/sn74LS258)
      (footprints
        (fp DIP?16*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS258))
      (pins
        (pin (num 1) (name S) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type 3state))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type input))
        (pin (num 7) (name ~) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ~) (type 3state))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type 3state))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name ~) (type input))
        (pin (num 15) (name OE) (type input))
        (pin (num 16) (name VCC) (type input))))
    (libpart (lib 74ls373) (part 74LS373)
      (description "8-bit Latch, 3-state outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS373)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS373))
      (pins
        (pin (num 1) (name OE) (type input))
        (pin (num 2) (name O0) (type 3state))
        (pin (num 3) (name D0) (type input))
        (pin (num 4) (name D1) (type input))
        (pin (num 5) (name O1) (type 3state))
        (pin (num 6) (name O2) (type 3state))
        (pin (num 7) (name D2) (type input))
        (pin (num 8) (name D3) (type input))
        (pin (num 9) (name O3) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name LE) (type input))
        (pin (num 12) (name O4) (type 3state))
        (pin (num 13) (name D4) (type input))
        (pin (num 14) (name D5) (type input))
        (pin (num 15) (name O5) (type 3state))
        (pin (num 16) (name O6) (type 3state))
        (pin (num 17) (name D6) (type input))
        (pin (num 18) (name D7) (type input))
        (pin (num 19) (name O7) (type 3state))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS05)
      (aliases
        (alias 74LS06)
        (alias 74LS06N))
      (description "Inverter Open Collect")
      (docs http://www.ti.com/lit/gpn/sn74LS05)
      (footprints
        (fp DIP*W7.62mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS05))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type openCol))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type openCol))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type openCol))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type openCol))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type openCol))
        (pin (num 11) (name ~) (type input))
        (pin (num 12) (name ~) (type openCol))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS139)
      (description "Dual Decoder 1 of 4, Active low outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS139)
      (footprints
        (fp DIP?16*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS139))
      (pins
        (pin (num 1) (name E) (type input))
        (pin (num 2) (name A0) (type input))
        (pin (num 3) (name A1) (type input))
        (pin (num 4) (name O0) (type output))
        (pin (num 5) (name O1) (type output))
        (pin (num 6) (name O2) (type output))
        (pin (num 7) (name O3) (type output))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name O3) (type output))
        (pin (num 10) (name O2) (type output))
        (pin (num 11) (name O1) (type output))
        (pin (num 12) (name O0) (type output))
        (pin (num 13) (name A1) (type input))
        (pin (num 14) (name A0) (type input))
        (pin (num 15) (name E) (type input))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS32)
      (description "Quad 2-input OR")
      (docs http://www.ti.com/lit/gpn/sn74LS32)
      (footprints
        (fp DIP?14*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS32))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type output))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib AMIGA_ROM) (part AMIGA_ROM)
      (fields
        (field (name Reference) U)
        (field (name Value) AMIGA_ROM)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name A18) (type input))
        (pin (num 2) (name A17) (type input))
        (pin (num 3) (name A7) (type input))
        (pin (num 4) (name A6) (type input))
        (pin (num 5) (name A5) (type input))
        (pin (num 6) (name A4) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A1) (type input))
        (pin (num 10) (name A0) (type input))
        (pin (num 11) (name ~CS) (type input))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name ~OE) (type input))
        (pin (num 14) (name D0) (type 3state))
        (pin (num 15) (name D8) (type 3state))
        (pin (num 16) (name D1) (type 3state))
        (pin (num 17) (name D9) (type 3state))
        (pin (num 18) (name D2) (type 3state))
        (pin (num 19) (name D10) (type 3state))
        (pin (num 20) (name D3) (type 3state))
        (pin (num 21) (name D11) (type 3state))
        (pin (num 22) (name VCC) (type power_in))
        (pin (num 23) (name D4) (type 3state))
        (pin (num 24) (name D12) (type 3state))
        (pin (num 25) (name D5) (type 3state))
        (pin (num 26) (name D13) (type 3state))
        (pin (num 27) (name D6) (type 3state))
        (pin (num 28) (name D14) (type 3state))
        (pin (num 29) (name D7) (type 3state))
        (pin (num 30) (name D15) (type 3state))
        (pin (num 31) (name GND) (type power_in))
        (pin (num 32) (name ~BYTE) (type input))
        (pin (num 33) (name A16) (type input))
        (pin (num 34) (name A15) (type input))
        (pin (num 35) (name A14) (type input))
        (pin (num 36) (name A13) (type input))
        (pin (num 37) (name A12) (type input))
        (pin (num 38) (name A11) (type input))
        (pin (num 39) (name A10) (type input))
        (pin (num 40) (name A9) (type input))
        (pin (num 41) (name A8) (type input))
        (pin (num 42) (name A19) (type input))))
    (libpart (lib Amplifier_Operational) (part LM2902)
      (aliases
        (alias LM324)
        (alias TLC274)
        (alias TLC279)
        (alias TL074)
        (alias LM324A)
        (alias MCP6004)
        (alias TL084)
        (alias TL064)
        (alias LMV324)
        (alias LMC6484)
        (alias MCP604)
        (alias MC33079)
        (alias MC33174)
        (alias MC33179)
        (alias OPA1604)
        (alias OPA1679)
        (alias OPA4134)
        (alias OPA4340UA)
        (alias OPA4376)
        (alias MCP6L94)
        (alias TSV914)
        (alias ADA4807-4)
        (alias TSV994))
      (description "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14")
      (docs http://www.ti.com/lit/ds/symlink/lm2902-n.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*4.4x5mm*P0.65mm*)
        (fp SSOP*5.3x6.2mm*P0.65mm*)
        (fp MSOP*3x3mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2902))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib BUSEXP) (part BUSEXP)
      (fields
        (field (name Reference) U)
        (field (name Value) BUSEXP)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name VCC) (type power_in))
        (pin (num 7) (name 7MHZ) (type input))
        (pin (num 8) (name -12V) (type power_in))
        (pin (num 9) (name NC) (type NotConnected))
        (pin (num 10) (name +12V) (type power_in))
        (pin (num 11) (name NC) (type NotConnected))
        (pin (num 12) (name ~CONFIG) (type input))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name ~CCKQ) (type input))
        (pin (num 15) (name ~CDAC) (type input))
        (pin (num 16) (name ~CCK) (type input))
        (pin (num 17) (name ~OVR) (type output))
        (pin (num 18) (name XRDY) (type output))
        (pin (num 19) (name ~INT2) (type openCol))
        (pin (num 20) (name NC) (type NotConnected))
        (pin (num 21) (name A5) (type input))
        (pin (num 22) (name ~INT6) (type openCol))
        (pin (num 23) (name A6) (type input))
        (pin (num 24) (name A4) (type input))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name A3) (type input))
        (pin (num 27) (name A2) (type input))
        (pin (num 28) (name A7) (type input))
        (pin (num 29) (name A1) (type input))
        (pin (num 30) (name A8) (type input))
        (pin (num 31) (name FC0) (type input))
        (pin (num 32) (name A9) (type input))
        (pin (num 33) (name FC1) (type input))
        (pin (num 34) (name A10) (type input))
        (pin (num 35) (name FC2) (type input))
        (pin (num 36) (name A11) (type input))
        (pin (num 37) (name GND) (type power_in))
        (pin (num 38) (name A12) (type input))
        (pin (num 39) (name A13) (type input))
        (pin (num 40) (name ~IPL0) (type input))
        (pin (num 41) (name A14) (type input))
        (pin (num 42) (name ~IPL1) (type input))
        (pin (num 43) (name A15) (type input))
        (pin (num 44) (name ~IPL2) (type input))
        (pin (num 45) (name A16) (type input))
        (pin (num 46) (name ~BERR) (type BiDi))
        (pin (num 47) (name A17) (type input))
        (pin (num 48) (name ~VPA) (type output))
        (pin (num 49) (name GND) (type power_in))
        (pin (num 50) (name E) (type input))
        (pin (num 51) (name ~VMA) (type input))
        (pin (num 52) (name A18) (type input))
        (pin (num 53) (name ~RESET) (type BiDi))
        (pin (num 54) (name A19) (type input))
        (pin (num 55) (name ~HALT) (type BiDi))
        (pin (num 56) (name A20) (type input))
        (pin (num 57) (name A22) (type input))
        (pin (num 58) (name A21) (type input))
        (pin (num 59) (name A23) (type input))
        (pin (num 60) (name ~BR) (type output))
        (pin (num 61) (name GND) (type power_in))
        (pin (num 62) (name ~BGACK) (type output))
        (pin (num 63) (name D15) (type BiDi))
        (pin (num 64) (name ~BG) (type input))
        (pin (num 65) (name D14) (type BiDi))
        (pin (num 66) (name ~DTACK) (type input))
        (pin (num 67) (name D13) (type BiDi))
        (pin (num 68) (name R~W) (type input))
        (pin (num 69) (name D12) (type BiDi))
        (pin (num 70) (name ~LDS) (type input))
        (pin (num 71) (name D11) (type BiDi))
        (pin (num 72) (name ~UDS) (type input))
        (pin (num 73) (name GND) (type power_in))
        (pin (num 74) (name ~AS) (type input))
        (pin (num 75) (name D0) (type BiDi))
        (pin (num 76) (name D10) (type BiDi))
        (pin (num 77) (name D1) (type BiDi))
        (pin (num 78) (name D9) (type BiDi))
        (pin (num 79) (name D2) (type BiDi))
        (pin (num 80) (name D8) (type BiDi))
        (pin (num 81) (name D3) (type BiDi))
        (pin (num 82) (name D7) (type BiDi))
        (pin (num 83) (name D4) (type BiDi))
        (pin (num 84) (name D6) (type BiDi))
        (pin (num 85) (name GND) (type input))
        (pin (num 86) (name D5) (type BiDi))))
    (libpart (lib Connector_Generic) (part Conn_02x03_Odd_Even)
      (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x03_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x17_Odd_Even)
      (description "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x17_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))))
    (libpart (lib DENISE) (part DENISE)
      (fields
        (field (name Reference) U)
        (field (name Value) DENISE)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name DRD6) (type input))
        (pin (num 2) (name DRD5) (type input))
        (pin (num 3) (name DRD4) (type input))
        (pin (num 4) (name DRD3) (type input))
        (pin (num 5) (name DRD2) (type input))
        (pin (num 6) (name DRD1) (type input))
        (pin (num 7) (name DRD0) (type input))
        (pin (num 8) (name M1H) (type input))
        (pin (num 9) (name M0H) (type input))
        (pin (num 10) (name RGA8) (type input))
        (pin (num 11) (name RGA7) (type input))
        (pin (num 12) (name RGA6) (type input))
        (pin (num 13) (name RGA5) (type input))
        (pin (num 14) (name RGA4) (type input))
        (pin (num 15) (name RGA3) (type input))
        (pin (num 16) (name RGA2) (type input))
        (pin (num 17) (name RGA1) (type input))
        (pin (num 18) (name BURST) (type output))
        (pin (num 19) (name VCC) (type power_in))
        (pin (num 20) (name R0) (type output))
        (pin (num 21) (name R1) (type output))
        (pin (num 22) (name R2) (type output))
        (pin (num 23) (name R3) (type output))
        (pin (num 24) (name B0) (type output))
        (pin (num 25) (name B1) (type output))
        (pin (num 26) (name B2) (type output))
        (pin (num 27) (name B3) (type output))
        (pin (num 28) (name G0) (type output))
        (pin (num 29) (name G1) (type output))
        (pin (num 30) (name G2) (type output))
        (pin (num 31) (name G3) (type output))
        (pin (num 32) (name BLANK) (type input))
        (pin (num 33) (name PIXELSW) (type output))
        (pin (num 34) (name ~CDAC) (type input))
        (pin (num 35) (name 7M) (type input))
        (pin (num 36) (name CCK) (type input))
        (pin (num 37) (name GND) (type power_in))
        (pin (num 38) (name M0V) (type input))
        (pin (num 39) (name M1V) (type input))
        (pin (num 40) (name DRD15) (type input))
        (pin (num 41) (name DRD14) (type input))
        (pin (num 42) (name DRD13) (type input))
        (pin (num 43) (name DRD12) (type input))
        (pin (num 44) (name DRD11) (type input))
        (pin (num 45) (name DRD10) (type input))
        (pin (num 46) (name DRD9) (type input))
        (pin (num 47) (name DRD8) (type input))
        (pin (num 48) (name DRD7) (type input))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP1)
      (description "Polarized capacitor, US symbol")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Variable)
      (description "Variable capacitor")
      (docs ~)
      (fields
        (field (name Reference) C)
        (field (name Value) C_Variable))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_GND2)
      (description "Three pin crystal, GND on pin 2")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part D)
      (description Diode)
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part EMI_Filter_LCL)
      (description "EMI T-filter (LCL)")
      (docs http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (footprints
        (fp Filter*)
        (fp Resonator*))
      (fields
        (field (name Reference) FL)
        (field (name Value) EMI_Filter_LCL))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead_Small)
      (description "Ferrite bead, small symbol")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Q_NJFET_DSG)
      (description "N-JFET transistor, drain/source/gate")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NJFET_DSG))
      (pins
        (pin (num 1) (name D) (type passive))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name G) (type input))))
    (libpart (lib Device) (part Q_PNP_EBC)
      (description "PNP transistor, emitter/base/collector")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PNP_EBC))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Network09)
      (description "9 resistor network, star topology, bussed resistors, small symbol")
      (docs http://www.vishay.com/docs/31509/csc.pdf)
      (footprints
        (fp R?Array?SIP*))
      (fields
        (field (name Reference) RN)
        (field (name Value) R_Network09)
        (field (name Footprint) Resistor_THT:R_Array_SIP10))
      (pins
        (pin (num 1) (name common) (type passive))
        (pin (num 2) (name R1) (type passive))
        (pin (num 3) (name R2) (type passive))
        (pin (num 4) (name R3) (type passive))
        (pin (num 5) (name R4) (type passive))
        (pin (num 6) (name R5) (type passive))
        (pin (num 7) (name R6) (type passive))
        (pin (num 8) (name R7) (type passive))
        (pin (num 9) (name R8) (type passive))
        (pin (num 10) (name R9) (type passive))))
    (libpart (lib Device) (part R_Pack05_SIP)
      (description "5 resistor network, parallel topology, SIP package")
      (docs http://www.vishay.com/docs/31509/csc.pdf)
      (footprints
        (fp R?Array?SIP*))
      (fields
        (field (name Reference) RN)
        (field (name Value) R_Pack05_SIP)
        (field (name Footprint) Resistor_THT:R_Array_SIP10))
      (pins
        (pin (num 1) (name R1.1) (type passive))
        (pin (num 2) (name R1.2) (type passive))
        (pin (num 3) (name R2.1) (type passive))
        (pin (num 4) (name R2.2) (type passive))
        (pin (num 5) (name R3.1) (type passive))
        (pin (num 6) (name R3.2) (type passive))
        (pin (num 7) (name R4.1) (type passive))
        (pin (num 8) (name R4.2) (type passive))
        (pin (num 9) (name R5.1) (type passive))
        (pin (num 10) (name R5.2) (type passive))))
    (libpart (lib Diode) (part 1N4148)
      (aliases
        (alias 1N4448)
        (alias 1N4149)
        (alias 1N4151)
        (alias 1N914)
        (alias BA243)
        (alias BA244)
        (alias BA282)
        (alias BA283)
        (alias BAV17)
        (alias BAV18)
        (alias BAV19)
        (alias BAV20)
        (alias BAV21)
        (alias BAW75)
        (alias BAW76)
        (alias BAY93))
      (description "100V 0.15A standard switching diode, DO-35")
      (docs https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf)
      (footprints
        (fp D*DO?35*))
      (fields
        (field (name Reference) D)
        (field (name Value) 1N4148)
        (field (name Footprint) Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Dispatcher) (part Dispatcher_3to1)
      (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Dispatcher_3to1))
      (pins
        (pin (num 1) (name In_1) (type passive))
        (pin (num 2) (name In_2) (type passive))
        (pin (num 3) (name In_3) (type passive))
        (pin (num 4) (name Out) (type passive))))
    (libpart (lib FAT_AGNUS_8375) (part FAT_AGNUS_8375)
      (fields
        (field (name Reference) U)
        (field (name Value) FAT_AGNUS_8375)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name DRD13) (type BiDi))
        (pin (num 2) (name DRD12) (type BiDi))
        (pin (num 3) (name DRD11) (type BiDi))
        (pin (num 4) (name DRD10) (type BiDi))
        (pin (num 5) (name DRD9) (type BiDi))
        (pin (num 6) (name DRD8) (type BiDi))
        (pin (num 7) (name DRD7) (type BiDi))
        (pin (num 8) (name DRD6) (type BiDi))
        (pin (num 9) (name DRD5) (type BiDi))
        (pin (num 10) (name DRD4) (type BiDi))
        (pin (num 11) (name DRD3) (type BiDi))
        (pin (num 12) (name DRD2) (type BiDi))
        (pin (num 13) (name DRD1) (type BiDi))
        (pin (num 14) (name DRD0) (type BiDi))
        (pin (num 15) (name VCC) (type power_in))
        (pin (num 16) (name ~RESET) (type input))
        (pin (num 17) (name ~INTR) (type output))
        (pin (num 18) (name DMAL) (type input))
        (pin (num 19) (name ~BLISS) (type input))
        (pin (num 20) (name ~BLIT) (type output))
        (pin (num 21) (name ~WE) (type output))
        (pin (num 22) (name R/~W) (type input))
        (pin (num 23) (name ~REGEN) (type input))
        (pin (num 24) (name ~AS) (type input))
        (pin (num 25) (name ~RAMEN) (type input))
        (pin (num 26) (name RGA8) (type output))
        (pin (num 27) (name RGA7) (type output))
        (pin (num 28) (name RGA6) (type output))
        (pin (num 29) (name RGA5) (type output))
        (pin (num 30) (name RGA4) (type output))
        (pin (num 31) (name RGA3) (type output))
        (pin (num 32) (name RGA2) (type output))
        (pin (num 33) (name RGA1) (type output))
        (pin (num 34) (name 28MHZ) (type input))
        (pin (num 35) (name A20) (type input))
        (pin (num 36) (name ~CDAC) (type output))
        (pin (num 37) (name 7MHZ) (type input))
        (pin (num 38) (name CCKQ) (type output))
        (pin (num 39) (name CCK) (type output))
        (pin (num 40) (name 14MHZ) (type input))
        (pin (num 41) (name GND) (type power_in))
        (pin (num 42) (name DRA0) (type output))
        (pin (num 43) (name DRA1) (type output))
        (pin (num 44) (name DRA2) (type output))
        (pin (num 45) (name DRA3) (type output))
        (pin (num 46) (name DRA4) (type output))
        (pin (num 47) (name DRA5) (type output))
        (pin (num 48) (name DRA6) (type output))
        (pin (num 49) (name DRA7) (type output))
        (pin (num 50) (name DRA8) (type output))
        (pin (num 51) (name ~LDS) (type input))
        (pin (num 52) (name ~UDS) (type input))
        (pin (num 53) (name ~CASL) (type output))
        (pin (num 54) (name ~CASU) (type output))
        (pin (num 55) (name DRA9) (type output))
        (pin (num 56) (name ~RAS1) (type output))
        (pin (num 57) (name ~RAS0) (type output))
        (pin (num 58) (name GND) (type power_in))
        (pin (num 59) (name A19) (type input))
        (pin (num 60) (name A1) (type input))
        (pin (num 61) (name A2) (type input))
        (pin (num 62) (name A3) (type input))
        (pin (num 63) (name A4) (type input))
        (pin (num 64) (name A5) (type input))
        (pin (num 65) (name A6) (type input))
        (pin (num 66) (name A7) (type input))
        (pin (num 67) (name A8) (type input))
        (pin (num 68) (name A9) (type input))
        (pin (num 69) (name A10) (type input))
        (pin (num 70) (name A11) (type input))
        (pin (num 71) (name A12) (type input))
        (pin (num 72) (name A13) (type input))
        (pin (num 73) (name A14) (type input))
        (pin (num 74) (name A15) (type input))
        (pin (num 75) (name A16) (type input))
        (pin (num 76) (name A17) (type input))
        (pin (num 77) (name A18) (type input))
        (pin (num 78) (name ~LPEN) (type passive))
        (pin (num 79) (name ~VSYNC) (type input))
        (pin (num 80) (name ~CSYNC) (type input))
        (pin (num 81) (name ~HSYNC) (type input))
        (pin (num 82) (name GND) (type power_in))
        (pin (num 83) (name DRD15) (type BiDi))
        (pin (num 84) (name DRD14) (type BiDi))))
    (libpart (lib GARY) (part GARY_5719)
      (fields
        (field (name Reference) U)
        (field (name Value) GARY_5719)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name ~VPA) (type input))
        (pin (num 3) (name ~OEL) (type output))
        (pin (num 4) (name ~OEB) (type output))
        (pin (num 5) (name ~KBRESET) (type input))
        (pin (num 6) (name VCC) (type power_in))
        (pin (num 7) (name ~MTR) (type input))
        (pin (num 8) (name DKWE) (type input))
        (pin (num 9) (name ~DKWD) (type input))
        (pin (num 10) (name ~LDS) (type input))
        (pin (num 11) (name ~UDS) (type input))
        (pin (num 12) (name R/~W) (type input))
        (pin (num 13) (name ~AS) (type input))
        (pin (num 14) (name ~BGACK) (type input))
        (pin (num 15) (name ~BLIT) (type input))
        (pin (num 16) (name ~SEL) (type input))
        (pin (num 17) (name VCC) (type power_in))
        (pin (num 18) (name ~REGEN) (type output))
        (pin (num 19) (name ~BLISS) (type output))
        (pin (num 20) (name ~RAMEN) (type output))
        (pin (num 21) (name ~ROMEN) (type output))
        (pin (num 22) (name ~CLKRD) (type output))
        (pin (num 23) (name ~CLKWR) (type output))
        (pin (num 24) (name GND) (type power_in))
        (pin (num 25) (name ~LATCH) (type output))
        (pin (num 26) (name ~CDAC) (type input))
        (pin (num 27) (name CCKQ) (type input))
        (pin (num 28) (name CCK) (type input))
        (pin (num 29) (name ~OVR) (type input))
        (pin (num 30) (name OVL) (type input))
        (pin (num 31) (name XRDY) (type input))
        (pin (num 32) (name ~EXRAM) (type input))
        (pin (num 33) (name A17) (type input))
        (pin (num 34) (name A18) (type input))
        (pin (num 35) (name A19) (type input))
        (pin (num 36) (name A20) (type input))
        (pin (num 37) (name A21) (type input))
        (pin (num 38) (name A22) (type input))
        (pin (num 39) (name A23) (type input))
        (pin (num 40) (name GND) (type power_in))
        (pin (num 41) (name ~RST) (type input))
        (pin (num 42) (name ~HLT) (type input))
        (pin (num 43) (name ~DTACK) (type input))
        (pin (num 44) (name DKWEB) (type output))
        (pin (num 45) (name DKWDB) (type output))
        (pin (num 46) (name MTRON) (type output))
        (pin (num 47) (name MTRX) (type output))
        (pin (num 48) (name VCC) (type power_in))))
    (libpart (lib Jumper) (part Jumper_2_Bridged)
      (description "Jumper, 2-pole, closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_2_Bridged))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part Jumper_2_Open)
      (description "Jumper, 2-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_2_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part Jumper_3_Bridged12)
      (description "Jumper, 3-pole, pins 1+2 closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged12*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_3_Bridged12))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib Jumper) (part Jumper_3_Open)
      (description "Jumper, 3-pole, both open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_3_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib Jumper_3_Bridged23) (part Jumper_3_Bridged23)
      (description "Jumper, 3-pole, pins 1+2 closed/bridged")
      (docs ~)
      (footprints
        (fp Jumper*Bridged12*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_3_Bridged23))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib Jumper_3_Bridged23) (part Jumper_3_Open)
      (description "Jumper, 3-pole, both open")
      (docs ~)
      (footprints
        (fp Jumper*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_3_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib MC1488) (part MC1488)
      (description "Quad Line EIA-232D Driver")
      (docs https://www.onsemi.com/pub/Collateral/MC1488-D.PDF)
      (fields
        (field (name Reference) U)
        (field (name Value) MC1488)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name VEE) (type power_in))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type output))
        (pin (num 4) (name IN1_B) (type input))
        (pin (num 5) (name IN2_B) (type input))
        (pin (num 6) (name OUT_B) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT_C) (type output))
        (pin (num 9) (name IN2_C) (type input))
        (pin (num 10) (name IN1_C) (type input))
        (pin (num 11) (name OUT_D) (type output))
        (pin (num 12) (name IN2_D) (type input))
        (pin (num 13) (name IN1_D) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib MSM6242B) (part MSM6242B)
      (fields
        (field (name Reference) U)
        (field (name Value) MSM6242B)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name STD.P) (type input))
        (pin (num 2) (name ~CS0) (type input))
        (pin (num 3) (name ALE) (type input))
        (pin (num 4) (name A0) (type input))
        (pin (num 5) (name A1) (type input))
        (pin (num 6) (name A2) (type input))
        (pin (num 7) (name A3) (type input))
        (pin (num 8) (name ~RD) (type input))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name ~WR) (type input))
        (pin (num 11) (name D3) (type BiDi))
        (pin (num 12) (name D2) (type BiDi))
        (pin (num 13) (name D1) (type BiDi))
        (pin (num 14) (name D0) (type BiDi))
        (pin (num 15) (name CS1) (type input))
        (pin (num 16) (name XT) (type input))
        (pin (num 17) (name ~XT) (type input))
        (pin (num 18) (name VCC) (type power_in))))
    (libpart (lib Mechanical) (part MountingHole_Pad)
      (description "Mounting Hole with connection")
      (docs ~)
      (footprints
        (fp MountingHole*Pad*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole_Pad))
      (pins
        (pin (num 1) (name 1) (type input))))
    (libpart (lib PAULA) (part PAULA)
      (fields
        (field (name Reference) U)
        (field (name Value) PAULA)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name DRD8) (type BiDi))
        (pin (num 2) (name DRD7) (type BiDi))
        (pin (num 3) (name DRD6) (type BiDi))
        (pin (num 4) (name DRD5) (type BiDi))
        (pin (num 5) (name DRD4) (type BiDi))
        (pin (num 6) (name DRD3) (type BiDi))
        (pin (num 7) (name DRD2) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name DRD1) (type BiDi))
        (pin (num 10) (name DRD0) (type BiDi))
        (pin (num 11) (name ~RESET) (type input))
        (pin (num 12) (name DMAL) (type output))
        (pin (num 13) (name ~IPL0) (type output))
        (pin (num 14) (name ~IPL1) (type output))
        (pin (num 15) (name ~IPL2) (type output))
        (pin (num 16) (name ~INT2) (type openCol))
        (pin (num 17) (name ~INT3) (type input))
        (pin (num 18) (name ~INT6) (type openCol))
        (pin (num 19) (name RGA8) (type input))
        (pin (num 20) (name RGA7) (type input))
        (pin (num 21) (name RGA6) (type input))
        (pin (num 22) (name RGA5) (type input))
        (pin (num 23) (name RGA4) (type input))
        (pin (num 24) (name RGA3) (type input))
        (pin (num 25) (name RGA2) (type input))
        (pin (num 26) (name RGA1) (type input))
        (pin (num 27) (name VCC) (type power_in))
        (pin (num 28) (name CCK) (type input))
        (pin (num 29) (name CCKQ) (type input))
        (pin (num 30) (name RIGHT) (type output))
        (pin (num 31) (name LEFT) (type output))
        (pin (num 32) (name P0X) (type input))
        (pin (num 33) (name P0Y) (type input))
        (pin (num 34) (name AGND) (type passive))
        (pin (num 35) (name P1X) (type input))
        (pin (num 36) (name P1Y) (type input))
        (pin (num 37) (name ~DKRD) (type input))
        (pin (num 38) (name ~DKWD) (type output))
        (pin (num 39) (name DKWE) (type output))
        (pin (num 40) (name ~TXD) (type output))
        (pin (num 41) (name ~RXD) (type input))
        (pin (num 42) (name DRD15) (type BiDi))
        (pin (num 43) (name DRD14) (type BiDi))
        (pin (num 44) (name DRD13) (type BiDi))
        (pin (num 45) (name DRD12) (type BiDi))
        (pin (num 46) (name DRD11) (type BiDi))
        (pin (num 47) (name DRD10) (type BiDi))
        (pin (num 48) (name DRD9) (type BiDi))))
    (libpart (lib PJRAN1X1U01X) (part PJRAN1X1U01X)
      (fields
        (field (name Reference) J)
        (field (name Value) PJRAN1X1U01X)
        (field (name Footprint) SWITCHCRAFT_PJRAN1X1U01X)
        (field (name Datasheet) A)
        (field (name Field4) Switchcraft)
        (field (name Field5) 13mm)
        (field (name Field6) "Manufacturer Recommendations"))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib TRAPDOOR) (part TRAPDOOR)
      (fields
        (field (name Reference) U)
        (field (name Value) TRAPDOOR)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name PIN1) (type input))
        (pin (num 2) (name PIN2) (type input))
        (pin (num 3) (name PIN3) (type input))
        (pin (num 4) (name PIN4) (type input))
        (pin (num 5) (name PIN5) (type input))
        (pin (num 6) (name PIN6) (type input))
        (pin (num 7) (name PIN7) (type input))
        (pin (num 8) (name PIN8) (type input))
        (pin (num 9) (name PIN9) (type input))
        (pin (num 10) (name PIN10) (type input))
        (pin (num 11) (name PIN11) (type input))
        (pin (num 12) (name PIN12) (type input))
        (pin (num 13) (name PIN13) (type input))
        (pin (num 14) (name PIN14) (type input))
        (pin (num 15) (name PIN15) (type input))
        (pin (num 16) (name PIN16) (type input))
        (pin (num 17) (name PIN17) (type input))
        (pin (num 18) (name PIN18) (type input))
        (pin (num 19) (name PIN19) (type input))
        (pin (num 20) (name PIN20) (type input))
        (pin (num 21) (name PIN21) (type input))
        (pin (num 22) (name PIN22) (type input))
        (pin (num 23) (name PIN23) (type input))
        (pin (num 24) (name PIN24) (type input))
        (pin (num 25) (name PIN25) (type input))
        (pin (num 26) (name PIN26) (type input))
        (pin (num 27) (name PIN27) (type input))
        (pin (num 28) (name PIN28) (type input))
        (pin (num 29) (name PIN29) (type input))
        (pin (num 30) (name PIN30) (type input))
        (pin (num 31) (name PIN31) (type input))
        (pin (num 32) (name PIN32) (type input))
        (pin (num 33) (name PIN33) (type input))
        (pin (num 34) (name PIN34) (type input))
        (pin (num 35) (name PIN35) (type input))
        (pin (num 36) (name PIN36) (type input))
        (pin (num 37) (name PIN37) (type input))
        (pin (num 38) (name PIN38) (type input))
        (pin (num 39) (name PIN39) (type input))
        (pin (num 40) (name PIN40) (type input))
        (pin (num 41) (name PIN41) (type input))
        (pin (num 42) (name PIN42) (type input))
        (pin (num 43) (name PIN43) (type input))
        (pin (num 44) (name PIN44) (type input))
        (pin (num 45) (name PIN45) (type input))
        (pin (num 46) (name PIN46) (type input))
        (pin (num 47) (name PIN47) (type input))
        (pin (num 48) (name PIN48) (type input))
        (pin (num 49) (name PIN49) (type input))
        (pin (num 50) (name PIN50) (type input))
        (pin (num 51) (name PIN51) (type input))
        (pin (num 52) (name PIN52) (type input))
        (pin (num 53) (name PIN53) (type input))
        (pin (num 54) (name PIN54) (type input))
        (pin (num 55) (name PIN55) (type input))
        (pin (num 56) (name PIN56) (type input))))
    (libpart (lib Transistor_BJT) (part 2N3904)
      (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3904.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3904)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Transistor_BJT) (part 2N3906)
      (aliases
        (alias 2N3905))
      (description "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92")
      (docs https://www.fairchildsemi.com/datasheets/2N/2N3906.pdf)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3906)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib VIA_8520) (part VIA_8520)
      (fields
        (field (name Reference) U)
        (field (name Value) VIA_8520)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name PA0) (type BiDi))
        (pin (num 3) (name PA1) (type BiDi))
        (pin (num 4) (name PA2) (type BiDi))
        (pin (num 5) (name PA3) (type BiDi))
        (pin (num 6) (name PA4) (type BiDi))
        (pin (num 7) (name PA5) (type BiDi))
        (pin (num 8) (name PA6) (type BiDi))
        (pin (num 9) (name PA7) (type BiDi))
        (pin (num 10) (name PB0) (type BiDi))
        (pin (num 11) (name PB1) (type BiDi))
        (pin (num 12) (name PB2) (type BiDi))
        (pin (num 13) (name PB3) (type BiDi))
        (pin (num 14) (name PB4) (type BiDi))
        (pin (num 15) (name PB5) (type BiDi))
        (pin (num 16) (name PB6) (type BiDi))
        (pin (num 17) (name PB7) (type BiDi))
        (pin (num 18) (name ~PC) (type input))
        (pin (num 19) (name TICK) (type input))
        (pin (num 20) (name VCC) (type power_in))
        (pin (num 21) (name ~INT) (type openCol))
        (pin (num 22) (name ~W) (type input))
        (pin (num 23) (name ~CS) (type input))
        (pin (num 24) (name ~F) (type input))
        (pin (num 25) (name E) (type input))
        (pin (num 26) (name D7) (type BiDi))
        (pin (num 27) (name D6) (type BiDi))
        (pin (num 28) (name D5) (type BiDi))
        (pin (num 29) (name D4) (type BiDi))
        (pin (num 30) (name D3) (type BiDi))
        (pin (num 31) (name D2) (type BiDi))
        (pin (num 32) (name D1) (type BiDi))
        (pin (num 33) (name D0) (type BiDi))
        (pin (num 34) (name ~RESET) (type input))
        (pin (num 35) (name RS3) (type input))
        (pin (num 36) (name RS2) (type input))
        (pin (num 37) (name RS1) (type input))
        (pin (num 38) (name RS0) (type input))
        (pin (num 39) (name S) (type input))
        (pin (num 40) (name C) (type input))))
    (libpart (lib VIDIOT) (part VIDIOT)
      (description "Video DAC")
      (docs https://github.com/SukkoPera/OpenAmigaVideoHybrid)
      (fields
        (field (name Reference) U)
        (field (name Value) VIDIOT)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name R3) (type input))
        (pin (num 4) (name R2) (type input))
        (pin (num 5) (name R1) (type input))
        (pin (num 6) (name R0) (type input))
        (pin (num 7) (name ROUT) (type output))
        (pin (num 8) (name G3) (type input))
        (pin (num 9) (name G2) (type input))
        (pin (num 10) (name G1) (type input))
        (pin (num 11) (name G0) (type input))
        (pin (num 12) (name GOUT) (type output))
        (pin (num 13) (name B3) (type input))
        (pin (num 14) (name B2) (type input))
        (pin (num 15) (name B1) (type input))
        (pin (num 16) (name B0) (type input))
        (pin (num 17) (name BOUT) (type output))
        (pin (num 18) (name CSYNC) (type input))
        (pin (num 19) (name COMP_OUT) (type output))
        (pin (num 20) (name SYNC_OUT) (type output))
        (pin (num 21) (name VCC) (type power_in))
        (pin (num 22) (name GND) (type power_in))))
    (libpart (lib VIDIOT) (part VIDIOT_ANNEX)
      (description "Video DAC Color Annex")
      (docs https://github.com/SukkoPera/OpenAmigaVideoHybrid)
      (fields
        (field (name Reference) U)
        (field (name Value) VIDIOT_ANNEX)
        (field (name Footprint) MODULE))
      (pins
        (pin (num 1) (name BURST) (type input))
        (pin (num 2) (name GATE) (type input))
        (pin (num 3) (name V+) (type input))))
    (libpart (lib XX4256) (part XX4256)
      (fields
        (field (name Reference) U)
        (field (name Value) XX4256)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name D1) (type BiDi))
        (pin (num 2) (name D2) (type BiDi))
        (pin (num 3) (name ~WE) (type input))
        (pin (num 4) (name ~RAS) (type input))
        (pin (num 5) (name NC) (type passive))
        (pin (num 6) (name A0) (type input))
        (pin (num 7) (name A1) (type input))
        (pin (num 8) (name A2) (type input))
        (pin (num 9) (name A3) (type input))
        (pin (num 10) (name VCC) (type power_in))
        (pin (num 11) (name A4) (type input))
        (pin (num 12) (name A5) (type input))
        (pin (num 13) (name A6) (type input))
        (pin (num 14) (name A7) (type input))
        (pin (num 15) (name A8) (type input))
        (pin (num 16) (name ~OE) (type input))
        (pin (num 17) (name ~CAS) (type input))
        (pin (num 18) (name D3) (type BiDi))
        (pin (num 19) (name D4) (type BiDi))
        (pin (num 20) (name GND) (type power_in))))
    (libpart (lib amipower) (part Amiga_Power_Conn)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (fields
        (field (name Reference) CN)
        (field (name Value) Amiga_Power_Conn))
      (pins
        (pin (num 1) (name +5V) (type power_out))
        (pin (num 2) (name SH1) (type passive))
        (pin (num 3) (name +12V) (type power_out))
        (pin (num 4) (name GND) (type power_out))
        (pin (num 5) (name -12V) (type power_out))
        (pin (num 6) (name SH2) (type power_out))))
    (libpart (lib conn) (part CONN_4)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_4))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_8)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_8))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib db23_male_mountingholes) (part DB23_Male_MountingHoles)
      (description "25-pin male D-SUB connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Male*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB23_Male_MountingHoles))
      (pins
        (pin (num 0) (name PAD) (type passive))
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))))
    (libpart (lib db23_mountingholes_2sides) (part DB23_MountingHoles_2sides)
      (description "25-pin male D-SUB connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Male*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB23_MountingHoles_2sides))
      (pins
        (pin (num 0) (name PAD) (type passive))
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))))
    (libpart (lib db25_female_mountingholes) (part DB25_Female_MountingHoles)
      (description "25-pin female D-SUB connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Female*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB25_Female_MountingHoles))
      (pins
        (pin (num 0) (name PAD) (type passive))
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))))
    (libpart (lib db25_male_mountingholes) (part DB25_Male_MountingHoles)
      (description "25-pin male D-SUB connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Male*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB25_Male_MountingHoles))
      (pins
        (pin (num 0) (name PAD) (type passive))
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))
        (pin (num 11) (name 11) (type passive))
        (pin (num 12) (name 12) (type passive))
        (pin (num 13) (name 13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P24) (type passive))
        (pin (num 25) (name P25) (type passive))))
    (libpart (lib db9_male_mountingholes) (part DB9_Male_MountingHoles)
      (description "9-pin male D-SUB connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Male*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB9_Male_MountingHoles))
      (pins
        (pin (num 0) (name PAD) (type passive))
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))))
    (libpart (lib emi_filter_lcl_small) (part EMI_Filter_LCL)
      (description "EMI T-filter (LCL)")
      (docs http://www.murata.com/~/media/webrenewal/support/library/catalog/products/emc/emifil/c31e.ashx?la=en-gb)
      (footprints
        (fp Filter*)
        (fp Resonator*))
      (fields
        (field (name Reference) FL)
        (field (name Value) EMI_Filter_LCL))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib linefilter) (part L)
      (description "Line Filter")
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) LF)
        (field (name Value) L))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib mc1489) (part MC1489)
      (description "Quad Line EIA-232D Receivers")
      (docs https://www.onsemi.com/pub/Collateral/MC1488-D.PDF)
      (fields
        (field (name Reference) U)
        (field (name Value) MC1489)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name IN_A) (type input))
        (pin (num 2) (name CTL_A) (type input))
        (pin (num 3) (name OUT_A) (type output))
        (pin (num 4) (name IN_B) (type input))
        (pin (num 5) (name CTL_A) (type input))
        (pin (num 6) (name OUT_B) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT_C) (type output))
        (pin (num 9) (name CTL_A) (type input))
        (pin (num 10) (name IN_C) (type input))
        (pin (num 11) (name OUT_D) (type output))
        (pin (num 12) (name CTL_A) (type input))
        (pin (num 13) (name IN_D) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib ne555) (part NE555)
      (description "Timer, DIP-8/SOIC-8/SSOP-8")
      (docs http://www.ti.com/lit/ds/symlink/lm555.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp TSSOP*3x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) NE555))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name TR) (type input))
        (pin (num 3) (name Q) (type output))
        (pin (num 4) (name R) (type input))
        (pin (num 5) (name CV) (type input))
        (pin (num 6) (name THR) (type input))
        (pin (num 7) (name DIS) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib r_pack05) (part R_Pack05)
      (description "5 resistor network, parallel topology, DIP package")
      (docs ~)
      (footprints
        (fp DIP*)
        (fp SOIC*))
      (fields
        (field (name Reference) RP)
        (field (name Value) R_Pack05))
      (pins
        (pin (num 1) (name R1.1) (type passive))
        (pin (num 2) (name R1.2) (type passive))
        (pin (num 3) (name R2.1) (type passive))
        (pin (num 4) (name R2.2) (type passive))
        (pin (num 5) (name R3.1) (type passive))
        (pin (num 6) (name R3.2) (type passive))
        (pin (num 7) (name R4.1) (type passive))
        (pin (num 8) (name R4.2) (type passive))
        (pin (num 9) (name R5.1) (type passive))
        (pin (num 10) (name R5.2) (type passive))))
    (libpart (lib void) (part Void)
      (fields
        (field (name Reference) V)
        (field (name Value) Void)))
    (libpart (lib xtal) (part XTAL)
      (description "Crystal Clock Oscillator")
      (docs http://www.txccorp.com/download/products/osc/7C_o.pdf)
      (footprints
        (fp Oscillator*SMD*TXC*7C*5.0x3.2mm*))
      (fields
        (field (name Reference) X)
        (field (name Value) XTAL)
        (field (name Footprint) Oscillator:Oscillator_SMD_TXC_7C-4Pin_5.0x3.2mm))
      (pins
        (pin (num 1) (name ~EN) (type input))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT) (type output))
        (pin (num 14) (name VDD) (type power_in)))))
  (libraries
    (library (logical 68000D)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/68000D.lib))
    (library (logical 74ls157)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/74ls157.lib))
    (library (logical 74ls244)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/74ls244.lib))
    (library (logical 74ls245)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/74ls245.lib))
    (library (logical 74ls258)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/74ls258.lib))
    (library (logical 74ls373)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/74ls373.lib))
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical AMIGA_ROM)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/AMIGA_ROM.lib))
    (library (logical Amplifier_Operational)
      (uri /usr/share/kicad/library/Amplifier_Operational.lib))
    (library (logical BUSEXP)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/BUSEXP.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical DENISE)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/DENISE.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Diode)
      (uri /usr/share/kicad/library/Diode.lib))
    (library (logical Dispatcher)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/Dispatcher.lib))
    (library (logical FAT_AGNUS_8375)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/FAT_AGNUS_8375.lib))
    (library (logical GARY)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/GARY.lib))
    (library (logical Jumper)
      (uri /usr/share/kicad/library/Jumper.lib))
    (library (logical Jumper_3_Bridged23)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/Jumper_3_Bridged23.lib))
    (library (logical MC1488)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/MC1488.lib))
    (library (logical MSM6242B)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/MSM6242B.lib))
    (library (logical Mechanical)
      (uri /usr/share/kicad/library/Mechanical.lib))
    (library (logical PAULA)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/PAULA.lib))
    (library (logical PJRAN1X1U01X)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/PJRAN1X1U01X.lib))
    (library (logical TRAPDOOR)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/TRAPDOOR.lib))
    (library (logical Transistor_BJT)
      (uri /usr/share/kicad/library/Transistor_BJT.lib))
    (library (logical VIA_8520)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/VIA_8520.lib))
    (library (logical VIDIOT)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/VIDIOT.lib))
    (library (logical XX4256)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/XX4256.lib))
    (library (logical amipower)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/amipower.lib))
    (library (logical conn)
      (uri /home/sukko/Documents/kicad/lib/libs-walter/library/conn.lib))
    (library (logical db23_male_mountingholes)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/db23_male_mountingholes.lib))
    (library (logical db23_mountingholes_2sides)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/db23_mountingholes_2sides.lib))
    (library (logical db25_female_mountingholes)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/db25_female_mountingholes.lib))
    (library (logical db25_male_mountingholes)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/db25_male_mountingholes.lib))
    (library (logical db9_male_mountingholes)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/db9_male_mountingholes.lib))
    (library (logical emi_filter_lcl_small)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/emi_filter_lcl_small.lib))
    (library (logical linefilter)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/linefilter.lib))
    (library (logical mc1489)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/mc1489.lib))
    (library (logical ne555)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/ne555.lib))
    (library (logical r_pack05)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/r_pack05.lib))
    (library (logical void)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/void.lib))
    (library (logical xtal)
      (uri /home/sukko/Documents/kicad/Raemixx500/libs/xtal.lib)))
  (nets
    (net (code 2) (name ~BR)
      (node (ref RP104) (pin 7))
      (node (ref P1) (pin 60))
      (node (ref U1) (pin 13)))
    (net (code 3) (name ~BEER)
      (node (ref U1) (pin 22))
      (node (ref P1) (pin 46))
      (node (ref RP104) (pin 5)))
    (net (code 4) (name ~BG)
      (node (ref U1) (pin 11))
      (node (ref P1) (pin 64)))
    (net (code 5) (name ~HLT)
      (node (ref U5) (pin 42))
      (node (ref U1) (pin 17))
      (node (ref P1) (pin 55))
      (node (ref RP101) (pin 3)))
    (net (code 6) (name ~BGACK)
      (node (ref U1) (pin 12))
      (node (ref P1) (pin 62))
      (node (ref U5) (pin 14))
      (node (ref RP104) (pin 6)))
    (net (code 7) (name E)
      (node (ref R109) (pin 2))
      (node (ref P1) (pin 50))
      (node (ref U1) (pin 20)))
    (net (code 8) (name 7MHZ)
      (node (ref P1) (pin 7))
      (node (ref U1) (pin 15))
      (node (ref R106) (pin 1))
      (node (ref E103) (pin 1)))
    (net (code 9) (name "Net-(R113-Pad1)")
      (node (ref U5) (pin 4))
      (node (ref R113) (pin 1)))
    (net (code 10) (name "Net-(R112-Pad2)")
      (node (ref R112) (pin 2))
      (node (ref U11) (pin 1))
      (node (ref U13) (pin 1)))
    (net (code 11) (name "Net-(R112-Pad1)")
      (node (ref U5) (pin 3))
      (node (ref R112) (pin 1)))
    (net (code 12) (name "Net-(R111-Pad1)")
      (node (ref U5) (pin 25))
      (node (ref R111) (pin 1)))
    (net (code 13) (name "Net-(R113-Pad2)")
      (node (ref U12) (pin 1))
      (node (ref U10) (pin 19))
      (node (ref U12) (pin 19))
      (node (ref R113) (pin 2))
      (node (ref U10) (pin 1)))
    (net (code 14) (name "Net-(R111-Pad2)")
      (node (ref R111) (pin 2))
      (node (ref U13) (pin 11))
      (node (ref U11) (pin 11)))
    (net (code 15) (name GND)
      (node (ref U32) (pin 8))
      (node (ref E632) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U12) (pin 10))
      (node (ref U34) (pin 10))
      (node (ref C32) (pin 2))
      (node (ref U36) (pin 7))
      (node (ref U35) (pin 10))
      (node (ref P9) (pin 54))
      (node (ref P9) (pin 22))
      (node (ref C804) (pin 2))
      (node (ref P9) (pin 4))
      (node (ref P9) (pin 3))
      (node (ref MT7) (pin 1))
      (node (ref C811) (pin 2))
      (node (ref LF1) (pin 8))
      (node (ref C803) (pin 1))
      (node (ref P9) (pin 21))
      (node (ref C821) (pin 2))
      (node (ref P9) (pin 34))
      (node (ref C813) (pin 2))
      (node (ref C802) (pin 2))
      (node (ref P9) (pin 53))
      (node (ref C816) (pin 2))
      (node (ref C815) (pin 2))
      (node (ref C814) (pin 2))
      (node (ref E110) (pin 2))
      (node (ref JP7A1) (pin 1))
      (node (ref MT4) (pin 1))
      (node (ref MT2) (pin 1))
      (node (ref MT1) (pin 1))
      (node (ref C801) (pin 2))
      (node (ref C812) (pin 2))
      (node (ref MT6) (pin 1))
      (node (ref U13) (pin 10))
      (node (ref MT5) (pin 1))
      (node (ref C822) (pin 1))
      (node (ref C403) (pin 2))
      (node (ref U40) (pin 19))
      (node (ref U41) (pin 19))
      (node (ref C4) (pin 2))
      (node (ref E406) (pin 2))
      (node (ref U4) (pin 37))
      (node (ref HY1) (pin 22))
      (node (ref HY1) (pin 1))
      (node (ref U41) (pin 10))
      (node (ref C712) (pin 2))
      (node (ref C711) (pin 2))
      (node (ref U35) (pin 19))
      (node (ref E502) (pin 2))
      (node (ref E503) (pin 2))
      (node (ref U34) (pin 1))
      (node (ref CN9) (pin 20))
      (node (ref CN9) (pin 19))
      (node (ref CN9) (pin 18))
      (node (ref CN9) (pin 17))
      (node (ref E405) (pin 2))
      (node (ref E404) (pin 2))
      (node (ref E403) (pin 2))
      (node (ref U40) (pin 10))
      (node (ref C402) (pin 2))
      (node (ref C401) (pin 2))
      (node (ref R409) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref X1) (pin 7))
      (node (ref X1) (pin 1))
      (node (ref C37) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref E631) (pin 2))
      (node (ref C713) (pin 2))
      (node (ref Q711) (pin 1))
      (node (ref CN8) (pin 6))
      (node (ref CN8) (pin 2))
      (node (ref CN10) (pin 1))
      (node (ref E435) (pin 2))
      (node (ref U35) (pin 1))
      (node (ref E501) (pin 2))
      (node (ref BT9) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U9) (pin 9))
      (node (ref C913) (pin 2))
      (node (ref JP9) (pin 1))
      (node (ref U10) (pin 10))
      (node (ref TC9) (pin 2))
      (node (ref C911) (pin 1))
      (node (ref E433) (pin 2))
      (node (ref E431) (pin 2))
      (node (ref E432) (pin 2))
      (node (ref RP107) (pin 10))
      (node (ref E423) (pin 2))
      (node (ref E704) (pin 2))
      (node (ref U37) (pin 10))
      (node (ref CN4) (pin 1))
      (node (ref E408) (pin 2))
      (node (ref E401) (pin 2))
      (node (ref E426) (pin 2))
      (node (ref CN3) (pin 1))
      (node (ref E415) (pin 2))
      (node (ref U2) (pin 41))
      (node (ref U1) (pin 53))
      (node (ref U1) (pin 16))
      (node (ref U5) (pin 40))
      (node (ref U5) (pin 24))
      (node (ref E414) (pin 2))
      (node (ref U15) (pin 8))
      (node (ref C15) (pin 2))
      (node (ref CN6) (pin 7))
      (node (ref J93) (pin 3))
      (node (ref CN6) (pin 0))
      (node (ref U6) (pin 12))
      (node (ref U6) (pin 31))
      (node (ref C6) (pin 2))
      (node (ref J92) (pin 3))
      (node (ref RP111) (pin 10))
      (node (ref U5) (pin 1))
      (node (ref U37) (pin 7))
      (node (ref C701) (pin 2))
      (node (ref U3) (pin 8))
      (node (ref C3) (pin 2))
      (node (ref C307) (pin 2))
      (node (ref RP109) (pin 10))
      (node (ref RP102) (pin 10))
      (node (ref P1) (pin 4))
      (node (ref P1) (pin 49))
      (node (ref RP106) (pin 10))
      (node (ref P1) (pin 1))
      (node (ref P1) (pin 12))
      (node (ref P1) (pin 13))
      (node (ref P1) (pin 2))
      (node (ref P1) (pin 25))
      (node (ref P1) (pin 3))
      (node (ref P1) (pin 85))
      (node (ref RP108) (pin 10))
      (node (ref P1) (pin 61))
      (node (ref P1) (pin 37))
      (node (ref RP105) (pin 10))
      (node (ref U11) (pin 10))
      (node (ref CN1) (pin 0))
      (node (ref FB802) (pin 2))
      (node (ref RP101) (pin 10))
      (node (ref E416) (pin 2))
      (node (ref C412) (pin 2))
      (node (ref C413) (pin 2))
      (node (ref C411) (pin 2))
      (node (ref CN1) (pin 8))
      (node (ref U37) (pin 13))
      (node (ref RP104) (pin 10))
      (node (ref U2) (pin 82))
      (node (ref C14) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref E101) (pin 2))
      (node (ref U2) (pin 58))
      (node (ref E703) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref P1) (pin 73))
      (node (ref E702) (pin 2))
      (node (ref RP110) (pin 10))
      (node (ref J91) (pin 3))
      (node (ref E413) (pin 2))
      (node (ref E412) (pin 2))
      (node (ref E411) (pin 2))
      (node (ref U42) (pin 1))
      (node (ref E417) (pin 2))
      (node (ref E303) (pin 2))
      (node (ref C42) (pin 2))
      (node (ref U15) (pin 15))
      (node (ref E441) (pin 2))
      (node (ref E443) (pin 2))
      (node (ref RP401) (pin 10))
      (node (ref E422) (pin 2))
      (node (ref E424) (pin 2))
      (node (ref CN13) (pin 6))
      (node (ref E421) (pin 2))
      (node (ref E427) (pin 2))
      (node (ref CN2) (pin 0))
      (node (ref CN2) (pin 8))
      (node (ref C421) (pin 2))
      (node (ref C423) (pin 2))
      (node (ref C422) (pin 2))
      (node (ref E425) (pin 2))
      (node (ref E444) (pin 2))
      (node (ref E442) (pin 2))
      (node (ref E537) (pin 2))
      (node (ref U39) (pin 7))
      (node (ref U38) (pin 7))
      (node (ref C39) (pin 2))
      (node (ref E535) (pin 2))
      (node (ref U6) (pin 11))
      (node (ref E106) (pin 2))
      (node (ref E107) (pin 2))
      (node (ref E108) (pin 2))
      (node (ref E302) (pin 2))
      (node (ref E532) (pin 2))
      (node (ref E534) (pin 2))
      (node (ref E533) (pin 2))
      (node (ref E103) (pin 2))
      (node (ref E794) (pin 2))
      (node (ref U33) (pin 15))
      (node (ref U33) (pin 15))
      (node (ref U33) (pin 15))
      (node (ref U33) (pin 8))
      (node (ref C33) (pin 2))
      (node (ref E793) (pin 2))
      (node (ref E792) (pin 2))
      (node (ref E791) (pin 2))
      (node (ref E109) (pin 2))
      (node (ref E102) (pin 2))
      (node (ref E407) (pin 2))
      (node (ref E105) (pin 2))
      (node (ref E104) (pin 2))
      (node (ref E618) (pin 2))
      (node (ref E617) (pin 2))
      (node (ref CN11) (pin 1))
      (node (ref CN11) (pin 11))
      (node (ref CN11) (pin 13))
      (node (ref E666) (pin 2))
      (node (ref C99) (pin 2))
      (node (ref E622) (pin 2))
      (node (ref E611) (pin 2))
      (node (ref E612) (pin 2))
      (node (ref CN11) (pin 27))
      (node (ref CN11) (pin 21))
      (node (ref CN11) (pin 23))
      (node (ref CN11) (pin 25))
      (node (ref E519) (pin 2))
      (node (ref E521) (pin 2))
      (node (ref CN11) (pin 29))
      (node (ref E602) (pin 2))
      (node (ref CN11) (pin 19))
      (node (ref CN11) (pin 15))
      (node (ref U22) (pin 16))
      (node (ref CN11) (pin 17))
      (node (ref U33) (pin 15))
      (node (ref E621) (pin 2))
      (node (ref E517) (pin 2))
      (node (ref E518) (pin 2))
      (node (ref U20) (pin 16))
      (node (ref U21) (pin 16))
      (node (ref E619) (pin 2))
      (node (ref E620) (pin 2))
      (node (ref CN7) (pin 0))
      (node (ref CN5) (pin 0))
      (node (ref CN12) (pin 3))
      (node (ref E402) (pin 2))
      (node (ref CN12) (pin 2))
      (node (ref CN11) (pin 5))
      (node (ref Q501) (pin 1))
      (node (ref CN11) (pin 31))
      (node (ref CN11) (pin 33))
      (node (ref R501) (pin 1))
      (node (ref CN11) (pin 7))
      (node (ref D501) (pin 2))
      (node (ref CN11) (pin 9))
      (node (ref E531) (pin 2))
      (node (ref E512) (pin 2))
      (node (ref E511) (pin 2))
      (node (ref U19) (pin 20))
      (node (ref U23) (pin 16))
      (node (ref C18) (pin 2))
      (node (ref CN14) (pin 3))
      (node (ref CN14) (pin 2))
      (node (ref U22) (pin 20))
      (node (ref U18) (pin 20))
      (node (ref E536) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref E625) (pin 2))
      (node (ref E626) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref U23) (pin 20))
      (node (ref E538) (pin 2))
      (node (ref U7) (pin 1))
      (node (ref U8) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref FB101) (pin 2))
      (node (ref E524) (pin 2))
      (node (ref U16) (pin 16))
      (node (ref FB102) (pin 2))
      (node (ref E522) (pin 2))
      (node (ref E523) (pin 2))
      (node (ref U17) (pin 16))
      (node (ref U16) (pin 20))
      (node (ref E624) (pin 2))
      (node (ref U20) (pin 20))
      (node (ref U18) (pin 16))
      (node (ref C20) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref U21) (pin 20))
      (node (ref U17) (pin 20))
      (node (ref C16) (pin 2))
      (node (ref E623) (pin 2))
      (node (ref U19) (pin 16))
      (node (ref CN7) (pin 20))
      (node (ref CN7) (pin 21))
      (node (ref CN7) (pin 22))
      (node (ref CN7) (pin 25))
      (node (ref E616) (pin 2))
      (node (ref CN7) (pin 24))
      (node (ref CN5) (pin 3))
      (node (ref CN7) (pin 18))
      (node (ref CN7) (pin 19))
      (node (ref CN5) (pin 4))
      (node (ref CN5) (pin 7))
      (node (ref CN5) (pin 6))
      (node (ref CN5) (pin 5))
      (node (ref E615) (pin 2))
      (node (ref E614) (pin 2))
      (node (ref CN7) (pin 23))
      (node (ref E613) (pin 2))
      (node (ref E434) (pin 2))
      (node (ref E514) (pin 2))
      (node (ref CN15) (pin 4))
      (node (ref E515) (pin 2))
      (node (ref CN9) (pin 16))
      (node (ref E513) (pin 2))
      (node (ref E516) (pin 2))
      (node (ref CN7) (pin 17))
      (node (ref E601) (pin 2))
      (node (ref CN9) (pin 0))
      (node (ref E520) (pin 2))
      (node (ref CN9) (pin 13)))
    (net (code 16) (name "Net-(FB101-Pad1)")
      (node (ref X1) (pin 8))
      (node (ref FB101) (pin 1)))
    (net (code 17) (name ~XCLKEN)
      (node (ref U33) (pin 1))
      (node (ref U33) (pin 1))
      (node (ref U33) (pin 1))
      (node (ref U33) (pin 1))
      (node (ref R403) (pin 2))
      (node (ref CN9) (pin 2)))
    (net (code 18) (name "Net-(FB102-Pad1)")
      (node (ref FB102) (pin 1))
      (node (ref U33) (pin 12)))
    (net (code 19) (name "Net-(FB101-Pad3)")
      (node (ref U33) (pin 13))
      (node (ref FB101) (pin 3)))
    (net (code 20) (name XCLK)
      (node (ref RP403) (pin 1))
      (node (ref U33) (pin 14))
      (node (ref R404) (pin 2)))
    (net (code 21) (name "Net-(E666-Pad1)")
      (node (ref E666) (pin 1))
      (node (ref U2) (pin 34))
      (node (ref FB102) (pin 3)))
    (net (code 22) (name "Net-(R101-Pad1)")
      (node (ref R101) (pin 1))
      (node (ref U5) (pin 43)))
    (net (code 23) (name ~EXTICK)
      (node (ref JP7B1) (pin 1))
      (node (ref U5) (pin 32))
      (node (ref RP501) (pin 9))
      (node (ref JP7A1) (pin 2)))
    (net (code 24) (name ~OVR)
      (node (ref CN15) (pin 2))
      (node (ref RP104) (pin 9))
      (node (ref U5) (pin 29))
      (node (ref P1) (pin 17)))
    (net (code 25) (name CCK)
      (node (ref R103) (pin 1))
      (node (ref U33) (pin 5))
      (node (ref U3) (pin 28))
      (node (ref E108) (pin 1))
      (node (ref U5) (pin 28))
      (node (ref U33) (pin 6))
      (node (ref U35) (pin 15))
      (node (ref U41) (pin 6))
      (node (ref U4) (pin 36)))
    (net (code 26) (name ~LDS)
      (node (ref U1) (pin 8))
      (node (ref RP101) (pin 5))
      (node (ref U2) (pin 51))
      (node (ref P1) (pin 70))
      (node (ref U5) (pin 10)))
    (net (code 27) (name ~UDS)
      (node (ref RP101) (pin 6))
      (node (ref U5) (pin 11))
      (node (ref U1) (pin 7))
      (node (ref U2) (pin 52))
      (node (ref P1) (pin 72)))
    (net (code 28) (name ~AS)
      (node (ref U2) (pin 24))
      (node (ref P1) (pin 74))
      (node (ref U5) (pin 13))
      (node (ref RP101) (pin 8))
      (node (ref U1) (pin 6)))
    (net (code 29) (name "Net-(R102-Pad1)")
      (node (ref R102) (pin 1))
      (node (ref U5) (pin 2)))
    (net (code 30) (name "Net-(R114-Pad2)")
      (node (ref U5) (pin 21))
      (node (ref R114) (pin 2)))
    (net (code 31) (name ~RAS1)
      (node (ref U2) (pin 56))
      (node (ref U35) (pin 4)))
    (net (code 32) (name ~RAS0)
      (node (ref U35) (pin 2))
      (node (ref U2) (pin 57)))
    (net (code 33) (name ~CASU)
      (node (ref U2) (pin 54))
      (node (ref U32) (pin 13))
      (node (ref U35) (pin 8)))
    (net (code 34) (name ~CASL)
      (node (ref U2) (pin 53))
      (node (ref U35) (pin 6))
      (node (ref U32) (pin 3)))
    (net (code 35) (name ~VSYNC)
      (node (ref U2) (pin 79))
      (node (ref RP403) (pin 7))
      (node (ref JP7B1) (pin 3)))
    (net (code 36) (name ~CDAC)
      (node (ref R105) (pin 1))
      (node (ref E106) (pin 1))
      (node (ref U33) (pin 2))
      (node (ref U5) (pin 26))
      (node (ref U4) (pin 34))
      (node (ref U33) (pin 3)))
    (net (code 37) (name CCKQ)
      (node (ref R104) (pin 1))
      (node (ref U5) (pin 27))
      (node (ref U33) (pin 11))
      (node (ref U33) (pin 10))
      (node (ref U3) (pin 29))
      (node (ref E107) (pin 1)))
    (net (code 38) (name ~INT3)
      (node (ref U2) (pin 17))
      (node (ref U3) (pin 17)))
    (net (code 39) (name DMAL)
      (node (ref U2) (pin 18))
      (node (ref U3) (pin 12)))
    (net (code 40) (name ~CSYNC)
      (node (ref U41) (pin 8))
      (node (ref U41) (pin 9))
      (node (ref U4) (pin 32))
      (node (ref U2) (pin 80)))
    (net (code 41) (name ~HSYNC)
      (node (ref U2) (pin 81))
      (node (ref RP403) (pin 5))
      (node (ref U8) (pin 19))
      (node (ref R402) (pin 2)))
    (net (code 42) (name ~LPEN)
      (node (ref JP8) (pin 2))
      (node (ref U2) (pin 78)))
    (net (code 43) (name ~WE)
      (node (ref U2) (pin 21))
      (node (ref U35) (pin 17)))
    (net (code 44) (name ~EVEN_CIA)
      (node (ref U8) (pin 23))
      (node (ref U37) (pin 6)))
    (net (code 45) (name ~ODD_CIA)
      (node (ref U37) (pin 3))
      (node (ref U7) (pin 23)))
    (net (code 46) (name "Net-(R103-Pad2)")
      (node (ref U2) (pin 39))
      (node (ref R103) (pin 2)))
    (net (code 47) (name "Net-(R104-Pad2)")
      (node (ref R104) (pin 2))
      (node (ref U2) (pin 38)))
    (net (code 48) (name "Net-(R105-Pad2)")
      (node (ref U2) (pin 36))
      (node (ref R105) (pin 2)))
    (net (code 49) (name "Net-(U2-Pad25)")
      (node (ref U2) (pin 25))
      (node (ref U5) (pin 20)))
    (net (code 50) (name ~CLKWR)
      (node (ref U5) (pin 23))
      (node (ref U9) (pin 10))
      (node (ref P9) (pin 50)))
    (net (code 51) (name ~CLKRD)
      (node (ref P9) (pin 49))
      (node (ref U9) (pin 8))
      (node (ref U5) (pin 22)))
    (net (code 52) (name XRDY)
      (node (ref RP104) (pin 8))
      (node (ref CN15) (pin 3))
      (node (ref U5) (pin 31))
      (node (ref P1) (pin 18)))
    (net (code 53) (name OVL)
      (node (ref RP101) (pin 9))
      (node (ref U7) (pin 2))
      (node (ref U5) (pin 30)))
    (net (code 54) (name ~ROMEN)
      (node (ref U6) (pin 13))
      (node (ref R114) (pin 1)))
    (net (code 55) (name ~RST)
      (node (ref U37) (pin 12))
      (node (ref U1) (pin 18))
      (node (ref U3) (pin 11))
      (node (ref P1) (pin 53))
      (node (ref RP101) (pin 4))
      (node (ref U2) (pin 16))
      (node (ref U5) (pin 41)))
    (net (code 56) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19))
      (node (ref U5) (pin 19)))
    (net (code 57) (name "Net-(U2-Pad20)")
      (node (ref U5) (pin 15))
      (node (ref U2) (pin 20)))
    (net (code 58) (name R~W)
      (node (ref U5) (pin 12))
      (node (ref U1) (pin 9))
      (node (ref U2) (pin 22))
      (node (ref U8) (pin 22))
      (node (ref P1) (pin 68))
      (node (ref U7) (pin 22))
      (node (ref RP101) (pin 7)))
    (net (code 59) (name "Net-(U2-Pad23)")
      (node (ref U2) (pin 23))
      (node (ref U5) (pin 18)))
    (net (code 60) (name ~VMA)
      (node (ref RP104) (pin 3))
      (node (ref P1) (pin 51))
      (node (ref U1) (pin 19))
      (node (ref U37) (pin 2))
      (node (ref U37) (pin 5)))
    (net (code 61) (name "Net-(JP2-Pad2)")
      (node (ref U2) (pin 59))
      (node (ref JP2) (pin 2)))
    (net (code 62) (name ~VPA)
      (node (ref RP104) (pin 4))
      (node (ref P1) (pin 48))
      (node (ref U1) (pin 21))
      (node (ref R102) (pin 2)))
    (net (code 63) (name "Net-(R106-Pad2)")
      (node (ref R106) (pin 2))
      (node (ref U2) (pin 37))
      (node (ref R107) (pin 2)))
    (net (code 64) (name 7MHZ_A)
      (node (ref E794) (pin 1))
      (node (ref C403) (pin 1))
      (node (ref U4) (pin 35))
      (node (ref R107) (pin 1)))
    (net (code 65) (name "Net-(C99-Pad1)")
      (node (ref C99) (pin 1))
      (node (ref U2) (pin 40)))
    (net (code 66) (name ~DTACK)
      (node (ref R101) (pin 2))
      (node (ref U1) (pin 10))
      (node (ref P1) (pin 66))
      (node (ref RP104) (pin 2)))
    (net (code 67) (name "Net-(CN9-Pad15)")
      (node (ref E402) (pin 3))
      (node (ref CN9) (pin 15)))
    (net (code 68) (name "Net-(CN9-Pad14)")
      (node (ref RP402) (pin 2))
      (node (ref CN9) (pin 14)))
    (net (code 69) (name "/Denise & Video Stuff/ar")
      (node (ref HY1) (pin 7))
      (node (ref E431) (pin 1)))
    (net (code 70) (name "/Denise & Video Stuff/ag")
      (node (ref E432) (pin 1))
      (node (ref HY1) (pin 12)))
    (net (code 71) (name "/Denise & Video Stuff/ab")
      (node (ref E433) (pin 1))
      (node (ref HY1) (pin 17)))
    (net (code 72) (name "/Denise & Video Stuff/cck_c")
      (node (ref E402) (pin 1))
      (node (ref RP403) (pin 3)))
    (net (code 73) (name +12V)
      (node (ref E602) (pin 1))
      (node (ref CN12) (pin 4))
      (node (ref HY2) (pin 3))
      (node (ref U38) (pin 14))
      (node (ref E404) (pin 1))
      (node (ref E502) (pin 1))
      (node (ref CN14) (pin 4))
      (node (ref C821) (pin 1))
      (node (ref E704) (pin 1))
      (node (ref C802) (pin 1))
      (node (ref R911) (pin 2))
      (node (ref LF1) (pin 5))
      (node (ref P9) (pin 55))
      (node (ref R301) (pin 1)))
    (net (code 74) (name -12V)
      (node (ref E403) (pin 1))
      (node (ref E503) (pin 1))
      (node (ref E703) (pin 1))
      (node (ref R302) (pin 2))
      (node (ref LF1) (pin 6))
      (node (ref C822) (pin 2))
      (node (ref U38) (pin 1))
      (node (ref C803) (pin 2))
      (node (ref P9) (pin 56)))
    (net (code 75) (name VCC)
      (node (ref U39) (pin 14))
      (node (ref C14) (pin 1))
      (node (ref R405) (pin 1))
      (node (ref R403) (pin 1))
      (node (ref RP108) (pin 1))
      (node (ref Q503) (pin 1))
      (node (ref CN12) (pin 1))
      (node (ref RP104) (pin 1))
      (node (ref E407) (pin 1))
      (node (ref Q502) (pin 1))
      (node (ref R507) (pin 2))
      (node (ref U38) (pin 10))
      (node (ref U6) (pin 32))
      (node (ref R505) (pin 2))
      (node (ref E101) (pin 1))
      (node (ref U38) (pin 5))
      (node (ref U38) (pin 13))
      (node (ref C1) (pin 1))
      (node (ref RP105) (pin 1))
      (node (ref C39) (pin 1))
      (node (ref R401) (pin 1))
      (node (ref R191) (pin 1))
      (node (ref R506) (pin 2))
      (node (ref RP110) (pin 1))
      (node (ref E702) (pin 1))
      (node (ref RP101) (pin 1))
      (node (ref R408) (pin 1))
      (node (ref R192) (pin 1))
      (node (ref E601) (pin 1))
      (node (ref R404) (pin 1))
      (node (ref R402) (pin 1))
      (node (ref R305) (pin 1))
      (node (ref U42) (pin 8))
      (node (ref C42) (pin 1))
      (node (ref E406) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref LF1) (pin 7))
      (node (ref RP102) (pin 1))
      (node (ref R309) (pin 1))
      (node (ref U19) (pin 10))
      (node (ref C13) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref U12) (pin 20))
      (node (ref U10) (pin 20))
      (node (ref U23) (pin 10))
      (node (ref C19) (pin 1))
      (node (ref R915) (pin 1))
      (node (ref P9) (pin 52))
      (node (ref P9) (pin 51))
      (node (ref C813) (pin 1))
      (node (ref C801) (pin 1))
      (node (ref R914) (pin 1))
      (node (ref RP501) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref U11) (pin 20))
      (node (ref C804) (pin 1))
      (node (ref U37) (pin 14))
      (node (ref P9) (pin 2))
      (node (ref P9) (pin 1))
      (node (ref C811) (pin 1))
      (node (ref RP111) (pin 1))
      (node (ref C812) (pin 1))
      (node (ref U7) (pin 20))
      (node (ref C32) (pin 1))
      (node (ref U36) (pin 14))
      (node (ref U35) (pin 20))
      (node (ref U34) (pin 20))
      (node (ref C7) (pin 1))
      (node (ref U8) (pin 20))
      (node (ref U13) (pin 20))
      (node (ref C8) (pin 1))
      (node (ref RP109) (pin 1))
      (node (ref U18) (pin 10))
      (node (ref C12) (pin 1))
      (node (ref U22) (pin 10))
      (node (ref CN14) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref C814) (pin 1))
      (node (ref U32) (pin 16))
      (node (ref U42) (pin 4))
      (node (ref C10) (pin 1))
      (node (ref R712) (pin 2))
      (node (ref C815) (pin 1))
      (node (ref C816) (pin 1))
      (node (ref U6) (pin 22))
      (node (ref RP107) (pin 1))
      (node (ref RP106) (pin 1))
      (node (ref D911) (pin 1))
      (node (ref CN13) (pin 4))
      (node (ref J93) (pin 1))
      (node (ref R916) (pin 1))
      (node (ref J91) (pin 1))
      (node (ref U15) (pin 16))
      (node (ref U5) (pin 17))
      (node (ref U5) (pin 48))
      (node (ref U5) (pin 6))
      (node (ref U1) (pin 14))
      (node (ref U1) (pin 49))
      (node (ref R711) (pin 2))
      (node (ref E501) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref RP401) (pin 1))
      (node (ref E110) (pin 1))
      (node (ref J92) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref R201) (pin 1))
      (node (ref R202) (pin 1))
      (node (ref U17) (pin 10))
      (node (ref U21) (pin 10))
      (node (ref C37) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref U20) (pin 10))
      (node (ref C34) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref C20) (pin 1))
      (node (ref U16) (pin 10)))
    (net (code 76) (name "Net-(CN9-Pad10)")
      (node (ref E434) (pin 3))
      (node (ref CN9) (pin 10)))
    (net (code 77) (name "/Denise & Video Stuff/bcsync_a")
      (node (ref RP403) (pin 9))
      (node (ref U41) (pin 12)))
    (net (code 78) (name "/Denise & Video Stuff/bpixelsw")
      (node (ref RP402) (pin 1))
      (node (ref U41) (pin 13)))
    (net (code 79) (name "Net-(CN9-Pad12)")
      (node (ref CN9) (pin 12))
      (node (ref RP403) (pin 8)))
    (net (code 80) (name "/Denise & Video Stuff/br3")
      (node (ref HY1) (pin 3))
      (node (ref RP402) (pin 9))
      (node (ref U40) (pin 18)))
    (net (code 81) (name "Net-(CN9-Pad23)")
      (node (ref E405) (pin 3))
      (node (ref CN9) (pin 23)))
    (net (code 82) (name "Net-(CN9-Pad21)")
      (node (ref E403) (pin 3))
      (node (ref CN9) (pin 21)))
    (net (code 83) (name "Net-(CN9-Pad22)")
      (node (ref E404) (pin 3))
      (node (ref CN9) (pin 22)))
    (net (code 84) (name "Net-(CN9-Pad4)")
      (node (ref CN9) (pin 4))
      (node (ref E432) (pin 3)))
    (net (code 85) (name "Net-(CN9-Pad3)")
      (node (ref CN9) (pin 3))
      (node (ref E431) (pin 3)))
    (net (code 86) (name "Net-(CN9-Pad5)")
      (node (ref E433) (pin 3))
      (node (ref CN9) (pin 5)))
    (net (code 87) (name "Net-(CN9-Pad6)")
      (node (ref CN9) (pin 6))
      (node (ref RP402) (pin 4)))
    (net (code 88) (name "/Denise & Video Stuff/rbcsync_a")
      (node (ref RP403) (pin 10))
      (node (ref JP11) (pin 1)))
    (net (code 89) (name "Net-(HY1-Pad20)")
      (node (ref JP11) (pin 3))
      (node (ref HY1) (pin 20)))
    (net (code 90) (name "/Denise & Video Stuff/csync_out")
      (node (ref E434) (pin 1))
      (node (ref JP11) (pin 2)))
    (net (code 91) (name "Net-(C401-Pad1)")
      (node (ref HY1) (pin 21))
      (node (ref C401) (pin 1))
      (node (ref R405) (pin 2)))
    (net (code 92) (name VDDA)
      (node (ref U4) (pin 19))
      (node (ref E406) (pin 3))
      (node (ref C4) (pin 1))
      (node (ref R406) (pin 2))
      (node (ref E405) (pin 1)))
    (net (code 93) (name VD)
      (node (ref C402) (pin 1))
      (node (ref U41) (pin 20))
      (node (ref HY1) (pin 2))
      (node (ref U40) (pin 1))
      (node (ref U41) (pin 1))
      (node (ref U40) (pin 20))
      (node (ref C41) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref R406) (pin 1)))
    (net (code 94) (name "Net-(U4-Pad24)")
      (node (ref U41) (pin 5))
      (node (ref U4) (pin 24)))
    (net (code 95) (name "Net-(U4-Pad25)")
      (node (ref U4) (pin 25))
      (node (ref U41) (pin 4)))
    (net (code 96) (name "Net-(U4-Pad26)")
      (node (ref U41) (pin 3))
      (node (ref U4) (pin 26)))
    (net (code 97) (name "Net-(U4-Pad27)")
      (node (ref U41) (pin 2))
      (node (ref U4) (pin 27)))
    (net (code 98) (name "Net-(U4-Pad28)")
      (node (ref U4) (pin 28))
      (node (ref U40) (pin 9)))
    (net (code 99) (name "Net-(U4-Pad29)")
      (node (ref U4) (pin 29))
      (node (ref U40) (pin 8)))
    (net (code 100) (name "Net-(U4-Pad30)")
      (node (ref U40) (pin 7))
      (node (ref U4) (pin 30)))
    (net (code 101) (name "Net-(U4-Pad33)")
      (node (ref U41) (pin 7))
      (node (ref U4) (pin 33)))
    (net (code 102) (name "Net-(U4-Pad31)")
      (node (ref U40) (pin 6))
      (node (ref U4) (pin 31)))
    (net (code 103) (name "Net-(U4-Pad20)")
      (node (ref U40) (pin 5))
      (node (ref U4) (pin 20)))
    (net (code 104) (name "Net-(U4-Pad21)")
      (node (ref U40) (pin 4))
      (node (ref U4) (pin 21)))
    (net (code 105) (name "Net-(U4-Pad22)")
      (node (ref U4) (pin 22))
      (node (ref U40) (pin 3)))
    (net (code 106) (name "Net-(U4-Pad23)")
      (node (ref U4) (pin 23))
      (node (ref U40) (pin 2)))
    (net (code 107) (name "/Denise & Video Stuff/br2")
      (node (ref U40) (pin 17))
      (node (ref HY1) (pin 4)))
    (net (code 108) (name "/Denise & Video Stuff/br1")
      (node (ref HY1) (pin 5))
      (node (ref U40) (pin 16)))
    (net (code 109) (name "/Denise & Video Stuff/br0")
      (node (ref HY1) (pin 6))
      (node (ref U40) (pin 15)))
    (net (code 110) (name M1H)
      (node (ref E442) (pin 3))
      (node (ref U4) (pin 8)))
    (net (code 111) (name M1V)
      (node (ref U4) (pin 39))
      (node (ref E444) (pin 3)))
    (net (code 112) (name M0H)
      (node (ref E443) (pin 3))
      (node (ref U4) (pin 9)))
    (net (code 113) (name M0V)
      (node (ref E441) (pin 3))
      (node (ref U4) (pin 38)))
    (net (code 114) (name "/Denise & Video Stuff/bb1")
      (node (ref U41) (pin 16))
      (node (ref HY1) (pin 15)))
    (net (code 115) (name "/Denise & Video Stuff/bcsync_b")
      (node (ref U41) (pin 11))
      (node (ref HY1) (pin 18)))
    (net (code 116) (name "/Denise & Video Stuff/bb2")
      (node (ref U41) (pin 17))
      (node (ref HY1) (pin 14)))
    (net (code 117) (name "/Denise & Video Stuff/bg3")
      (node (ref U40) (pin 14))
      (node (ref HY1) (pin 8))
      (node (ref RP402) (pin 7)))
    (net (code 118) (name "/Denise & Video Stuff/bb0")
      (node (ref RP402) (pin 3))
      (node (ref HY1) (pin 16))
      (node (ref U41) (pin 15)))
    (net (code 119) (name "/Denise & Video Stuff/bb3")
      (node (ref U41) (pin 18))
      (node (ref RP402) (pin 5))
      (node (ref HY1) (pin 13)))
    (net (code 120) (name "/Denise & Video Stuff/bg0")
      (node (ref U40) (pin 11))
      (node (ref HY1) (pin 11)))
    (net (code 121) (name "/Denise & Video Stuff/bg1")
      (node (ref U40) (pin 12))
      (node (ref HY1) (pin 10)))
    (net (code 122) (name "/Denise & Video Stuff/bg2")
      (node (ref HY1) (pin 9))
      (node (ref U40) (pin 13)))
    (net (code 123) (name "Net-(CN9-Pad9)")
      (node (ref CN9) (pin 9))
      (node (ref RP402) (pin 10)))
    (net (code 124) (name "Net-(CN9-Pad7)")
      (node (ref RP402) (pin 6))
      (node (ref CN9) (pin 7)))
    (net (code 125) (name "Net-(CN9-Pad8)")
      (node (ref CN9) (pin 8))
      (node (ref RP402) (pin 8)))
    (net (code 126) (name "Net-(CN9-Pad11)")
      (node (ref CN9) (pin 11))
      (node (ref RP403) (pin 6)))
    (net (code 127) (name "Net-(CN9-Pad1)")
      (node (ref RP403) (pin 2))
      (node (ref CN9) (pin 1)))
    (net (code 128) (name "/Denise & Video Stuff/bcck")
      (node (ref U41) (pin 14))
      (node (ref RP403) (pin 4))
      (node (ref HY2) (pin 1)))
    (net (code 129) (name "Net-(E435-Pad1)")
      (node (ref HY1) (pin 19))
      (node (ref E435) (pin 1)))
    (net (code 130) (name "Net-(CN10-Pad3)")
      (node (ref CN10) (pin 3)))
    (net (code 131) (name "Net-(CN10-Pad2)")
      (node (ref R409) (pin 1))
      (node (ref E435) (pin 3))
      (node (ref CN10) (pin 2)))
    (net (code 132) (name "Net-(HY2-Pad2)")
      (node (ref U4) (pin 18))
      (node (ref HY2) (pin 2)))
    (net (code 133) (name ~CLKCS)
      (node (ref U36) (pin 12))
      (node (ref R916) (pin 2))
      (node (ref JP9) (pin 2))
      (node (ref P9) (pin 33))
      (node (ref U36) (pin 11)))
    (net (code 134) (name "Net-(C911-Pad2)")
      (node (ref Y9) (pin 3))
      (node (ref C911) (pin 2))
      (node (ref U9) (pin 17)))
    (net (code 135) (name "Net-(U9-Pad1)")
      (node (ref U9) (pin 1))
      (node (ref Y9) (pin 2)))
    (net (code 136) (name "Net-(BT9-Pad1)")
      (node (ref D913) (pin 2))
      (node (ref BT9) (pin 1)))
    (net (code 137) (name "Net-(TC9-Pad1)")
      (node (ref Y9) (pin 1))
      (node (ref TC9) (pin 1))
      (node (ref U9) (pin 16)))
    (net (code 138) (name "Net-(R914-Pad2)")
      (node (ref R914) (pin 2))
      (node (ref U9) (pin 15))
      (node (ref U9) (pin 3)))
    (net (code 139) (name "Net-(D911-Pad2)")
      (node (ref R911) (pin 1))
      (node (ref D911) (pin 2))
      (node (ref D912) (pin 2)))
    (net (code 140) (name "Net-(C9-Pad1)")
      (node (ref C913) (pin 1))
      (node (ref D912) (pin 1))
      (node (ref D913) (pin 1))
      (node (ref U9) (pin 18))
      (node (ref C9) (pin 1)))
    (net (code 141) (name "Net-(R915-Pad2)")
      (node (ref R915) (pin 2))
      (node (ref U36) (pin 10))
      (node (ref U9) (pin 2)))
    (net (code 142) (name ~CCK_A)
      (node (ref E104) (pin 3))
      (node (ref E102) (pin 1))
      (node (ref P9) (pin 40)))
    (net (code 143) (name ~BRAS0)
      (node (ref P9) (pin 38))
      (node (ref JP3B1) (pin 2))
      (node (ref RP203) (pin 1)))
    (net (code 144) (name ~BCASU1)
      (node (ref JP4B1) (pin 3))
      (node (ref P9) (pin 36))
      (node (ref U32) (pin 11)))
    (net (code 145) (name ~BWE)
      (node (ref U35) (pin 3))
      (node (ref RP203) (pin 9))
      (node (ref P9) (pin 39)))
    (net (code 146) (name ~BRAS1)
      (node (ref JP3A1) (pin 1))
      (node (ref P9) (pin 37))
      (node (ref RP203) (pin 3)))
    (net (code 147) (name ~BCASL1)
      (node (ref U32) (pin 5))
      (node (ref JP4A1) (pin 3))
      (node (ref P9) (pin 35)))
    (net (code 149) (name "Net-(JP7A1-Pad3)")
      (node (ref P9) (pin 32))
      (node (ref JP7A1) (pin 3)))
    (net (code 153) (name ~CCKQ_A)
      (node (ref E109) (pin 1))
      (node (ref E105) (pin 3))
      (node (ref U15) (pin 1)))
    (net (code 154) (name "Net-(E424-Pad1)")
      (node (ref E424) (pin 1))
      (node (ref U15) (pin 14))
      (node (ref RP401) (pin 2)))
    (net (code 155) (name "Net-(CN2-Pad2)")
      (node (ref CN2) (pin 2))
      (node (ref E422) (pin 3)))
    (net (code 156) (name "Net-(CN2-Pad1)")
      (node (ref CN2) (pin 1))
      (node (ref E421) (pin 3)))
    (net (code 157) (name "Net-(CN2-Pad4)")
      (node (ref CN2) (pin 4))
      (node (ref E424) (pin 3)))
    (net (code 158) (name "Net-(CN2-Pad3)")
      (node (ref CN2) (pin 3))
      (node (ref E423) (pin 3)))
    (net (code 159) (name "Net-(E442-Pad1)")
      (node (ref E442) (pin 1))
      (node (ref U15) (pin 12)))
    (net (code 160) (name "Net-(E444-Pad1)")
      (node (ref U15) (pin 9))
      (node (ref E444) (pin 1)))
    (net (code 161) (name "Net-(E441-Pad1)")
      (node (ref U15) (pin 4))
      (node (ref E441) (pin 1)))
    (net (code 162) (name "Net-(E443-Pad1)")
      (node (ref U15) (pin 7))
      (node (ref E443) (pin 1)))
    (net (code 163) (name "Net-(E412-Pad1)")
      (node (ref RP401) (pin 9))
      (node (ref E412) (pin 1))
      (node (ref U15) (pin 6)))
    (net (code 164) (name "Net-(E414-Pad1)")
      (node (ref E414) (pin 1))
      (node (ref U15) (pin 5))
      (node (ref RP401) (pin 6)))
    (net (code 165) (name "Net-(E422-Pad1)")
      (node (ref U15) (pin 13))
      (node (ref RP401) (pin 4))
      (node (ref E422) (pin 1)))
    (net (code 166) (name "Net-(E411-Pad1)")
      (node (ref E411) (pin 1))
      (node (ref RP401) (pin 8))
      (node (ref U15) (pin 3)))
    (net (code 167) (name ~FIRE1)
      (node (ref JP8) (pin 3))
      (node (ref U7) (pin 9))
      (node (ref E425) (pin 1)))
    (net (code 168) (name "Net-(C423-Pad1)")
      (node (ref E426) (pin 3))
      (node (ref CN2) (pin 9))
      (node (ref C423) (pin 1)))
    (net (code 169) (name "Net-(CN2-Pad7)")
      (node (ref E408) (pin 3))
      (node (ref CN2) (pin 7)))
    (net (code 170) (name "Net-(C421-Pad1)")
      (node (ref CN2) (pin 6))
      (node (ref E425) (pin 3))
      (node (ref C421) (pin 1)))
    (net (code 171) (name "Net-(C422-Pad1)")
      (node (ref CN2) (pin 5))
      (node (ref E427) (pin 3))
      (node (ref C422) (pin 1)))
    (net (code 172) (name "Net-(E401-Pad1)")
      (node (ref E401) (pin 1))
      (node (ref R401) (pin 2)))
    (net (code 173) (name ~FIRE0)
      (node (ref JP8) (pin 1))
      (node (ref U7) (pin 8))
      (node (ref E415) (pin 1)))
    (net (code 174) (name "/Paula & Audio Stuff/pot1x")
      (node (ref U3) (pin 35))
      (node (ref E427) (pin 1))
      (node (ref C313) (pin 1)))
    (net (code 175) (name "Net-(CN1-Pad3)")
      (node (ref CN1) (pin 3))
      (node (ref E413) (pin 3)))
    (net (code 176) (name "Net-(CN1-Pad2)")
      (node (ref CN1) (pin 2))
      (node (ref E412) (pin 3)))
    (net (code 177) (name "/Paula & Audio Stuff/pot0y")
      (node (ref E416) (pin 1))
      (node (ref U3) (pin 33))
      (node (ref C312) (pin 1)))
    (net (code 178) (name "Net-(CN1-Pad1)")
      (node (ref E411) (pin 3))
      (node (ref CN1) (pin 1)))
    (net (code 179) (name "Net-(E413-Pad1)")
      (node (ref RP401) (pin 7))
      (node (ref E413) (pin 1))
      (node (ref U15) (pin 2)))
    (net (code 180) (name "Net-(E421-Pad1)")
      (node (ref E421) (pin 1))
      (node (ref RP401) (pin 5))
      (node (ref U15) (pin 10)))
    (net (code 181) (name "Net-(CN1-Pad4)")
      (node (ref CN1) (pin 4))
      (node (ref E414) (pin 3)))
    (net (code 182) (name "Net-(C334-Pad2)")
      (node (ref R334) (pin 2))
      (node (ref C334) (pin 2))
      (node (ref C335) (pin 1)))
    (net (code 183) (name "Net-(E303-Pad1)")
      (node (ref R334) (pin 1))
      (node (ref E303) (pin 1))
      (node (ref R335) (pin 1)))
    (net (code 184) (name GNDA)
      (node (ref C323) (pin 2))
      (node (ref FB802) (pin 1))
      (node (ref C308) (pin 2))
      (node (ref C305) (pin 2))
      (node (ref C306) (pin 2))
      (node (ref R304) (pin 1))
      (node (ref E305) (pin 2))
      (node (ref C302) (pin 1))
      (node (ref C304) (pin 1))
      (node (ref C303) (pin 2))
      (node (ref U3) (pin 34))
      (node (ref C312) (pin 2))
      (node (ref C313) (pin 2))
      (node (ref C301) (pin 2))
      (node (ref R325) (pin 2))
      (node (ref R335) (pin 2))
      (node (ref C314) (pin 2))
      (node (ref E306) (pin 2))
      (node (ref C333) (pin 2))
      (node (ref C311) (pin 2)))
    (net (code 185) (name "Net-(CN3-Pad2)")
      (node (ref E303) (pin 3))
      (node (ref CN3) (pin 2))
      (node (ref CN4) (pin 3)))
    (net (code 186) (name VAC)
      (node (ref C305) (pin 1))
      (node (ref R304) (pin 2))
      (node (ref U14) (pin 10))
      (node (ref R303) (pin 1))
      (node (ref U14) (pin 12))
      (node (ref C306) (pin 1)))
    (net (code 187) (name "Net-(C332-Pad1)")
      (node (ref U14) (pin 6))
      (node (ref C334) (pin 1))
      (node (ref C335) (pin 2))
      (node (ref U14) (pin 7))
      (node (ref C332) (pin 1)))
    (net (code 188) (name "Net-(C332-Pad2)")
      (node (ref C332) (pin 2))
      (node (ref R333) (pin 2))
      (node (ref R332) (pin 1)))
    (net (code 189) (name "/Paula & Audio Stuff/right")
      (node (ref U3) (pin 30))
      (node (ref E305) (pin 1)))
    (net (code 190) (name +VDC)
      (node (ref Q301) (pin 1))
      (node (ref C303) (pin 1))
      (node (ref R301) (pin 2))
      (node (ref R307) (pin 2))
      (node (ref C301) (pin 1))
      (node (ref U14) (pin 4)))
    (net (code 191) (name "/Paula & Audio Stuff/left")
      (node (ref E306) (pin 1))
      (node (ref U3) (pin 31)))
    (net (code 192) (name "Net-(R306-Pad2)")
      (node (ref U38) (pin 3))
      (node (ref R306) (pin 2)))
    (net (code 193) (name "Net-(C324-Pad2)")
      (node (ref R324) (pin 2))
      (node (ref JP10B1) (pin 1))
      (node (ref C325) (pin 1))
      (node (ref C324) (pin 2)))
    (net (code 194) (name "Net-(Q301-Pad2)")
      (node (ref R307) (pin 1))
      (node (ref Q301) (pin 2))
      (node (ref R306) (pin 1)))
    (net (code 195) (name ~DKRD)
      (node (ref CN11) (pin 30))
      (node (ref U3) (pin 37))
      (node (ref E612) (pin 1))
      (node (ref R305) (pin 2)))
    (net (code 196) (name ~LED)
      (node (ref R503) (pin 2))
      (node (ref R505) (pin 1))
      (node (ref U7) (pin 3))
      (node (ref U38) (pin 2)))
    (net (code 197) (name "Net-(C333-Pad1)")
      (node (ref Q331) (pin 2))
      (node (ref C333) (pin 1))
      (node (ref R333) (pin 1))
      (node (ref U14) (pin 5)))
    (net (code 198) (name "Net-(Q331-Pad3)")
      (node (ref R336) (pin 1))
      (node (ref Q331) (pin 3)))
    (net (code 199) (name "Net-(C331-Pad1)")
      (node (ref C331) (pin 1))
      (node (ref R331) (pin 1))
      (node (ref R332) (pin 2))
      (node (ref U14) (pin 8))
      (node (ref Q331) (pin 1)))
    (net (code 200) (name "Net-(C308-Pad1)")
      (node (ref C308) (pin 1))
      (node (ref R308) (pin 1))
      (node (ref Q301) (pin 3))
      (node (ref R326) (pin 2))
      (node (ref R336) (pin 2)))
    (net (code 201) (name "Net-(C331-Pad2)")
      (node (ref U14) (pin 9))
      (node (ref C331) (pin 2))
      (node (ref E305) (pin 3))
      (node (ref R339) (pin 1))
      (node (ref R331) (pin 2)))
    (net (code 202) (name "Net-(C323-Pad1)")
      (node (ref R323) (pin 1))
      (node (ref U14) (pin 3))
      (node (ref C323) (pin 1))
      (node (ref Q321) (pin 2)))
    (net (code 203) (name "Net-(C322-Pad1)")
      (node (ref U14) (pin 1))
      (node (ref U14) (pin 2))
      (node (ref C322) (pin 1))
      (node (ref C325) (pin 2))
      (node (ref C324) (pin 1)))
    (net (code 204) (name "Net-(C321-Pad2)")
      (node (ref C321) (pin 2))
      (node (ref E306) (pin 3))
      (node (ref U14) (pin 13))
      (node (ref R321) (pin 2)))
    (net (code 205) (name "/Paula & Audio Stuff/pot1y")
      (node (ref U3) (pin 36))
      (node (ref C314) (pin 1))
      (node (ref E426) (pin 1)))
    (net (code 206) (name "/Paula & Audio Stuff/pot0x")
      (node (ref U3) (pin 32))
      (node (ref E417) (pin 1))
      (node (ref C311) (pin 1)))
    (net (code 207) (name "Net-(E302-Pad1)")
      (node (ref R324) (pin 1))
      (node (ref E302) (pin 1))
      (node (ref R325) (pin 1)))
    (net (code 208) (name "Net-(Q321-Pad3)")
      (node (ref R326) (pin 1))
      (node (ref Q321) (pin 3)))
    (net (code 209) (name "Net-(C321-Pad1)")
      (node (ref R322) (pin 2))
      (node (ref Q321) (pin 1))
      (node (ref R321) (pin 1))
      (node (ref C321) (pin 1))
      (node (ref U14) (pin 14)))
    (net (code 210) (name "Net-(C322-Pad2)")
      (node (ref R322) (pin 1))
      (node (ref R323) (pin 2))
      (node (ref C322) (pin 2)))
    (net (code 211) (name -VDC)
      (node (ref C304) (pin 2))
      (node (ref C302) (pin 2))
      (node (ref U14) (pin 11))
      (node (ref R302) (pin 1))
      (node (ref R308) (pin 2)))
    (net (code 212) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref C307) (pin 1))
      (node (ref R303) (pin 2))
      (node (ref R309) (pin 2))
      (node (ref U3) (pin 27)))
    (net (code 213) (name ~RXD)
      (node (ref U39) (pin 3))
      (node (ref U3) (pin 41)))
    (net (code 214) (name "Net-(C411-Pad1)")
      (node (ref CN1) (pin 6))
      (node (ref C411) (pin 1))
      (node (ref E415) (pin 3)))
    (net (code 215) (name "Net-(E408-Pad1)")
      (node (ref R408) (pin 2))
      (node (ref E408) (pin 1)))
    (net (code 216) (name "Net-(CN3-Pad3)")
      (node (ref CN4) (pin 2))
      (node (ref E302) (pin 3))
      (node (ref CN3) (pin 3)))
    (net (code 217) (name "Net-(E423-Pad1)")
      (node (ref U15) (pin 11))
      (node (ref E423) (pin 1))
      (node (ref RP401) (pin 3)))
    (net (code 218) (name ~INT6)
      (node (ref U3) (pin 18))
      (node (ref P1) (pin 22))
      (node (ref U8) (pin 21))
      (node (ref R192) (pin 2)))
    (net (code 219) (name "Net-(C412-Pad1)")
      (node (ref E417) (pin 3))
      (node (ref C412) (pin 1))
      (node (ref CN1) (pin 5)))
    (net (code 220) (name "Net-(CN1-Pad7)")
      (node (ref E401) (pin 3))
      (node (ref CN1) (pin 7)))
    (net (code 221) (name "Net-(C413-Pad1)")
      (node (ref CN1) (pin 9))
      (node (ref E416) (pin 3))
      (node (ref C413) (pin 1)))
    (net (code 222) (name ~INT2)
      (node (ref P1) (pin 19))
      (node (ref U3) (pin 16))
      (node (ref R191) (pin 2))
      (node (ref CN15) (pin 1))
      (node (ref U7) (pin 21)))
    (net (code 223) (name ~TXD)
      (node (ref U38) (pin 9))
      (node (ref U3) (pin 40)))
    (net (code 224) (name ~DKWD)
      (node (ref U5) (pin 9))
      (node (ref U3) (pin 38)))
    (net (code 225) (name DKWE)
      (node (ref U5) (pin 8))
      (node (ref U3) (pin 39)))
    (net (code 226) (name RGA4)
      (node (ref U4) (pin 14))
      (node (ref U2) (pin 30))
      (node (ref U3) (pin 23)))
    (net (code 227) (name RGA1)
      (node (ref U3) (pin 26))
      (node (ref U4) (pin 17))
      (node (ref U2) (pin 33)))
    (net (code 228) (name RGA2)
      (node (ref U4) (pin 16))
      (node (ref U2) (pin 32))
      (node (ref U3) (pin 25)))
    (net (code 229) (name RGA3)
      (node (ref U4) (pin 15))
      (node (ref U3) (pin 24))
      (node (ref U2) (pin 31)))
    (net (code 230) (name RGA5)
      (node (ref U4) (pin 13))
      (node (ref U2) (pin 29))
      (node (ref U3) (pin 22)))
    (net (code 231) (name RGA6)
      (node (ref U2) (pin 28))
      (node (ref U4) (pin 12))
      (node (ref U3) (pin 21)))
    (net (code 232) (name RGA7)
      (node (ref U3) (pin 20))
      (node (ref U2) (pin 27))
      (node (ref U4) (pin 11)))
    (net (code 233) (name RGA8)
      (node (ref U4) (pin 10))
      (node (ref U2) (pin 26))
      (node (ref U3) (pin 19)))
    (net (code 234) (name "Net-(JP10A1-Pad2)")
      (node (ref JP10A1) (pin 2))
      (node (ref R339) (pin 2)))
    (net (code 235) (name AUDIN)
      (node (ref C501) (pin 1))
      (node (ref JP10A1) (pin 1)))
    (net (code 236) (name AUDOUT)
      (node (ref C502) (pin 2))
      (node (ref JP10B1) (pin 2)))
    (net (code 237) (name "Net-(RP105-Pad9)")
      (node (ref RP105) (pin 9)))
    (net (code 238) (name "Net-(RP101-Pad2)")
      (node (ref RP101) (pin 2)))
    (net (code 239) (name A21)
      (node (ref U5) (pin 37))
      (node (ref P1) (pin 58))
      (node (ref RP105) (pin 4))
      (node (ref U1) (pin 50)))
    (net (code 240) (name A18)
      (node (ref P1) (pin 52))
      (node (ref U1) (pin 46))
      (node (ref J91) (pin 2))
      (node (ref U5) (pin 34))
      (node (ref RP105) (pin 7))
      (node (ref U2) (pin 77)))
    (net (code 241) (name A19)
      (node (ref P1) (pin 54))
      (node (ref RP105) (pin 6))
      (node (ref J92) (pin 2))
      (node (ref U1) (pin 47))
      (node (ref U5) (pin 35))
      (node (ref JP2) (pin 3)))
    (net (code 242) (name A20)
      (node (ref U5) (pin 36))
      (node (ref U2) (pin 35))
      (node (ref U1) (pin 48))
      (node (ref P1) (pin 56))
      (node (ref J93) (pin 2))
      (node (ref RP105) (pin 5)))
    (net (code 243) (name ~IORESET)
      (node (ref E520) (pin 1))
      (node (ref E615) (pin 1))
      (node (ref U37) (pin 8)))
    (net (code 244) (name ~RESET)
      (node (ref U37) (pin 9))
      (node (ref U8) (pin 34))
      (node (ref U37) (pin 11))
      (node (ref U7) (pin 34)))
    (net (code 245) (name "Net-(RP102-Pad2)")
      (node (ref RP102) (pin 2)))
    (net (code 246) (name "Net-(RP102-Pad3)")
      (node (ref RP102) (pin 3)))
    (net (code 247) (name "/Kickstart ROM/a19_rom")
      (node (ref U6) (pin 1))
      (node (ref J92) (pin 4)))
    (net (code 248) (name "/Kickstart ROM/a20_rom")
      (node (ref J93) (pin 4))
      (node (ref U6) (pin 42)))
    (net (code 249) (name "/Kickstart ROM/a18_rom")
      (node (ref U6) (pin 2))
      (node (ref J91) (pin 4)))
    (net (code 250) (name D15)
      (node (ref U1) (pin 54))
      (node (ref U6) (pin 30))
      (node (ref U13) (pin 19))
      (node (ref P1) (pin 63))
      (node (ref RP108) (pin 2))
      (node (ref U12) (pin 17))
      (node (ref U8) (pin 26)))
    (net (code 251) (name D14)
      (node (ref P1) (pin 65))
      (node (ref U1) (pin 55))
      (node (ref U13) (pin 16))
      (node (ref RP108) (pin 3))
      (node (ref U12) (pin 15))
      (node (ref U8) (pin 27))
      (node (ref U6) (pin 28)))
    (net (code 252) (name D13)
      (node (ref P1) (pin 67))
      (node (ref U6) (pin 26))
      (node (ref U8) (pin 28))
      (node (ref RP108) (pin 4))
      (node (ref U13) (pin 15))
      (node (ref U12) (pin 13))
      (node (ref U1) (pin 56)))
    (net (code 253) (name ~CCKQ)
      (node (ref RP103) (pin 8))
      (node (ref E791) (pin 1))
      (node (ref P1) (pin 14)))
    (net (code 254) (name CDAC)
      (node (ref RP103) (pin 4))
      (node (ref E793) (pin 1))
      (node (ref P1) (pin 15)))
    (net (code 255) (name "Net-(C33-Pad1)")
      (node (ref C33) (pin 1))
      (node (ref U33) (pin 16))
      (node (ref E407) (pin 3)))
    (net (code 256) (name "Net-(RP103-Pad1)")
      (node (ref RP103) (pin 1)))
    (net (code 257) (name "Net-(RP103-Pad10)")
      (node (ref RP103) (pin 10)))
    (net (code 258) (name "Net-(RP103-Pad2)")
      (node (ref RP103) (pin 2)))
    (net (code 259) (name ~CCK)
      (node (ref P1) (pin 16))
      (node (ref E792) (pin 1))
      (node (ref RP103) (pin 6)))
    (net (code 260) (name "Net-(RP103-Pad9)")
      (node (ref RP103) (pin 9)))
    (net (code 261) (name "Net-(E105-Pad1)")
      (node (ref U33) (pin 9))
      (node (ref RP103) (pin 7))
      (node (ref E105) (pin 1)))
    (net (code 262) (name "Net-(RP103-Pad3)")
      (node (ref U33) (pin 4))
      (node (ref RP103) (pin 3)))
    (net (code 263) (name "Net-(E104-Pad1)")
      (node (ref E104) (pin 1))
      (node (ref U33) (pin 7))
      (node (ref RP103) (pin 5)))
    (net (code 264) (name ~KBRESET)
      (node (ref U5) (pin 5))
      (node (ref JP1) (pin 2))
      (node (ref CN13) (pin 3))
      (node (ref RP501) (pin 5)))
    (net (code 265) (name "Net-(JP1-Pad1)")
      (node (ref JP1) (pin 1))
      (node (ref Q711) (pin 3)))
    (net (code 266) (name ~KBDATA)
      (node (ref RP501) (pin 3))
      (node (ref U7) (pin 39))
      (node (ref E631) (pin 3)))
    (net (code 267) (name "Net-(R713-Pad2)")
      (node (ref U42) (pin 3))
      (node (ref R713) (pin 2)))
    (net (code 268) (name "Net-(C713-Pad1)")
      (node (ref C713) (pin 1))
      (node (ref U42) (pin 5)))
    (net (code 269) (name ~KBCLOCK)
      (node (ref E632) (pin 3))
      (node (ref U7) (pin 40))
      (node (ref RP501) (pin 2)))
    (net (code 270) (name "Net-(U42-Pad7)")
      (node (ref U42) (pin 7)))
    (net (code 271) (name "Net-(C711-Pad1)")
      (node (ref U42) (pin 2))
      (node (ref R711) (pin 1))
      (node (ref C711) (pin 1)))
    (net (code 272) (name "Net-(C712-Pad1)")
      (node (ref U42) (pin 6))
      (node (ref R712) (pin 1))
      (node (ref C712) (pin 1)))
    (net (code 273) (name "Net-(C502-Pad1)")
      (node (ref CN6) (pin 11))
      (node (ref C502) (pin 1)))
    (net (code 274) (name "Net-(CN13-Pad5)")
      (node (ref CN13) (pin 5)))
    (net (code 275) (name ~SEL0)
      (node (ref J90) (pin 3))
      (node (ref U5) (pin 16))
      (node (ref CN11) (pin 10)))
    (net (code 276) (name ~SEL1)
      (node (ref E625) (pin 1))
      (node (ref CN11) (pin 12))
      (node (ref J90) (pin 4)))
    (net (code 277) (name "/Parallel & Serial/sel1_out")
      (node (ref J90) (pin 5))
      (node (ref U8) (pin 14))
      (node (ref J90) (pin 6)))
    (net (code 278) (name "/Parallel & Serial/sel0_out")
      (node (ref U8) (pin 13))
      (node (ref J90) (pin 1))
      (node (ref J90) (pin 2)))
    (net (code 279) (name "Net-(E536-Pad1)")
      (node (ref U39) (pin 10))
      (node (ref E536) (pin 1)))
    (net (code 280) (name "Net-(E535-Pad1)")
      (node (ref U39) (pin 4))
      (node (ref E535) (pin 1)))
    (net (code 281) (name "Net-(E537-Pad1)")
      (node (ref U39) (pin 13))
      (node (ref E537) (pin 1)))
    (net (code 282) (name "Net-(Q711-Pad2)")
      (node (ref Q711) (pin 2))
      (node (ref R713) (pin 1)))
    (net (code 283) (name "Net-(CN7-Pad11)")
      (node (ref CN7) (pin 11))
      (node (ref E522) (pin 3)))
    (net (code 284) (name "Net-(CN7-Pad13)")
      (node (ref E524) (pin 3))
      (node (ref CN7) (pin 13)))
    (net (code 285) (name "Net-(CN7-Pad12)")
      (node (ref CN7) (pin 12))
      (node (ref E523) (pin 3)))
    (net (code 286) (name "Net-(E523-Pad1)")
      (node (ref E523) (pin 1))
      (node (ref U8) (pin 40))
      (node (ref U8) (pin 3)))
    (net (code 287) (name "Net-(CN7-Pad10)")
      (node (ref E521) (pin 3))
      (node (ref CN7) (pin 10)))
    (net (code 288) (name "Net-(CN7-Pad9)")
      (node (ref E519) (pin 3))
      (node (ref CN7) (pin 9)))
    (net (code 289) (name "Net-(CN7-Pad8)")
      (node (ref E518) (pin 3))
      (node (ref CN7) (pin 8)))
    (net (code 290) (name "Net-(CN7-Pad7)")
      (node (ref CN7) (pin 7))
      (node (ref E517) (pin 3)))
    (net (code 291) (name "/Parallel & Serial/~init")
      (node (ref E520) (pin 3))
      (node (ref CN7) (pin 16)))
    (net (code 292) (name "/Parallel & Serial/~auto")
      (node (ref E501) (pin 3))
      (node (ref CN7) (pin 14)))
    (net (code 293) (name "/Parallel & Serial/~err")
      (node (ref CN7) (pin 15)))
    (net (code 294) (name "Net-(CN7-Pad6)")
      (node (ref E516) (pin 3))
      (node (ref CN7) (pin 6)))
    (net (code 295) (name "Net-(CN7-Pad5)")
      (node (ref E515) (pin 3))
      (node (ref CN7) (pin 5)))
    (net (code 296) (name "Net-(CN7-Pad4)")
      (node (ref E514) (pin 3))
      (node (ref CN7) (pin 4)))
    (net (code 297) (name "Net-(CN7-Pad3)")
      (node (ref CN7) (pin 3))
      (node (ref E513) (pin 3)))
    (net (code 298) (name "Net-(CN7-Pad2)")
      (node (ref CN7) (pin 2))
      (node (ref E512) (pin 3)))
    (net (code 299) (name "Net-(CN7-Pad1)")
      (node (ref CN7) (pin 1))
      (node (ref E511) (pin 3)))
    (net (code 300) (name "Net-(E511-Pad1)")
      (node (ref RP501) (pin 10))
      (node (ref E511) (pin 1))
      (node (ref U7) (pin 18)))
    (net (code 301) (name "/Parallel & Serial/pp4")
      (node (ref U7) (pin 14))
      (node (ref E516) (pin 1)))
    (net (code 302) (name "/Parallel & Serial/pp7")
      (node (ref E519) (pin 1))
      (node (ref U7) (pin 17)))
    (net (code 303) (name "/Parallel & Serial/pp6")
      (node (ref E518) (pin 1))
      (node (ref U7) (pin 16)))
    (net (code 304) (name "/Parallel & Serial/pp5")
      (node (ref U7) (pin 15))
      (node (ref E517) (pin 1)))
    (net (code 305) (name "/Parallel & Serial/pp3")
      (node (ref U7) (pin 13))
      (node (ref E515) (pin 1)))
    (net (code 306) (name "/Parallel & Serial/pp2")
      (node (ref E514) (pin 1))
      (node (ref U7) (pin 12)))
    (net (code 307) (name "/Parallel & Serial/pp1")
      (node (ref E513) (pin 1))
      (node (ref U7) (pin 11)))
    (net (code 308) (name "/Parallel & Serial/pp0")
      (node (ref E512) (pin 1))
      (node (ref U7) (pin 10)))
    (net (code 309) (name ~INDEX)
      (node (ref RP501) (pin 7))
      (node (ref U8) (pin 24))
      (node (ref CN11) (pin 8))
      (node (ref E626) (pin 1)))
    (net (code 310) (name ~CHNG)
      (node (ref CN11) (pin 2))
      (node (ref U7) (pin 4))
      (node (ref E616) (pin 1)))
    (net (code 311) (name ~WPROT)
      (node (ref CN11) (pin 28))
      (node (ref U7) (pin 5))
      (node (ref E618) (pin 1)))
    (net (code 312) (name ~TRK0)
      (node (ref U7) (pin 6))
      (node (ref E619) (pin 1))
      (node (ref CN11) (pin 26)))
    (net (code 313) (name ~RDY)
      (node (ref U7) (pin 7))
      (node (ref CN11) (pin 34))
      (node (ref E611) (pin 1)))
    (net (code 314) (name "Net-(E521-Pad1)")
      (node (ref RP501) (pin 6))
      (node (ref U7) (pin 24))
      (node (ref E521) (pin 1)))
    (net (code 315) (name "Net-(E522-Pad1)")
      (node (ref U8) (pin 2))
      (node (ref U8) (pin 39))
      (node (ref E522) (pin 1)))
    (net (code 316) (name "Net-(RP501-Pad8)")
      (node (ref RP501) (pin 8)))
    (net (code 317) (name "Net-(U8-Pad18)")
      (node (ref U8) (pin 18)))
    (net (code 318) (name "Net-(JP7B1-Pad2)")
      (node (ref U7) (pin 19))
      (node (ref JP7B1) (pin 2)))
    (net (code 319) (name "Net-(R109-Pad1)")
      (node (ref R109) (pin 1))
      (node (ref U8) (pin 25))
      (node (ref U7) (pin 25)))
    (net (code 320) (name "Net-(U39-Pad11)")
      (node (ref U39) (pin 11))
      (node (ref U8) (pin 7)))
    (net (code 321) (name "Net-(U39-Pad6)")
      (node (ref U39) (pin 6))
      (node (ref U8) (pin 6)))
    (net (code 322) (name "Net-(U39-Pad8)")
      (node (ref U8) (pin 5))
      (node (ref U39) (pin 8)))
    (net (code 323) (name "Net-(D501-Pad1)")
      (node (ref R502) (pin 2))
      (node (ref Q501) (pin 2))
      (node (ref R501) (pin 2))
      (node (ref D501) (pin 1)))
    (net (code 324) (name "Net-(E532-Pad1)")
      (node (ref U38) (pin 8))
      (node (ref E532) (pin 1)))
    (net (code 325) (name "Net-(U39-Pad5)")
      (node (ref U39) (pin 5)))
    (net (code 326) (name "Net-(U38-Pad4)")
      (node (ref U8) (pin 8))
      (node (ref U38) (pin 4)))
    (net (code 327) (name "Net-(U39-Pad12)")
      (node (ref U39) (pin 12)))
    (net (code 328) (name "Net-(U39-Pad9)")
      (node (ref U39) (pin 9)))
    (net (code 329) (name "Net-(U38-Pad12)")
      (node (ref U8) (pin 9))
      (node (ref U38) (pin 12)))
    (net (code 330) (name "Net-(E533-Pad1)")
      (node (ref U38) (pin 6))
      (node (ref E533) (pin 1)))
    (net (code 331) (name "Net-(E531-Pad1)")
      (node (ref E531) (pin 1))
      (node (ref U38) (pin 11)))
    (net (code 332) (name "Net-(U39-Pad2)")
      (node (ref U39) (pin 2)))
    (net (code 333) (name "Net-(E534-Pad1)")
      (node (ref U39) (pin 1))
      (node (ref E534) (pin 1)))
    (net (code 334) (name "/Parallel & Serial/dtr")
      (node (ref CN6) (pin 20))
      (node (ref E531) (pin 3)))
    (net (code 335) (name "/Parallel & Serial/bz")
      (node (ref CN6) (pin 25)))
    (net (code 336) (name "/Parallel & Serial/clk")
      (node (ref CN6) (pin 24)))
    (net (code 337) (name "/Parallel & Serial/sqd")
      (node (ref CN6) (pin 21)))
    (net (code 338) (name "/Parallel & Serial/ss")
      (node (ref CN6) (pin 23)))
    (net (code 339) (name "Net-(E538-Pad1)")
      (node (ref E538) (pin 1))
      (node (ref R502) (pin 1)))
    (net (code 340) (name "Net-(E524-Pad1)")
      (node (ref E524) (pin 1))
      (node (ref U8) (pin 4))
      (node (ref RP501) (pin 4))
      (node (ref Q501) (pin 3)))
    (net (code 341) (name "Net-(CN6-Pad22)")
      (node (ref E538) (pin 3))
      (node (ref CN6) (pin 22)))
    (net (code 342) (name "Net-(Q502-Pad2)")
      (node (ref R503) (pin 1))
      (node (ref Q502) (pin 2)))
    (net (code 343) (name "/Parallel & Serial/clock")
      (node (ref CN13) (pin 1))
      (node (ref E632) (pin 1)))
    (net (code 344) (name "/Parallel & Serial/data")
      (node (ref E631) (pin 1))
      (node (ref CN13) (pin 2)))
    (net (code 345) (name "/Parallel & Serial/inuse")
      (node (ref Q503) (pin 3))
      (node (ref CN13) (pin 8)))
    (net (code 346) (name "/Parallel & Serial/status")
      (node (ref CN13) (pin 7))
      (node (ref Q502) (pin 3))
      (node (ref R507) (pin 1)))
    (net (code 347) (name "Net-(Q503-Pad2)")
      (node (ref R504) (pin 1))
      (node (ref Q503) (pin 2)))
    (net (code 348) (name ~MTR0)
      (node (ref U36) (pin 4))
      (node (ref CN11) (pin 4))
      (node (ref R506) (pin 1))
      (node (ref CN11) (pin 16))
      (node (ref R504) (pin 2)))
    (net (code 349) (name ~STEP)
      (node (ref CN11) (pin 20))
      (node (ref E622) (pin 1))
      (node (ref U8) (pin 10)))
    (net (code 350) (name DIR)
      (node (ref CN11) (pin 18))
      (node (ref E623) (pin 1))
      (node (ref U8) (pin 11)))
    (net (code 351) (name ~SIDE)
      (node (ref E617) (pin 1))
      (node (ref CN11) (pin 32))
      (node (ref U8) (pin 12)))
    (net (code 352) (name ~SEL2)
      (node (ref E614) (pin 1))
      (node (ref U8) (pin 15)))
    (net (code 353) (name ~SEL3)
      (node (ref E624) (pin 1))
      (node (ref U8) (pin 16)))
    (net (code 354) (name ~MTR)
      (node (ref U8) (pin 17))
      (node (ref U5) (pin 7)))
    (net (code 355) (name "/Parallel & Serial/srts")
      (node (ref CN6) (pin 19)))
    (net (code 356) (name "Net-(C501-Pad2)")
      (node (ref CN6) (pin 18))
      (node (ref C501) (pin 2)))
    (net (code 357) (name "/Parallel & Serial/-v")
      (node (ref CN6) (pin 10))
      (node (ref E503) (pin 3)))
    (net (code 358) (name "/Parallel & Serial/+v")
      (node (ref E502) (pin 3))
      (node (ref CN6) (pin 9)))
    (net (code 359) (name "/Parallel & Serial/scts")
      (node (ref CN6) (pin 13)))
    (net (code 360) (name "/Parallel & Serial/scd")
      (node (ref CN6) (pin 12)))
    (net (code 361) (name "/Parallel & Serial/txc")
      (node (ref CN6) (pin 15)))
    (net (code 362) (name "/Parallel & Serial/srxd")
      (node (ref CN6) (pin 16)))
    (net (code 363) (name "/Parallel & Serial/rxc")
      (node (ref CN6) (pin 17)))
    (net (code 364) (name "/Parallel & Serial/txd")
      (node (ref E532) (pin 3))
      (node (ref CN6) (pin 2)))
    (net (code 365) (name "/Parallel & Serial/rxd")
      (node (ref E534) (pin 3))
      (node (ref CN6) (pin 3)))
    (net (code 366) (name "/Parallel & Serial/rts")
      (node (ref CN6) (pin 4))
      (node (ref E533) (pin 3)))
    (net (code 367) (name "/Parallel & Serial/cts")
      (node (ref E535) (pin 3))
      (node (ref CN6) (pin 5)))
    (net (code 368) (name "/Parallel & Serial/dsr")
      (node (ref CN6) (pin 6))
      (node (ref E536) (pin 3)))
    (net (code 369) (name "/Parallel & Serial/cd")
      (node (ref E537) (pin 3))
      (node (ref CN6) (pin 8)))
    (net (code 370) (name "/Parallel & Serial/fg")
      (node (ref CN6) (pin 1)))
    (net (code 371) (name "/Parallel & Serial/stxd")
      (node (ref CN6) (pin 14)))
    (net (code 373) (name D6)
      (node (ref U6) (pin 27))
      (node (ref U7) (pin 27))
      (node (ref RP110) (pin 3))
      (node (ref P1) (pin 84))
      (node (ref U10) (pin 15))
      (node (ref U1) (pin 63))
      (node (ref U11) (pin 16)))
    (net (code 374) (name D5)
      (node (ref P1) (pin 86))
      (node (ref U1) (pin 64))
      (node (ref RP110) (pin 4))
      (node (ref U7) (pin 28))
      (node (ref U11) (pin 15))
      (node (ref U6) (pin 25))
      (node (ref U10) (pin 13)))
    (net (code 375) (name D4)
      (node (ref U7) (pin 29))
      (node (ref U11) (pin 12))
      (node (ref U6) (pin 23))
      (node (ref U1) (pin 1))
      (node (ref U10) (pin 11))
      (node (ref RP110) (pin 9))
      (node (ref P1) (pin 83)))
    (net (code 376) (name D3)
      (node (ref P9) (pin 44))
      (node (ref U10) (pin 8))
      (node (ref U6) (pin 20))
      (node (ref U11) (pin 9))
      (node (ref U7) (pin 30))
      (node (ref U9) (pin 11))
      (node (ref P1) (pin 81))
      (node (ref U1) (pin 2))
      (node (ref RP110) (pin 8)))
    (net (code 377) (name D2)
      (node (ref U9) (pin 12))
      (node (ref P9) (pin 43))
      (node (ref U11) (pin 6))
      (node (ref U10) (pin 6))
      (node (ref U1) (pin 3))
      (node (ref P1) (pin 79))
      (node (ref RP110) (pin 7))
      (node (ref U7) (pin 31))
      (node (ref U6) (pin 18)))
    (net (code 378) (name D1)
      (node (ref U9) (pin 13))
      (node (ref RP110) (pin 6))
      (node (ref U1) (pin 4))
      (node (ref P9) (pin 42))
      (node (ref U11) (pin 5))
      (node (ref U10) (pin 4))
      (node (ref U7) (pin 32))
      (node (ref P1) (pin 77))
      (node (ref U6) (pin 16)))
    (net (code 379) (name D0)
      (node (ref U1) (pin 5))
      (node (ref U7) (pin 33))
      (node (ref U10) (pin 2))
      (node (ref U11) (pin 2))
      (node (ref RP110) (pin 5))
      (node (ref U6) (pin 14))
      (node (ref U9) (pin 14))
      (node (ref P1) (pin 75))
      (node (ref P9) (pin 41)))
    (net (code 380) (name D7)
      (node (ref RP110) (pin 2))
      (node (ref P1) (pin 82))
      (node (ref U10) (pin 17))
      (node (ref U11) (pin 19))
      (node (ref U6) (pin 29))
      (node (ref U7) (pin 26))
      (node (ref U1) (pin 62)))
    (net (code 382) (name D12)
      (node (ref RP108) (pin 5))
      (node (ref P1) (pin 69))
      (node (ref U13) (pin 12))
      (node (ref U12) (pin 11))
      (node (ref U1) (pin 57))
      (node (ref U6) (pin 24))
      (node (ref U8) (pin 29)))
    (net (code 383) (name D11)
      (node (ref U1) (pin 58))
      (node (ref RP108) (pin 6))
      (node (ref U8) (pin 30))
      (node (ref U13) (pin 9))
      (node (ref P1) (pin 71))
      (node (ref U12) (pin 8))
      (node (ref U6) (pin 21)))
    (net (code 384) (name D10)
      (node (ref U6) (pin 19))
      (node (ref U12) (pin 6))
      (node (ref RP108) (pin 7))
      (node (ref U8) (pin 31))
      (node (ref P1) (pin 76))
      (node (ref U13) (pin 6))
      (node (ref U1) (pin 59)))
    (net (code 385) (name D9)
      (node (ref U12) (pin 4))
      (node (ref P1) (pin 78))
      (node (ref U8) (pin 32))
      (node (ref U6) (pin 17))
      (node (ref RP108) (pin 8))
      (node (ref U1) (pin 60))
      (node (ref U13) (pin 5)))
    (net (code 386) (name D8)
      (node (ref U8) (pin 33))
      (node (ref U13) (pin 2))
      (node (ref RP108) (pin 9))
      (node (ref U6) (pin 15))
      (node (ref U1) (pin 61))
      (node (ref P1) (pin 80))
      (node (ref U12) (pin 2)))
    (net (code 387) (name "Net-(P1-Pad11)")
      (node (ref P1) (pin 11)))
    (net (code 388) (name "Net-(P1-Pad20)")
      (node (ref P1) (pin 20)))
    (net (code 389) (name "Net-(E704-Pad3)")
      (node (ref E704) (pin 3))
      (node (ref P1) (pin 10)))
    (net (code 390) (name "Net-(E703-Pad3)")
      (node (ref E703) (pin 3))
      (node (ref P1) (pin 8)))
    (net (code 391) (name ~IPL2)
      (node (ref U3) (pin 15))
      (node (ref RP102) (pin 9))
      (node (ref P1) (pin 44))
      (node (ref U1) (pin 23)))
    (net (code 392) (name "Net-(P1-Pad9)")
      (node (ref P1) (pin 9)))
    (net (code 393) (name FC0)
      (node (ref RP102) (pin 4))
      (node (ref P1) (pin 31))
      (node (ref U1) (pin 28)))
    (net (code 394) (name FC1)
      (node (ref P1) (pin 33))
      (node (ref RP102) (pin 5))
      (node (ref U1) (pin 27)))
    (net (code 395) (name FC2)
      (node (ref U1) (pin 26))
      (node (ref RP102) (pin 6))
      (node (ref P1) (pin 35)))
    (net (code 396) (name ~IPL1)
      (node (ref U3) (pin 14))
      (node (ref P1) (pin 42))
      (node (ref RP102) (pin 8))
      (node (ref U1) (pin 24)))
    (net (code 397) (name ~IPL0)
      (node (ref U1) (pin 25))
      (node (ref P1) (pin 40))
      (node (ref RP102) (pin 7))
      (node (ref U3) (pin 13)))
    (net (code 398) (name "Net-(E702-Pad3)")
      (node (ref P1) (pin 5))
      (node (ref P1) (pin 6))
      (node (ref E702) (pin 3)))
    (net (code 399) (name A8)
      (node (ref U1) (pin 36))
      (node (ref P1) (pin 30))
      (node (ref U2) (pin 67))
      (node (ref U6) (pin 3))
      (node (ref U7) (pin 38))
      (node (ref U8) (pin 38))
      (node (ref RP107) (pin 3)))
    (net (code 400) (name A1)
      (node (ref U2) (pin 60))
      (node (ref P1) (pin 29))
      (node (ref U1) (pin 29))
      (node (ref RP107) (pin 9))
      (node (ref U6) (pin 10)))
    (net (code 401) (name A7)
      (node (ref U2) (pin 66))
      (node (ref RP107) (pin 2))
      (node (ref U1) (pin 35))
      (node (ref U6) (pin 4))
      (node (ref P1) (pin 28)))
    (net (code 402) (name A2)
      (node (ref U1) (pin 30))
      (node (ref RP107) (pin 8))
      (node (ref U2) (pin 61))
      (node (ref P1) (pin 27))
      (node (ref U6) (pin 9))
      (node (ref U9) (pin 4))
      (node (ref P9) (pin 45)))
    (net (code 403) (name A3)
      (node (ref RP107) (pin 7))
      (node (ref U2) (pin 62))
      (node (ref P9) (pin 46))
      (node (ref U6) (pin 8))
      (node (ref P1) (pin 26))
      (node (ref U9) (pin 5))
      (node (ref U1) (pin 31)))
    (net (code 404) (name A4)
      (node (ref U2) (pin 63))
      (node (ref P9) (pin 47))
      (node (ref U6) (pin 7))
      (node (ref U9) (pin 6))
      (node (ref U1) (pin 32))
      (node (ref P1) (pin 24))
      (node (ref RP107) (pin 6)))
    (net (code 405) (name A6)
      (node (ref U6) (pin 5))
      (node (ref U1) (pin 34))
      (node (ref RP107) (pin 4))
      (node (ref P1) (pin 23))
      (node (ref U2) (pin 65)))
    (net (code 406) (name A5)
      (node (ref P1) (pin 21))
      (node (ref U1) (pin 33))
      (node (ref RP107) (pin 5))
      (node (ref U9) (pin 7))
      (node (ref P9) (pin 48))
      (node (ref U2) (pin 64))
      (node (ref U6) (pin 6)))
    (net (code 407) (name A9)
      (node (ref U1) (pin 37))
      (node (ref U2) (pin 68))
      (node (ref P1) (pin 32))
      (node (ref U7) (pin 37))
      (node (ref U8) (pin 37))
      (node (ref U6) (pin 41))
      (node (ref RP106) (pin 2)))
    (net (code 408) (name A15)
      (node (ref P1) (pin 43))
      (node (ref U36) (pin 13))
      (node (ref U1) (pin 43))
      (node (ref U6) (pin 35))
      (node (ref RP106) (pin 8))
      (node (ref U2) (pin 74)))
    (net (code 409) (name A17)
      (node (ref U2) (pin 76))
      (node (ref U1) (pin 45))
      (node (ref RP105) (pin 8))
      (node (ref U6) (pin 33))
      (node (ref P1) (pin 47))
      (node (ref U5) (pin 33)))
    (net (code 410) (name A16)
      (node (ref RP106) (pin 9))
      (node (ref U6) (pin 34))
      (node (ref U2) (pin 75))
      (node (ref U1) (pin 44))
      (node (ref P1) (pin 45)))
    (net (code 411) (name A14)
      (node (ref RP106) (pin 7))
      (node (ref P1) (pin 41))
      (node (ref U1) (pin 42))
      (node (ref U6) (pin 36))
      (node (ref U2) (pin 73)))
    (net (code 412) (name A13)
      (node (ref U37) (pin 4))
      (node (ref P1) (pin 39))
      (node (ref RP106) (pin 6))
      (node (ref U1) (pin 41))
      (node (ref U2) (pin 72))
      (node (ref U6) (pin 37)))
    (net (code 413) (name A12)
      (node (ref RP106) (pin 5))
      (node (ref U2) (pin 71))
      (node (ref P1) (pin 38))
      (node (ref U6) (pin 38))
      (node (ref U1) (pin 40))
      (node (ref U37) (pin 1)))
    (net (code 414) (name A11)
      (node (ref U8) (pin 35))
      (node (ref U7) (pin 35))
      (node (ref U6) (pin 39))
      (node (ref RP106) (pin 4))
      (node (ref U2) (pin 70))
      (node (ref U1) (pin 39))
      (node (ref P1) (pin 36)))
    (net (code 415) (name A10)
      (node (ref U6) (pin 40))
      (node (ref U8) (pin 36))
      (node (ref U7) (pin 36))
      (node (ref U1) (pin 38))
      (node (ref P1) (pin 34))
      (node (ref RP106) (pin 3))
      (node (ref U2) (pin 69)))
    (net (code 416) (name A23)
      (node (ref JP2) (pin 1))
      (node (ref RP105) (pin 2))
      (node (ref U5) (pin 39))
      (node (ref P1) (pin 59))
      (node (ref U1) (pin 52)))
    (net (code 417) (name A22)
      (node (ref U1) (pin 51))
      (node (ref U5) (pin 38))
      (node (ref RP105) (pin 3))
      (node (ref P1) (pin 57)))
    (net (code 418) (name "Net-(C2-Pad1)")
      (node (ref E101) (pin 3))
      (node (ref C2) (pin 1))
      (node (ref U2) (pin 15)))
    (net (code 419) (name "Net-(C701-Pad1)")
      (node (ref E110) (pin 3))
      (node (ref X1) (pin 14))
      (node (ref C701) (pin 1)))
    (net (code 420) (name "Net-(CN8-Pad5)")
      (node (ref CN8) (pin 5))
      (node (ref LF1) (pin 3)))
    (net (code 421) (name "Net-(CN8-Pad3)")
      (node (ref CN8) (pin 3))
      (node (ref LF1) (pin 4)))
    (net (code 422) (name "Net-(C800-Pad2)")
      (node (ref C800) (pin 2))
      (node (ref CN8) (pin 1))
      (node (ref LF1) (pin 2)))
    (net (code 423) (name "Net-(C800-Pad1)")
      (node (ref C800) (pin 1))
      (node (ref CN8) (pin 4))
      (node (ref LF1) (pin 1)))
    (net (code 424) (name BDRA3)
      (node (ref U34) (pin 19))
      (node (ref P9) (pin 26))
      (node (ref RP202) (pin 9)))
    (net (code 425) (name BDRA2)
      (node (ref P9) (pin 25))
      (node (ref U34) (pin 9))
      (node (ref RP202) (pin 8)))
    (net (code 426) (name BDRA1)
      (node (ref RP202) (pin 6))
      (node (ref U35) (pin 7))
      (node (ref P9) (pin 24)))
    (net (code 427) (name BDRA8)
      (node (ref U34) (pin 12))
      (node (ref RP202) (pin 2))
      (node (ref P9) (pin 31)))
    (net (code 428) (name /RAM/ma8)
      (node (ref U21) (pin 15))
      (node (ref RP202) (pin 1))
      (node (ref U18) (pin 15))
      (node (ref U22) (pin 15))
      (node (ref U17) (pin 15))
      (node (ref U16) (pin 15))
      (node (ref U20) (pin 15))
      (node (ref U23) (pin 15))
      (node (ref U19) (pin 15)))
    (net (code 429) (name /RAM/ma3)
      (node (ref U19) (pin 9))
      (node (ref U17) (pin 9))
      (node (ref U18) (pin 9))
      (node (ref U22) (pin 9))
      (node (ref U16) (pin 9))
      (node (ref U23) (pin 9))
      (node (ref U20) (pin 9))
      (node (ref U21) (pin 9))
      (node (ref RP202) (pin 10)))
    (net (code 430) (name /RAM/ma2)
      (node (ref U16) (pin 8))
      (node (ref U19) (pin 8))
      (node (ref U23) (pin 8))
      (node (ref U21) (pin 8))
      (node (ref U22) (pin 8))
      (node (ref U18) (pin 8))
      (node (ref U17) (pin 8))
      (node (ref U20) (pin 8))
      (node (ref RP202) (pin 7)))
    (net (code 431) (name /RAM/ma1)
      (node (ref U22) (pin 7))
      (node (ref U17) (pin 7))
      (node (ref U19) (pin 7))
      (node (ref RP202) (pin 5))
      (node (ref U21) (pin 7))
      (node (ref U18) (pin 7))
      (node (ref U16) (pin 7))
      (node (ref U23) (pin 7))
      (node (ref U20) (pin 7)))
    (net (code 432) (name /RAM/ma0)
      (node (ref U20) (pin 6))
      (node (ref U16) (pin 6))
      (node (ref U19) (pin 6))
      (node (ref U18) (pin 6))
      (node (ref RP202) (pin 3))
      (node (ref U17) (pin 6))
      (node (ref U22) (pin 6))
      (node (ref U21) (pin 6))
      (node (ref U23) (pin 6)))
    (net (code 433) (name /RAM/ma4)
      (node (ref U23) (pin 11))
      (node (ref RP201) (pin 10))
      (node (ref U17) (pin 11))
      (node (ref U16) (pin 11))
      (node (ref U19) (pin 11))
      (node (ref U21) (pin 11))
      (node (ref U22) (pin 11))
      (node (ref U20) (pin 11))
      (node (ref U18) (pin 11)))
    (net (code 434) (name /RAM/ma6)
      (node (ref RP201) (pin 5))
      (node (ref U20) (pin 13))
      (node (ref U21) (pin 13))
      (node (ref U16) (pin 13))
      (node (ref U19) (pin 13))
      (node (ref U23) (pin 13))
      (node (ref U17) (pin 13))
      (node (ref U22) (pin 13))
      (node (ref U18) (pin 13)))
    (net (code 435) (name /RAM/ma7)
      (node (ref U21) (pin 14))
      (node (ref U22) (pin 14))
      (node (ref U20) (pin 14))
      (node (ref U17) (pin 14))
      (node (ref U18) (pin 14))
      (node (ref U19) (pin 14))
      (node (ref U16) (pin 14))
      (node (ref U23) (pin 14))
      (node (ref RP201) (pin 3)))
    (net (code 436) (name BDRA0)
      (node (ref RP202) (pin 4))
      (node (ref U35) (pin 9))
      (node (ref P9) (pin 23)))
    (net (code 437) (name "Net-(RP201-Pad2)")
      (node (ref RP201) (pin 2)))
    (net (code 438) (name "Net-(RP201-Pad1)")
      (node (ref RP201) (pin 1)))
    (net (code 439) (name BDRA7)
      (node (ref RP201) (pin 4))
      (node (ref U34) (pin 5))
      (node (ref P9) (pin 30)))
    (net (code 440) (name BDRA6)
      (node (ref RP201) (pin 6))
      (node (ref U34) (pin 15))
      (node (ref P9) (pin 29)))
    (net (code 441) (name BDRA5)
      (node (ref RP201) (pin 7))
      (node (ref U34) (pin 6))
      (node (ref P9) (pin 28)))
    (net (code 442) (name BDRA4)
      (node (ref RP201) (pin 9))
      (node (ref U34) (pin 16))
      (node (ref P9) (pin 27)))
    (net (code 444) (name BDRA9)
      (node (ref U34) (pin 2))
      (node (ref U32) (pin 2))
      (node (ref U32) (pin 14)))
    (net (code 445) (name "Net-(U32-Pad9)")
      (node (ref U32) (pin 9)))
    (net (code 446) (name "Net-(U32-Pad10)")
      (node (ref U32) (pin 10)))
    (net (code 447) (name "Net-(U32-Pad7)")
      (node (ref U32) (pin 7)))
    (net (code 448) (name "Net-(U32-Pad6)")
      (node (ref U32) (pin 6)))
    (net (code 449) (name "Net-(JP3A1-Pad2)")
      (node (ref U35) (pin 16))
      (node (ref JP3A1) (pin 2)))
    (net (code 450) (name "Net-(JP3B1-Pad1)")
      (node (ref U35) (pin 18))
      (node (ref JP3B1) (pin 1)))
    (net (code 451) (name /RAM/~bcasu0)
      (node (ref JP4B1) (pin 1))
      (node (ref U32) (pin 12))
      (node (ref RP203) (pin 5)))
    (net (code 452) (name "Net-(JP4B1-Pad2)")
      (node (ref U35) (pin 12))
      (node (ref JP4B1) (pin 2)))
    (net (code 453) (name "Net-(U32-Pad1)")
      (node (ref U32) (pin 15))
      (node (ref U35) (pin 5))
      (node (ref U32) (pin 1))
      (node (ref U34) (pin 11)))
    (net (code 454) (name DRD2)
      (node (ref U20) (pin 19))
      (node (ref U16) (pin 19))
      (node (ref U2) (pin 12))
      (node (ref U4) (pin 5))
      (node (ref U10) (pin 14))
      (node (ref P9) (pin 7))
      (node (ref U11) (pin 7))
      (node (ref RP111) (pin 3))
      (node (ref U3) (pin 7)))
    (net (code 455) (name DRD0)
      (node (ref U11) (pin 3))
      (node (ref U4) (pin 7))
      (node (ref U3) (pin 10))
      (node (ref P9) (pin 5))
      (node (ref U10) (pin 18))
      (node (ref U20) (pin 18))
      (node (ref U2) (pin 14))
      (node (ref RP111) (pin 2))
      (node (ref U16) (pin 18)))
    (net (code 456) (name DRD1)
      (node (ref U11) (pin 4))
      (node (ref U20) (pin 2))
      (node (ref U3) (pin 9))
      (node (ref U2) (pin 13))
      (node (ref U16) (pin 2))
      (node (ref U4) (pin 6))
      (node (ref U10) (pin 16))
      (node (ref P9) (pin 6))
      (node (ref RP109) (pin 2)))
    (net (code 457) (name DRD3)
      (node (ref RP109) (pin 3))
      (node (ref U2) (pin 11))
      (node (ref U3) (pin 6))
      (node (ref U11) (pin 8))
      (node (ref P9) (pin 8))
      (node (ref U4) (pin 4))
      (node (ref U16) (pin 1))
      (node (ref U10) (pin 12))
      (node (ref U20) (pin 1)))
    (net (code 458) (name DRA0)
      (node (ref U35) (pin 11))
      (node (ref U2) (pin 42)))
    (net (code 459) (name DRA1)
      (node (ref U35) (pin 13))
      (node (ref U2) (pin 43)))
    (net (code 460) (name DRA3)
      (node (ref U2) (pin 45))
      (node (ref U34) (pin 18)))
    (net (code 461) (name DRA7)
      (node (ref U2) (pin 49))
      (node (ref U34) (pin 4)))
    (net (code 462) (name DRA9)
      (node (ref U2) (pin 55))
      (node (ref U34) (pin 3)))
    (net (code 463) (name DRA5)
      (node (ref U34) (pin 7))
      (node (ref U2) (pin 47)))
    (net (code 464) (name DRA2)
      (node (ref U34) (pin 8))
      (node (ref U2) (pin 44)))
    (net (code 465) (name DRA8)
      (node (ref U34) (pin 13))
      (node (ref U2) (pin 50)))
    (net (code 466) (name DRA6)
      (node (ref U34) (pin 14))
      (node (ref U2) (pin 48)))
    (net (code 467) (name DRA4)
      (node (ref U2) (pin 46))
      (node (ref U34) (pin 17)))
    (net (code 468) (name DRD13)
      (node (ref U2) (pin 1))
      (node (ref U19) (pin 2))
      (node (ref U4) (pin 42))
      (node (ref U3) (pin 44))
      (node (ref RP109) (pin 8))
      (node (ref U23) (pin 2))
      (node (ref U13) (pin 14))
      (node (ref U12) (pin 7))
      (node (ref P9) (pin 18)))
    (net (code 472) (name DRD14)
      (node (ref U13) (pin 17))
      (node (ref U3) (pin 43))
      (node (ref U12) (pin 5))
      (node (ref U2) (pin 84))
      (node (ref U19) (pin 19))
      (node (ref U4) (pin 41))
      (node (ref U23) (pin 19))
      (node (ref RP111) (pin 9))
      (node (ref P9) (pin 19)))
    (net (code 473) (name DRD12)
      (node (ref U19) (pin 18))
      (node (ref U12) (pin 9))
      (node (ref U13) (pin 13))
      (node (ref U4) (pin 43))
      (node (ref U23) (pin 18))
      (node (ref RP111) (pin 8))
      (node (ref P9) (pin 17))
      (node (ref U3) (pin 45))
      (node (ref U2) (pin 2)))
    (net (code 474) (name DRD15)
      (node (ref U4) (pin 40))
      (node (ref U2) (pin 83))
      (node (ref U3) (pin 42))
      (node (ref P9) (pin 20))
      (node (ref U12) (pin 3))
      (node (ref U19) (pin 1))
      (node (ref U13) (pin 18))
      (node (ref RP109) (pin 9))
      (node (ref U23) (pin 1)))
    (net (code 475) (name DRD10)
      (node (ref U4) (pin 45))
      (node (ref U18) (pin 19))
      (node (ref P9) (pin 15))
      (node (ref U13) (pin 7))
      (node (ref U2) (pin 4))
      (node (ref U22) (pin 19))
      (node (ref U12) (pin 14))
      (node (ref U3) (pin 47))
      (node (ref RP111) (pin 7)))
    (net (code 476) (name DRD8)
      (node (ref U13) (pin 3))
      (node (ref U18) (pin 18))
      (node (ref RP111) (pin 6))
      (node (ref P9) (pin 13))
      (node (ref U22) (pin 18))
      (node (ref U3) (pin 1))
      (node (ref U2) (pin 6))
      (node (ref U4) (pin 47))
      (node (ref U12) (pin 18)))
    (net (code 477) (name DRD4)
      (node (ref U2) (pin 10))
      (node (ref U11) (pin 13))
      (node (ref U21) (pin 18))
      (node (ref RP111) (pin 4))
      (node (ref U10) (pin 9))
      (node (ref U17) (pin 18))
      (node (ref P9) (pin 9))
      (node (ref U3) (pin 5))
      (node (ref U4) (pin 3)))
    (net (code 478) (name DRD5)
      (node (ref U17) (pin 2))
      (node (ref P9) (pin 10))
      (node (ref RP109) (pin 4))
      (node (ref U2) (pin 9))
      (node (ref U4) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref U10) (pin 7))
      (node (ref U21) (pin 2))
      (node (ref U11) (pin 14)))
    (net (code 479) (name DRD7)
      (node (ref U17) (pin 1))
      (node (ref U11) (pin 18))
      (node (ref U10) (pin 3))
      (node (ref P9) (pin 12))
      (node (ref U4) (pin 48))
      (node (ref RP109) (pin 5))
      (node (ref U3) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref U21) (pin 1)))
    (net (code 480) (name DRD6)
      (node (ref U3) (pin 3))
      (node (ref U4) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref U11) (pin 17))
      (node (ref U10) (pin 5))
      (node (ref U17) (pin 19))
      (node (ref P9) (pin 11))
      (node (ref U21) (pin 19))
      (node (ref RP111) (pin 5)))
    (net (code 482) (name DRD9)
      (node (ref U22) (pin 2))
      (node (ref RP109) (pin 6))
      (node (ref U4) (pin 46))
      (node (ref U18) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref U12) (pin 16))
      (node (ref U13) (pin 4))
      (node (ref P9) (pin 14))
      (node (ref U3) (pin 48)))
    (net (code 483) (name DRD11)
      (node (ref U13) (pin 8))
      (node (ref U2) (pin 3))
      (node (ref RP109) (pin 7))
      (node (ref U12) (pin 12))
      (node (ref P9) (pin 16))
      (node (ref U3) (pin 46))
      (node (ref U4) (pin 44))
      (node (ref U18) (pin 1))
      (node (ref U22) (pin 1)))
    (net (code 486) (name "Net-(R201-Pad2)")
      (node (ref U21) (pin 5))
      (node (ref U22) (pin 5))
      (node (ref U16) (pin 5))
      (node (ref U20) (pin 5))
      (node (ref R201) (pin 2))
      (node (ref U17) (pin 4))
      (node (ref U16) (pin 4))
      (node (ref U17) (pin 5))
      (node (ref U18) (pin 5))
      (node (ref U18) (pin 4))
      (node (ref RP203) (pin 2))
      (node (ref U19) (pin 4))
      (node (ref U19) (pin 5))
      (node (ref U23) (pin 5)))
    (net (code 487) (name "Net-(RP203-Pad8)")
      (node (ref U21) (pin 17))
      (node (ref RP203) (pin 8))
      (node (ref U17) (pin 17))
      (node (ref U20) (pin 17))
      (node (ref U16) (pin 17)))
    (net (code 488) (name /RAM/ma5)
      (node (ref U21) (pin 12))
      (node (ref RP201) (pin 8))
      (node (ref U19) (pin 12))
      (node (ref U23) (pin 12))
      (node (ref U16) (pin 12))
      (node (ref U20) (pin 12))
      (node (ref U22) (pin 12))
      (node (ref U18) (pin 12))
      (node (ref U17) (pin 12)))
    (net (code 489) (name /RAM/~bcasl0)
      (node (ref RP203) (pin 7))
      (node (ref JP4A1) (pin 1))
      (node (ref U32) (pin 4)))
    (net (code 490) (name "Net-(RP203-Pad6)")
      (node (ref RP203) (pin 6))
      (node (ref U18) (pin 17))
      (node (ref U22) (pin 17))
      (node (ref U19) (pin 17))
      (node (ref U23) (pin 17)))
    (net (code 491) (name "Net-(JP4A1-Pad2)")
      (node (ref JP4A1) (pin 2))
      (node (ref U35) (pin 14)))
    (net (code 495) (name "Net-(RP203-Pad10)")
      (node (ref U19) (pin 3))
      (node (ref RP203) (pin 10))
      (node (ref U17) (pin 3))
      (node (ref U18) (pin 3))
      (node (ref U22) (pin 3))
      (node (ref U21) (pin 3))
      (node (ref U16) (pin 3))
      (node (ref U23) (pin 3))
      (node (ref U20) (pin 3)))
    (net (code 496) (name "Net-(R202-Pad2)")
      (node (ref U22) (pin 4))
      (node (ref U21) (pin 4))
      (node (ref RP203) (pin 4))
      (node (ref U23) (pin 4))
      (node (ref R202) (pin 2))
      (node (ref U20) (pin 4)))
    (net (code 501) (name "Net-(CN5-Pad13)")
      (node (ref E617) (pin 3))
      (node (ref CN5) (pin 13)))
    (net (code 502) (name "Net-(CN5-Pad2)")
      (node (ref E612) (pin 3))
      (node (ref CN5) (pin 2)))
    (net (code 503) (name "Net-(CN5-Pad1)")
      (node (ref E611) (pin 3))
      (node (ref CN5) (pin 1)))
    (net (code 504) (name "Net-(CN5-Pad18)")
      (node (ref CN5) (pin 18))
      (node (ref E622) (pin 3)))
    (net (code 505) (name ~DKWEB)
      (node (ref E620) (pin 1))
      (node (ref CN11) (pin 24))
      (node (ref U36) (pin 8)))
    (net (code 506) (name "Net-(CN5-Pad17)")
      (node (ref E621) (pin 3))
      (node (ref CN5) (pin 17)))
    (net (code 507) (name "Net-(CN5-Pad16)")
      (node (ref CN5) (pin 16))
      (node (ref E620) (pin 3)))
    (net (code 508) (name "Net-(CN5-Pad14)")
      (node (ref CN5) (pin 14))
      (node (ref E618) (pin 3)))
    (net (code 509) (name "Net-(CN5-Pad15)")
      (node (ref E619) (pin 3))
      (node (ref CN5) (pin 15)))
    (net (code 510) (name "Net-(CN5-Pad11)")
      (node (ref E616) (pin 3))
      (node (ref CN5) (pin 11)))
    (net (code 511) (name "Net-(CN5-Pad9)")
      (node (ref CN5) (pin 9))
      (node (ref E614) (pin 3)))
    (net (code 512) (name ~MTRX)
      (node (ref U36) (pin 2))
      (node (ref E613) (pin 1)))
    (net (code 513) (name ~DKWDB)
      (node (ref E621) (pin 1))
      (node (ref CN11) (pin 22))
      (node (ref U36) (pin 6)))
    (net (code 514) (name "Net-(CN5-Pad23)")
      (node (ref E602) (pin 3))
      (node (ref CN5) (pin 23)))
    (net (code 515) (name "Net-(CN5-Pad22)")
      (node (ref CN5) (pin 22))
      (node (ref E626) (pin 3)))
    (net (code 516) (name "Net-(CN5-Pad21)")
      (node (ref E625) (pin 3))
      (node (ref CN5) (pin 21)))
    (net (code 517) (name "Net-(CN5-Pad20)")
      (node (ref CN5) (pin 20))
      (node (ref E624) (pin 3)))
    (net (code 518) (name "Net-(CN5-Pad19)")
      (node (ref CN5) (pin 19))
      (node (ref E623) (pin 3)))
    (net (code 519) (name "Net-(CN11-Pad3)")
      (node (ref CN11) (pin 3)))
    (net (code 520) (name "Net-(CN11-Pad14)")
      (node (ref CN11) (pin 14)))
    (net (code 521) (name "Net-(CN11-Pad6)")
      (node (ref CN11) (pin 6)))
    (net (code 522) (name "Net-(U36-Pad3)")
      (node (ref U36) (pin 3))
      (node (ref U5) (pin 46)))
    (net (code 523) (name "Net-(U36-Pad5)")
      (node (ref U36) (pin 5))
      (node (ref U5) (pin 45)))
    (net (code 524) (name "Net-(U36-Pad1)")
      (node (ref U36) (pin 1))
      (node (ref U5) (pin 47)))
    (net (code 525) (name "Net-(U36-Pad9)")
      (node (ref U5) (pin 44))
      (node (ref U36) (pin 9)))
    (net (code 526) (name "Net-(CN5-Pad12)")
      (node (ref E601) (pin 3))
      (node (ref CN5) (pin 12)))
    (net (code 527) (name "Net-(CN5-Pad8)")
      (node (ref E613) (pin 3))
      (node (ref CN5) (pin 8)))
    (net (code 528) (name "Net-(CN5-Pad10)")
      (node (ref E615) (pin 3))
      (node (ref CN5) (pin 10)))))