[platformio]
default_envs = dev

[env:dev]
platform = espressif8266
board = esp12e
framework = ${common.framework}
lib_deps = ${common.lib_deps}
build_flags =
    -D DEBUG_MODE=1
extra_scripts =
    pre:scripts/addversion.py
    scripts/makeweb.py
monitor_speed = 115200 ; If serial port is shared with HAN, use 2400 and parity E (or N for Norwegian Kamstrup)
monitor_flags = 
    --parity
    N
