       1                                ;;;;
       2                                ;
       3                                ; Test that .ENABL AMA  doesn't survive to the next pass.
       4                                ; The default at the start of each pass is set by the command line
       5                                ; option -d AMA or -e AMA. It is disabled by default.
       6                                
       7 000000                         	.psect	foo,i,rw
       8 000000 000000                  y:	.word	0
       9 000002 005067  177772          	clr	y	; should be pc-relative, no relocation
      10                                
      11                                	.enabl ama	; after this, Y would be @#Y
      11                                


Symbol table

.       000006R      002 Y       000000R      002 


Program sections:

. ABS.  000000    000   (RW,I,GBL,ABS,OVR,NOSAV)
        000000    001   (RW,I,LCL,REL,CON,NOSAV)
FOO     000006    002   (RW,I,LCL,REL,CON,NOSAV)
