TR1101 Instructions [written on inside of box lid]

Enter Unit Z[?] by keyboard         Restart 0030

Execute 10000 04 0000 with A Sgn = 1

Before read in:

    Cell 0001   5000
            2   Card units
            3   TSU's
            4   1 in A-1
            5   0
            6   0

Prg Switches - 6 [7 crossed out]

               5 6 7 & 9 (locks up on Sect 3)

_____________

Program switch use (deduced from behavior):

1   Lock up execution on current test

4   Skips initial positioning of mag tape drives

5   Skips printing test name on SPO

