# Example ICL file for 32/7x
# this line ignored
*DEV04=0E150400,02		Cartridge disc with two platters
*DEV08=0E160800,04		Moving head disc
*DEV10=0E181000,04		9-Track magnetic tape
*DEV20=0E1A2000,10		GPMC with 16 terminals
*DEV60=0E1E6000,08		ADS
*DEV78=01207800			Primary card reader
*DEV7A=00217802			Primary line printer
*DEV7E=02237801			Primary Teletype
*INT00=1F				Power fail/Auto restart
*INT01=1E				System Overide
*INT12=1D				Memory parity
*INT13=1C				Console Interrupt
*INT24=1B				Nonpresent memory
*INT25=1A				Undefined instruction trap
*INT26=19				Privlege violation
*INT27=18				Call Monitor
*INT28=16				Real-time clock
*INT29=17				Arithmetic exception
*INT2A=15				External interrupt
*INT2B=14				External interrupt
*INT2C=13				External interrupt
*INT2D=12				External interrupt
*END
