(export (version D)
  (design
    (source /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/nubus-to-ztex.sch)
    (date "Thu Jan 20 09:40:26 2022")
    (tool "Eeschema 5.0.2+dfsg1-1~bpo9+1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source nubus-to-ztex.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /B2B/) (tstamps /618E8C75/)
      (title_block
        (title "nubus-to-ztex B2B connector")
        (company)
        (rev)
        (date)
        (source B2B.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /nubus/) (tstamps /618F532C/)
      (title_block
        (title "nubus-to-ztex NuBus connection & level shifting")
        (company)
        (rev)
        (date)
        (source nubus.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /hdmi/) (tstamps /61B62C00/)
      (title_block
        (title "nubus-to-ztex HDMI")
        (company)
        (rev)
        (date)
        (source hdmi.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /usb/) (tstamps /61B604DE/)
      (title_block
        (title "nubus-to-ztex USB")
        (company)
        (rev)
        (date)
        (source usb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /fan/) (tstamps /61B99D2C/)
      (title_block
        (title "nubus-to-ztex extra conenctors (fan, ...)")
        (company)
        (rev)
        (date)
        (source fan.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /vga/) (tstamps /6193AB43/)
      (title_block
        (title "nubus-to-ztex VGA")
        (company)
        (rev)
        (date)
        (source vga.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref JAB1)
      (value ZTEX_AB-ztex_AB)
      (footprint For_SeeedStudio:PinHeader_2x32_P2.54mm_Vertical_For_SeeedStudio)
      (fields
        (field (name MPN) 10-89-7642)
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/10-89-7642?qs=%2Fha2pyFadugCxzQFZUdvioDcljDVidgd4vXrOFuSRYM%3D))
      (libsource (lib ztex_AB) (part ZTEX_AB) (description ""))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 5F676E85))
    (comp (ref J3)
      (value Conn_01x06_Male)
      (footprint For_SeeedStudio:PinHeader_1x06_P2.54mm_Horizontal_For_SeeedStudio)
      (datasheet ~)
      (fields
        (field (name MPN) PZ254R-11-06P)
        (field (name MPN-ALT) 22-28-8060)
        (field (name URL) https://lcsc.com/product-detail/Pin-Header-Female-Header_XFCN-PZ254R-11-06P_C492414.html)
        (field (name URL-ALT) https://www2.mouser.com/ProductDetail/Molex/22-28-8060?qs=4XSMV6Twtb2rYD%2F%2F316gfQ==))
      (libsource (lib Connector) (part Conn_01x06_Male) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 5F69129B))
    (comp (ref JCD1)
      (value ZTEX_CD-ztex_CD)
      (footprint For_SeeedStudio:PinHeader_2x32_P2.54mm_Vertical_For_SeeedStudio)
      (fields
        (field (name MPN) 10-89-7642)
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/10-89-7642?qs=%2Fha2pyFadugCxzQFZUdvioDcljDVidgd4vXrOFuSRYM%3D))
      (libsource (lib ztex_CD) (part ZTEX_CD) (description ""))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 5F676F65))
    (comp (ref J1)
      (value Conn_02x07_Odd_Even)
      (footprint For_SeeedStudio:PinHeader_2x07_P2.00mm_Vertical_For_SeeedStudio)
      (datasheet https://www.molex.com/pdm_docs/sd/878331420_sd.pdf)
      (fields
        (field (name Datasheet-ALT) https://datasheet.lcsc.com/lcsc/1811051309_MOLEX-878311420_C240854.pdf)
        (field (name MPN) 87831-1420)
        (field (name "MPN Right Angle") 87833-1420)
        (field (name "MPN-ALT Right Angle") A2005WR-N-2X7P-B)
        (field (name Notes) "87831-1419, 87831-1420, 87831-1421, 87831-1436 only change plating")
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/87831-1420?qs=QtQX4uD3c2VDCL534TqpVg%3D%3D)
        (field (name "URL Rihgt Angle") https://www2.mouser.com/ProductDetail/Molex/87833-1420?qs=%2Fha2pyFadujYFYCIYI1IvFCvLi7no9WQYzIL%2FpYxKhg%3D))
      (libsource (lib Connector_Generic) (part Conn_02x07_Odd_Even) (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 5F749BE1))
    (comp (ref R1)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61B5DFBC))
    (comp (ref D1)
      (value RED)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://optoelectronics.liteon.com/upload/download/DS-22-99-0150/LTST-C170KRKT.pdf)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KRKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KRKT_C94868.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61B5DFCC))
    (comp (ref R2)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61B5F3F5))
    (comp (ref D2)
      (value RED)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://optoelectronics.liteon.com/upload/download/DS-22-99-0150/LTST-C170KRKT.pdf)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KRKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KRKT_C94868.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61B5F405))
    (comp (ref C1)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB104_C92490.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61B7E3FB))
    (comp (ref J2)
      (value Conn_02x07_Odd_Even)
      (footprint For_SeeedStudio:PinHeader_2x07_P2.00mm_Vertical_For_SeeedStudio)
      (datasheet https://www.molex.com/pdm_docs/sd/878331420_sd.pdf)
      (fields
        (field (name MPN) 87831-1420)
        (field (name "MPN Right Angle") 87833-1420)
        (field (name "MPN-ALT Right Angle") A2005WR-N-2X7P-B)
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/87831-1420?qs=QtQX4uD3c2VDCL534TqpVg%3D%3D)
        (field (name "URL Rihgt Angle") https://www2.mouser.com/ProductDetail/Molex/87833-1420?qs=%2Fha2pyFadujYFYCIYI1IvFCvLi7no9WQYzIL%2FpYxKhg%3D))
      (libsource (lib Connector_Generic) (part Conn_02x07_Odd_Even) (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61CD2AB9))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 61F08531))
    (comp (ref R3)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 621E3C4D))
    (comp (ref D3)
      (value BLUE)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://eu.mouser.com/datasheet/2/239/Lite-On-LTST-C170TBKT-1175372.pdf)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170TBKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_LTST-C170TBKT-blue_C98222.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 621E3C57))
    (comp (ref C3)
      (value "47uF 10V+")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (fields
        (field (name MPN) C2012X5R1A476MTJ00E)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_TDK-C2012X5R1A476MTJ00E_C76636.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /B2B/) (tstamps /618E8C75/))
      (tstamp 621FCA7B))
    (comp (ref C19)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 5F8CA5C6))
    (comp (ref R4)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 5F93CF72))
    (comp (ref J4)
      (value C96ABC)
      (footprint For_SeeedStudio:DIN41612_C_3x32_Male_Horizontal_THT)
      (datasheet " ~")
      (fields
        (field (name MPN) 85003-0567)
        (field (name "MPN (3M)") DIN-096CPC-RR1-HM)
        (field (name "MPN (Harting 2)") 09033966921)
        (field (name "MPN (Harting)") 09033967921)
        (field (name "Notes (3M)") "RR1L would also work (for .062 PCBs)")
        (field (name URL) https://www.mouser.fr/ProductDetail/Molex/85003-0567?qs=U4pz39agNJB6P1oBpJ4bJA%3D%3D))
      (libsource (lib C96ABC) (part C96ABC_NUBUS) (description ""))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61912527))
    (comp (ref R7)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61AF5DD2))
    (comp (ref R5)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61AF6878))
    (comp (ref R6)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61AF68D0))
    (comp (ref C7)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61B12074))
    (comp (ref U8)
      (value 74LVT245BPW,118)
      (footprint For_SeeedStudio:TSSOP-20_4.4x6.5mm_P0.65mm_ForSeeedStudio)
      (datasheet http://www.ti.com/lit/gpn/sn74LS245)
      (fields
        (field (name MPN) 74LVT245BPW,118)
        (field (name URL) https://eu.mouser.com/ProductDetail/?qs=me8TqzrmIYVnC5%252BK4SaiTg%3D%3D))
      (libsource (lib 74xx) (part 74LS245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BC9B90))
    (comp (ref C18)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BCFF40))
    (comp (ref U7)
      (value 74LVT245BPW,118)
      (footprint For_SeeedStudio:TSSOP-20_4.4x6.5mm_P0.65mm_ForSeeedStudio)
      (datasheet http://www.ti.com/lit/gpn/sn74LS245)
      (fields
        (field (name MPN) 74LVT245BPW,118)
        (field (name URL) https://eu.mouser.com/ProductDetail/?qs=me8TqzrmIYVnC5%252BK4SaiTg%3D%3D))
      (libsource (lib 74xx) (part 74LS245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BCFF5A))
    (comp (ref C17)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BD1EF4))
    (comp (ref U6)
      (value 74LVT245BPW,118)
      (footprint For_SeeedStudio:TSSOP-20_4.4x6.5mm_P0.65mm_ForSeeedStudio)
      (datasheet http://www.ti.com/lit/gpn/sn74LS245)
      (fields
        (field (name MPN) 74LVT245BPW,118)
        (field (name URL) https://eu.mouser.com/ProductDetail/?qs=me8TqzrmIYVnC5%252BK4SaiTg%3D%3D))
      (libsource (lib 74xx) (part 74LS245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BD1F0E))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BD1F21))
    (comp (ref U5)
      (value 74LVT245BPW,118)
      (footprint For_SeeedStudio:TSSOP-20_4.4x6.5mm_P0.65mm_ForSeeedStudio)
      (datasheet http://www.ti.com/lit/gpn/sn74LS245)
      (fields
        (field (name "Datasheet - Packaging") https://www.renesas.com/document/psc/pcpcg-package-outline-150-body-width-qsop-025-pitch?language=en)
        (field (name Drawings) https://www.renesas.com/us/en/package/pcg20)
        (field (name MPN) 74LVT245BPW,118)
        (field (name "Package Drawings") https://assets.nexperia.com/documents/package-information/SOT360-1.pdf)
        (field (name URL) https://eu.mouser.com/ProductDetail/?qs=me8TqzrmIYVnC5%252BK4SaiTg%3D%3D))
      (libsource (lib 74xx) (part 74LS245) (description "Octal BUS Transceivers, 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BD1F3B))
    (comp (ref C8)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BFF690))
    (comp (ref C9)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB104_C92490.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61CBFFB1))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61CC2A0D))
    (comp (ref C11)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61CC44CF))
    (comp (ref C12)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61BC6E4B))
    (comp (ref R16)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85DF0))
    (comp (ref D11)
      (value GREEN)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KGKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85DFA))
    (comp (ref R17)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85E0D))
    (comp (ref D12)
      (value GREEN)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KGKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85E17))
    (comp (ref R18)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85E2A))
    (comp (ref D13)
      (value GREEN)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KGKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85E34))
    (comp (ref R19)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85E47))
    (comp (ref D14)
      (value GREEN)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KGKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KGKT_C98221.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61D85E51))
    (comp (ref R11)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DA4E68))
    (comp (ref D6)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DA4E72))
    (comp (ref R12)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DA5DAA))
    (comp (ref D7)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DA5DB4))
    (comp (ref R13)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DABC59))
    (comp (ref D8)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DABC63))
    (comp (ref R14)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DB5BFB))
    (comp (ref D9)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DB5C05))
    (comp (ref R20)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DC5CFD))
    (comp (ref D15)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DC5D07))
    (comp (ref R21)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DC5D18))
    (comp (ref D16)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DC5D22))
    (comp (ref R9)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DE9DA5))
    (comp (ref D4)
      (value ORANGE)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KFKT_C284931.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KFKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KFKT_C284931.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DE9DAF))
    (comp (ref R10)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DEBB52))
    (comp (ref D5)
      (value ORANGE)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KFKT_C284931.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KFKT)
        (field (name URL) https://www.lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KFKT_C284931.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61DEBB5C))
    (comp (ref C13)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB105)
        (field (name Mouser) 603-CC603KRX7R8BB105)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB105_C106858.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61E28221))
    (comp (ref C15)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61E88C18))
    (comp (ref C16)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61E88C28))
    (comp (ref R8)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61AF68A2))
    (comp (ref U3)
      (value 74LVT125)
      (footprint Package_SO:TSSOP-14_4.4x5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LVT125)
      (fields
        (field (name MPN) 74LVT125PW,118)
        (field (name "Package Drawings") https://assets.nexperia.com/documents/package-information/SOT402-1.pdf)
        (field (name URL) https://eu.mouser.com/ProductDetail/Nexperia/74LVT125PW118?qs=me8TqzrmIYWdhdg6%252BsGGHw%3D%3D))
      (libsource (lib 74xx) (part 74LVC125) (description "Quad buffer 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61F62FDB))
    (comp (ref C6)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61F85FB5))
    (comp (ref U1)
      (value 74LVT125)
      (footprint Package_SO:TSSOP-14_4.4x5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LVT125)
      (fields
        (field (name MPN) 74LVT125PW,118)
        (field (name URL) https://eu.mouser.com/ProductDetail/Nexperia/74LVT125PW118?qs=me8TqzrmIYWdhdg6%252BsGGHw%3D%3D))
      (libsource (lib 74xx) (part 74LVC125) (description "Quad buffer 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61F9D997))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61FA599B))
    (comp (ref R15)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5490T5E_C23079.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 62006A45))
    (comp (ref D10)
      (value YELLOW)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html)
      (fields
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KSKT)
        (field (name URL) https://lcsc.com/product-detail/Light-Emitting-Diodes-LED_Lite-On-LTST-C170KSKT_C125091.html))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 62006A4F))
    (comp (ref U4)
      (value XC9572XL-VQ64)
      (footprint For_SeeedStudio:TQFP-64_10x10mm_P0.5mm_Xlinx)
      (datasheet http://www.xilinx.com/support/documentation/data_sheets/ds057.pdf)
      (fields
        (field (name Drawings) https://www.xilinx.com/support/documentation/package_specs/vq64.pdf)
        (field (name MPN) XC9572XL-5VQ64C)
        (field (name URL) https://eu.mouser.com/ProductDetail/Xilinx/XC9572XL-5VQ64C?qs=rrS6PyfT74eW60XLpVlI8A%3D%3D))
      (libsource (lib CPLD_Xilinx) (part XC9572XL-VQ64) (description "CPLD, 72 Macrocells, 1600 Usable Gates"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 61E36DA9))
    (comp (ref U2)
      (value 74LVT125)
      (footprint Package_SO:TSSOP-14_4.4x5mm_P0.65mm)
      (datasheet http://www.ti.com/lit/gpn/sn74LVT125)
      (fields
        (field (name MPN) 74LVT125PW,118)
        (field (name URL) https://eu.mouser.com/ProductDetail/Nexperia/74LVT125PW118?qs=me8TqzrmIYWdhdg6%252BsGGHw%3D%3D))
      (libsource (lib 74xx) (part 74LVC125) (description "Quad buffer 3-State outputs"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621875DB))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 6218760B))
    (comp (ref R36)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621BDDCB))
    (comp (ref R37)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621C4817))
    (comp (ref R38)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621C7B16))
    (comp (ref R39)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621CAE13))
    (comp (ref R40)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621CE10E))
    (comp (ref R41)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621D1407))
    (comp (ref R42)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621D4704))
    (comp (ref R43)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621D7A01))
    (comp (ref R44)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621DAD00))
    (comp (ref R45)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /nubus/) (tstamps /618F532C/))
      (tstamp 621DDFFF))
    (comp (ref U9)
      (value TPD12S016PWR)
      (footprint For_SeeedStudio:SOP65P640X120-24N)
      (fields
        (field (name MANUFACTURER) "Texas Instruments")
        (field (name MAXIMUM_PACKAGE_HEIGHT) "1.2 mm")
        (field (name MPN) TPD12S016PWR)
        (field (name PARTREV) F)
        (field (name STANDARD) "IPC 7351B")
        (field (name URL) https://lcsc.com/product-detail/Interface-Specialized_Texas-Instruments-TPD12S016PWR_C201665.html))
      (libsource (lib TPD12S016PWR) (part TPD12S016PWR) (description ""))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 6148D344))
    (comp (ref C24)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 6148D345))
    (comp (ref C22)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB104_C92490.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 6148D349))
    (comp (ref C23)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 6148D34B))
    (comp (ref J5)
      (value HDMI_A)
      (footprint For_SeeedStudio:HDMI_A_Amphenol_10029449-111)
      (datasheet https://en.wikipedia.org/wiki/HDMI)
      (fields
        (field (name MPN) 10029449-111)
        (field (name URL) https://www2.mouser.com/ProductDetail/Amphenol-FCI/10029449-111RLF?qs=fmpTyLOWOey0HPdD9%2F%2FaXA%3D%3D))
      (libsource (lib Connector) (part HDMI_A) (description "HDMI type A connector"))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 6148D34C))
    (comp (ref C21)
      (value "47uF 10V+")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (fields
        (field (name MPN) C2012X5R1A476MTJ00E)
        (field (name MPN-ALT) "CC0805MRX5R5BB476 # obsolete")
        (field (name MPN-ALT2) "GRM21BR60J476ME15L # 6V3 # delay")
        (field (name MPN-ALT3) "GRM21BR61A476ME15L # 10V")
        (field (name MPN-PREV) GRM21BR60J476ME01L)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_TDK-C2012X5R1A476MTJ00E_C76636.html)
        (field (name URL-ALT2) https://www2.mouser.com/ProductDetail/Murata/GRM21BR60J476ME15L?qs=Tw3AuTVwGeLlkNhaDtjM1w%3D%3D)
        (field (name URL-PREV) https://www2.mouser.com/ProductDetail/?qs=u16ybLDytRYYQtTToF3RWA%3D%3D))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 6148D34D))
    (comp (ref C20)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /hdmi/) (tstamps /61B62C00/))
      (tstamp 61B9B186))
    (comp (ref J6)
      (value "USB micro-B")
      (footprint Connector_USB:USB_Micro-B_Molex-105017-0001)
      (datasheet https://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
      (fields
        (field (name MPN) 105017-0001)
        (field (name Manufacturer) Molex)
        (field (name URL) https://lcsc.com/product-detail/USB-Connectors_MOLEX-1050170001_C136000.html)
        (field (name URL-ALT) https://www.mouser.fr/ProductDetail/Molex/105017-0001?qs=hlXxxvYE36k7QcsR97GUKA%3D%3D))
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A6A3))
    (comp (ref R27)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF1002T5E_C25804.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A6C2))
    (comp (ref R26)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF1002T5E_C25804.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A6CD))
    (comp (ref C26)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A6E1))
    (comp (ref U10)
      (value SN65220)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet http://www.ti.com/lit/ds/symlink/sn65220.pdf)
      (fields
        (field (name MPN) SN65220DBVR)
        (field (name URL) https://lcsc.com/product-detail/TVS_Texas-Instruments-SN65220DBVR_C21787.html)
        (field (name URL-ALT) https://www2.mouser.com/ProductDetail/Texas-Instruments/SN65220DBVR?qs=5nGYs9Do7G0gEpYxbYqyeA%3D%3D))
      (libsource (lib Power_Protection) (part SN65220) (description "USB port transient suppressors"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A6FD))
    (comp (ref R24)
      (value 15k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1502T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF1502T5E_C22809.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A70F))
    (comp (ref R25)
      (value 15k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1502T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF1502T5E_C22809.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A717))
    (comp (ref R22)
      (value 27)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF270JT5E)
        (field (name MPN-ALT) ERJ-3EKF27R0V)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF270JT5E_C25190.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A72D))
    (comp (ref R23)
      (value 27)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF270JT5E)
        (field (name MPN-ALT) ERJ-3EKF27R0V)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF270JT5E_C25190.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A735))
    (comp (ref C25)
      (value 150uF)
      (footprint Capacitor_SMD:C_1206_3216Metric)
      (datasheet ~)
      (fields
        (field (name MPN) GRM31CR60J157ME11L)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_Murata-Electronics-GRM31CR60J157ME11L_C528968.html)
        (field (name "URL (mouser)") https://www.mouser.fr/ProductDetail/Murata-Electronics/GRM31CR60J157ME11L?qs=qSv5qXjCIG3a12X8fU8miQ%3D%3D))
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A750))
    (comp (ref FB1)
      (value Ferrite_Bead_Small)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name MPN) PZ2012U221-2R0TF)
        (field (name MPN-ALT) 742792022)
        (field (name URL) https://lcsc.com/product-detail/Ferrite-Beads_Sunlord-PZ2012U221-2R0TF_C44361.html))
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A758))
    (comp (ref C27)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 612D3A06))
    (comp (ref U11)
      (value TPS2051C)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (fields
        (field (name MPN) TPS2051CDBVR)
        (field (name "Mouser No") 595-TPS2051CDBVR)
        (field (name URL) https://lcsc.com/product-detail/Power-Distribution-Switches_Texas-Instruments-TPS2051CDBVR_C129581.html)
        (field (name "URL (Mouser)") https://www.mouser.fr/ProductDetail/Texas-Instruments/TPS2051CDBVR?qs=PF3AD18CSE5vi2HeWLJCmw%3D%3D))
      (libsource (lib Power_Management) (part TPS2041B) (description "Single power-distribution switcher"))
      (sheetpath (names /usb/) (tstamps /61B604DE/))
      (tstamp 60D9A6AC))
    (comp (ref J7)
      (value Conn_01x03_Male)
      (footprint Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) 640456-3)
        (field (name MPN-ALT) 22-27-2031)
        (field (name Manufacturer) "TE Connectivity")
        (field (name Manufacturer-ALT) Molex)
        (field (name URL) https://www.lcsc.com/product-detail/Wire-To-Board-Wire-To-Wire-Connector_TE-Connectivity-640456-3_C86503.html)
        (field (name URL-ALT) https://www.mouser.fr/ProductDetail/Molex/22-27-2031?qs=%2Fha2pyFadugXOaGYK9vaczm7nZ04txhJn3OGcnGWT3U=))
      (libsource (lib Connector) (part Conn_01x03_Male) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /fan/) (tstamps /61B99D2C/))
      (tstamp 60E1E49E))
    (comp (ref C28)
      (value "47uF 10V+")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (fields
        (field (name MPN) C2012X5R1A476MTJ00E)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_TDK-C2012X5R1A476MTJ00E_C76636.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /fan/) (tstamps /61B99D2C/))
      (tstamp 60E24715))
    (comp (ref J8)
      (value Conn_01x02)
      (footprint For_SeeedStudio:PinSocket_1x02_P2.54mm_Vertical_for_SeeedStudio)
      (datasheet ~)
      (fields
        (field (name MPN) PM254V-11-02-H85)
        (field (name URL) https://www.lcsc.com/product-detail/Pin-Header-Female-Header_XFCN-PM254V-11-02-H85_C541849.html))
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /fan/) (tstamps /61B99D2C/))
      (tstamp 61BEF34E))
    (comp (ref C29)
      (value "47uF 10V+")
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (fields
        (field (name MPN) C2012X5R1A476MTJ00E)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_TDK-C2012X5R1A476MTJ00E_C76636.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /fan/) (tstamps /61B99D2C/))
      (tstamp 61C19258))
    (comp (ref C35)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193B655))
    (comp (ref C32)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193B673))
    (comp (ref C36)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193B699))
    (comp (ref C37)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB105)
        (field (name Mouser) 603-CC603KRX7R8BB105)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB105_C106858.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193CCFB))
    (comp (ref C31)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193D710))
    (comp (ref R28)
      (value 536)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF5360T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF5360T5E_C23201.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193DCA3))
    (comp (ref J9)
      (value DB15_Female_HighDensity_MountingHoles)
      (footprint For_SeeedStudio:L77HDE15SD1CH4RHNVGA)
      (datasheet " ~")
      (fields
        (field (name "Amphenol Catalog") https://www.mouser.com/datasheet/2/18/1/HD_high_density-1501066.pdf)
        (field (name MPN) L77HDE15SD1CH4FVGA)
        (field (name MPN-STD) L77HDE15SD1CH4F)
        (field (name Notes) "4F, 4R, 3R, 3F: variations on the screw bits")
        (field (name URL) https://www.mouser.fr/ProductDetail/Amphenol-Commercial-Products/L77HDE15SD1CH4FVGA?qs=ToP8pWlZ0bNtQSp9f8k5Rw%3D%3D)
        (field (name URL-STD) https://www.mouser.fr/ProductDetail/Amphenol/L77HDE15SD1CH4F?qs=mq7kV%2Fq8lk6plQnZOUKCHg%3D%3D))
      (libsource (lib Connector) (part DB15_Female_HighDensity_MountingHoles) (description "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 619402B4))
    (comp (ref R33)
      (value 1M)
      (footprint Resistor_SMD:R_1210_3225Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 1210W2F1004T5E)
        (field (name MPN-ALT) RC1210FR-071ML)
        (field (name URL) https://www.lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-1210W2F1004T5E_C620664.html)
        (field (name URL-ALT) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_YAGEO-RC1210FR-071ML_C470029.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61988921))
    (comp (ref C39)
      (value "1 uF (250+V)")
      (footprint Capacitor_THT:CP_Radial_D6.3mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name MPN) KM010M400E110A)
        (field (name MPN-ALT) 860021373002)
        (field (name URL) https://lcsc.com/product-detail/Aluminum-Electrolytic-Capacitors-Leaded_Capxon-International-Elec-KM010M400E110A_C59365.html)
        (field (name URL-ALT) https://www2.mouser.com/ProductDetail/Wurth-Elektronik/860021373002?qs=0KOYDY2FL28tNXbPyU6hsg%3D%3D))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 619889C3))
    (comp (ref R34)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF1000T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_Uniroyal-Elec-0603WAF1000T5E_C22775.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6198A863))
    (comp (ref R35)
      (value 100)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF1000T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_Uniroyal-Elec-0603WAF1000T5E_C22775.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6198C039))
    (comp (ref C34)
      (value 10nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB103)
        (field (name Mouser) 603-CC603KRX7R8BB103)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB103_C327204.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6198FD18))
    (comp (ref C33)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61BBB5E6))
    (comp (ref C30)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61C0186A))
    (comp (ref U12)
      (value ADV7125-lqfp48)
      (footprint For_SeeedStudio:ADV7125KSTZ140)
      (datasheet https://www.mouser.fr/datasheet/2/609/ADV7125-1503638.pdf)
      (fields
        (field (name MPN) ADV7125JSTZ240)
        (field (name URL) https://lcsc.com/product-detail/Digital-To-Analog-Converters-DACs_Analog-Devices-ADV7125JSTZ240_C514373.html))
      (libsource (lib ADV7125-lqfp48) (part ADV7125-lqfp48) (description ""))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 6193ABB5))
    (comp (ref R30)
      (value 75)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF750JT5E)
        (field (name URL) https://www.lcsc.com/product-detail/Chip-Resistor-Surface-Mount_Uniroyal-Elec-0603WAF750JT5E_C4275.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61D22A7E))
    (comp (ref R31)
      (value 75)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF750JT5E)
        (field (name URL) https://www.lcsc.com/product-detail/Chip-Resistor-Surface-Mount_Uniroyal-Elec-0603WAF750JT5E_C4275.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61D23580))
    (comp (ref R32)
      (value 75)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF750JT5E)
        (field (name URL) https://www.lcsc.com/product-detail/Chip-Resistor-Surface-Mount_Uniroyal-Elec-0603WAF750JT5E_C4275.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61D235C2))
    (comp (ref U13)
      (value AD1580)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (fields
        (field (name MPN) AD1580ARTZ)
        (field (name MPN-ALT) AD1580BRTZ)
        (field (name URL) https://www.mouser.fr/ProductDetail/Analog-Devices/AD1580ARTZ-REEL7?qs=NmRFExCfTkENN3U3%252BacLbA%3D%3D)
        (field (name URL-ALT) https://www.mouser.fr/ProductDetail/Analog-Devices/AD1580BRTZ-REEL7?qs=NmRFExCfTkFZVi9%2F1ZfkXg%3D%3D))
      (libsource (lib ad1580) (part AD1580) (description ""))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61BFA3D6))
    (comp (ref R29)
      (value 1k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name MPN) 0603WAF1001T5E)
        (field (name URL) https://lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-0603WAF1001T5E_C21190.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 61BFD6CE))
    (comp (ref C38)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB105)
        (field (name Mouser) 603-CC603KRX7R8BB105)
        (field (name Side) TB)
        (field (name URL) https://lcsc.com/product-detail/Multilayer-Ceramic-Capacitors-MLCC-SMD-SMT_YAGEO-CC0603KRX7R8BB105_C106858.html))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /vga/) (tstamps /6193AB43/))
      (tstamp 62023361)))
  (libparts
    (libpart (lib 74xx) (part 74LS125)
      (aliases
        (alias 74LVC125))
      (description "Quad buffer 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS125)
      (footprints
        (fp DIP?14*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS125))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type 3state))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type 3state))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name ~) (type 3state))
        (pin (num 9) (name ~) (type input))
        (pin (num 10) (name ~) (type input))
        (pin (num 11) (name ~) (type 3state))
        (pin (num 12) (name ~) (type input))
        (pin (num 13) (name ~) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib 74xx) (part 74LS245)
      (aliases
        (alias 74HC245))
      (description "Octal BUS Transceivers, 3-State outputs")
      (docs http://www.ti.com/lit/gpn/sn74LS245)
      (footprints
        (fp DIP?20*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LS245))
      (pins
        (pin (num 1) (name A->B) (type input))
        (pin (num 2) (name A0) (type 3state))
        (pin (num 3) (name A1) (type 3state))
        (pin (num 4) (name A2) (type 3state))
        (pin (num 5) (name A3) (type 3state))
        (pin (num 6) (name A4) (type 3state))
        (pin (num 7) (name A5) (type 3state))
        (pin (num 8) (name A6) (type 3state))
        (pin (num 9) (name A7) (type 3state))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name B7) (type 3state))
        (pin (num 12) (name B6) (type 3state))
        (pin (num 13) (name B5) (type 3state))
        (pin (num 14) (name B4) (type 3state))
        (pin (num 15) (name B3) (type 3state))
        (pin (num 16) (name B2) (type 3state))
        (pin (num 17) (name B1) (type 3state))
        (pin (num 18) (name B0) (type 3state))
        (pin (num 19) (name CE) (type input))
        (pin (num 20) (name VCC) (type power_in))))
    (libpart (lib ADV7125-lqfp48) (part ADV7125-lqfp48)
      (fields
        (field (name Reference) U)
        (field (name Value) ADV7125-lqfp48)
        (field (name Footprint) MODULE)
        (field (name Datasheet) DOCUMENTATION))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name G0) (type input))
        (pin (num 4) (name G1) (type input))
        (pin (num 5) (name G2) (type input))
        (pin (num 6) (name G3) (type input))
        (pin (num 7) (name G4) (type input))
        (pin (num 8) (name G5) (type input))
        (pin (num 9) (name G6) (type input))
        (pin (num 10) (name G7) (type input))
        (pin (num 11) (name BLANKB) (type input))
        (pin (num 12) (name SYNCB) (type input))
        (pin (num 13) (name VAA) (type input))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name B0) (type input))
        (pin (num 17) (name B1) (type input))
        (pin (num 18) (name B2) (type input))
        (pin (num 19) (name B3) (type input))
        (pin (num 20) (name B4) (type input))
        (pin (num 21) (name B5) (type input))
        (pin (num 22) (name B6) (type input))
        (pin (num 23) (name B7) (type input))
        (pin (num 24) (name CLOCK) (type input))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name GND) (type power_in))
        (pin (num 27) (name "#IOB") (type input))
        (pin (num 28) (name IOB) (type input))
        (pin (num 29) (name VAA) (type input))
        (pin (num 30) (name VAA) (type input))
        (pin (num 31) (name "#IOG") (type input))
        (pin (num 32) (name IOG) (type input))
        (pin (num 33) (name "#IOR") (type input))
        (pin (num 34) (name IOR) (type input))
        (pin (num 35) (name COMP) (type input))
        (pin (num 36) (name VREF) (type input))
        (pin (num 37) (name RSET) (type input))
        (pin (num 38) (name PSAVEB) (type input))
        (pin (num 39) (name GND) (type power_in))
        (pin (num 40) (name GND) (type power_in))
        (pin (num 41) (name R0) (type input))
        (pin (num 42) (name R1) (type input))
        (pin (num 43) (name R2) (type input))
        (pin (num 44) (name R3) (type input))
        (pin (num 45) (name R4) (type input))
        (pin (num 46) (name R5) (type input))
        (pin (num 47) (name R6) (type input))
        (pin (num 48) (name R7) (type input))))
    (libpart (lib C96ABC) (part C96ABC_NUBUS)
      (fields
        (field (name Reference) J)
        (field (name Value) C96ABC_NUBUS))
      (pins
        (pin (num a1) (name a1) (type passive))
        (pin (num a2) (name a2) (type passive))
        (pin (num a3) (name a3) (type passive))
        (pin (num a4) (name a4) (type passive))
        (pin (num a5) (name a5) (type passive))
        (pin (num a6) (name a6) (type passive))
        (pin (num a7) (name a7) (type passive))
        (pin (num a8) (name a8) (type passive))
        (pin (num a9) (name a9) (type passive))
        (pin (num a10) (name a10) (type passive))
        (pin (num a11) (name a11) (type passive))
        (pin (num a12) (name a12) (type passive))
        (pin (num a13) (name a13) (type passive))
        (pin (num a14) (name a14) (type passive))
        (pin (num a15) (name a15) (type passive))
        (pin (num a16) (name a16) (type passive))
        (pin (num a17) (name a17) (type passive))
        (pin (num a18) (name a18) (type passive))
        (pin (num a19) (name a19) (type passive))
        (pin (num a20) (name a20) (type passive))
        (pin (num a21) (name a21) (type 3state))
        (pin (num a22) (name a22) (type passive))
        (pin (num a23) (name a23) (type passive))
        (pin (num a24) (name a24) (type passive))
        (pin (num a25) (name a25) (type passive))
        (pin (num a26) (name a26) (type passive))
        (pin (num a27) (name a27) (type passive))
        (pin (num a28) (name a28) (type passive))
        (pin (num a29) (name a29) (type passive))
        (pin (num a30) (name a30) (type passive))
        (pin (num a31) (name a31) (type passive))
        (pin (num a32) (name a32) (type passive))
        (pin (num b1) (name b1) (type passive))
        (pin (num b2) (name b2) (type passive))
        (pin (num b3) (name b3) (type passive))
        (pin (num b4) (name b4) (type passive))
        (pin (num b5) (name b5) (type passive))
        (pin (num b6) (name b6) (type passive))
        (pin (num b7) (name b7) (type passive))
        (pin (num b8) (name b8) (type passive))
        (pin (num b9) (name b9) (type passive))
        (pin (num b10) (name b10) (type passive))
        (pin (num b11) (name b11) (type passive))
        (pin (num b12) (name b12) (type passive))
        (pin (num b13) (name b13) (type passive))
        (pin (num b14) (name b14) (type passive))
        (pin (num b15) (name b15) (type passive))
        (pin (num b16) (name b16) (type passive))
        (pin (num b17) (name b17) (type passive))
        (pin (num b18) (name b18) (type passive))
        (pin (num b19) (name b19) (type passive))
        (pin (num b20) (name b20) (type passive))
        (pin (num b21) (name b21) (type passive))
        (pin (num b22) (name b22) (type passive))
        (pin (num b23) (name b23) (type passive))
        (pin (num b24) (name b24) (type passive))
        (pin (num b25) (name b25) (type passive))
        (pin (num b26) (name b26) (type passive))
        (pin (num b27) (name b27) (type passive))
        (pin (num b28) (name b28) (type passive))
        (pin (num b29) (name b29) (type passive))
        (pin (num b30) (name b30) (type passive))
        (pin (num b31) (name b31) (type passive))
        (pin (num b32) (name b32) (type passive))
        (pin (num c1) (name c1) (type passive))
        (pin (num c2) (name c2) (type passive))
        (pin (num c3) (name c3) (type passive))
        (pin (num c4) (name c4) (type passive))
        (pin (num c5) (name c5) (type passive))
        (pin (num c6) (name c6) (type passive))
        (pin (num c7) (name c7) (type passive))
        (pin (num c8) (name c8) (type passive))
        (pin (num c9) (name c9) (type passive))
        (pin (num c10) (name c10) (type passive))
        (pin (num c11) (name c11) (type passive))
        (pin (num c12) (name c12) (type passive))
        (pin (num c13) (name c13) (type passive))
        (pin (num c14) (name c14) (type passive))
        (pin (num c15) (name c15) (type passive))
        (pin (num c16) (name c16) (type passive))
        (pin (num c17) (name c17) (type passive))
        (pin (num c18) (name c18) (type passive))
        (pin (num c19) (name c19) (type passive))
        (pin (num c20) (name c20) (type passive))
        (pin (num c21) (name c21) (type passive))
        (pin (num c22) (name c22) (type passive))
        (pin (num c23) (name c23) (type passive))
        (pin (num c24) (name c24) (type passive))
        (pin (num c25) (name c25) (type passive))
        (pin (num c26) (name c26) (type passive))
        (pin (num c27) (name c27) (type passive))
        (pin (num c28) (name c28) (type passive))
        (pin (num c29) (name c29) (type passive))
        (pin (num c30) (name c30) (type passive))
        (pin (num c31) (name c31) (type passive))
        (pin (num c32) (name c32) (type passive))))
    (libpart (lib CPLD_Xilinx) (part XC9572XL-VQ64)
      (description "CPLD, 72 Macrocells, 1600 Usable Gates")
      (docs http://www.xilinx.com/support/documentation/data_sheets/ds057.pdf)
      (footprints
        (fp TQFP*10x10mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) XC9572XL-VQ64)
        (field (name Footprint) Package_QFP:TQFP-64_10x10mm_P0.5mm))
      (pins
        (pin (num 1) (name P1) (type BiDi))
        (pin (num 2) (name I/O/GTS2) (type BiDi))
        (pin (num 3) (name VCC) (type power_in))
        (pin (num 4) (name P4) (type BiDi))
        (pin (num 5) (name I/O/GTS1) (type BiDi))
        (pin (num 6) (name P6) (type BiDi))
        (pin (num 7) (name P7) (type BiDi))
        (pin (num 8) (name P8) (type BiDi))
        (pin (num 9) (name P9) (type BiDi))
        (pin (num 10) (name P10) (type BiDi))
        (pin (num 11) (name P11) (type BiDi))
        (pin (num 12) (name P12) (type BiDi))
        (pin (num 13) (name P13) (type BiDi))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name I/O/GCK1) (type BiDi))
        (pin (num 16) (name I/O/GCK2) (type BiDi))
        (pin (num 17) (name I/O/GCK3) (type BiDi))
        (pin (num 18) (name P18) (type BiDi))
        (pin (num 19) (name P19) (type BiDi))
        (pin (num 20) (name P20) (type BiDi))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name P22) (type BiDi))
        (pin (num 23) (name P23) (type BiDi))
        (pin (num 24) (name P24) (type BiDi))
        (pin (num 25) (name P25) (type BiDi))
        (pin (num 26) (name VCCIO) (type power_in))
        (pin (num 27) (name P27) (type BiDi))
        (pin (num 28) (name TDI) (type input))
        (pin (num 29) (name TMS) (type input))
        (pin (num 30) (name TCK) (type input))
        (pin (num 31) (name P31) (type BiDi))
        (pin (num 32) (name P32) (type BiDi))
        (pin (num 33) (name P33) (type BiDi))
        (pin (num 34) (name P34) (type BiDi))
        (pin (num 35) (name P35) (type BiDi))
        (pin (num 36) (name P36) (type BiDi))
        (pin (num 37) (name VCC) (type power_in))
        (pin (num 38) (name P38) (type BiDi))
        (pin (num 39) (name P39) (type BiDi))
        (pin (num 40) (name P40) (type BiDi))
        (pin (num 41) (name GND) (type power_in))
        (pin (num 42) (name P42) (type BiDi))
        (pin (num 43) (name P43) (type BiDi))
        (pin (num 44) (name P44) (type BiDi))
        (pin (num 45) (name P45) (type BiDi))
        (pin (num 46) (name P46) (type BiDi))
        (pin (num 47) (name P47) (type BiDi))
        (pin (num 48) (name P48) (type BiDi))
        (pin (num 49) (name P49) (type BiDi))
        (pin (num 50) (name P50) (type BiDi))
        (pin (num 51) (name P51) (type BiDi))
        (pin (num 52) (name P52) (type BiDi))
        (pin (num 53) (name TDO) (type output))
        (pin (num 54) (name GND) (type power_in))
        (pin (num 55) (name VCCIO) (type power_in))
        (pin (num 56) (name P56) (type BiDi))
        (pin (num 57) (name P57) (type BiDi))
        (pin (num 58) (name P58) (type BiDi))
        (pin (num 59) (name P59) (type BiDi))
        (pin (num 60) (name P60) (type BiDi))
        (pin (num 61) (name P61) (type BiDi))
        (pin (num 62) (name P62) (type BiDi))
        (pin (num 63) (name P63) (type BiDi))
        (pin (num 64) (name I/O/GSR) (type BiDi))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector) (part Conn_01x06_Male)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector) (part DB15_Female_HighDensity_MountingHoles)
      (description "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Female*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB15_Female_HighDensity_MountingHoles))
      (pins
        (pin (num 0) (name ~) (type passive))
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num 13) (name ~) (type passive))
        (pin (num 14) (name ~) (type passive))
        (pin (num 15) (name ~) (type passive))))
    (libpart (lib Connector) (part HDMI_A)
      (description "HDMI type A connector")
      (docs https://en.wikipedia.org/wiki/HDMI)
      (footprints
        (fp HDMI*A*))
      (fields
        (field (name Reference) J)
        (field (name Value) HDMI_A))
      (pins
        (pin (num 1) (name D2+) (type passive))
        (pin (num 2) (name D2S) (type power_in))
        (pin (num 3) (name D2-) (type passive))
        (pin (num 4) (name D1+) (type passive))
        (pin (num 5) (name D1S) (type power_in))
        (pin (num 6) (name D1-) (type passive))
        (pin (num 7) (name D0+) (type passive))
        (pin (num 8) (name D0S) (type power_in))
        (pin (num 9) (name D0-) (type passive))
        (pin (num 10) (name CK+) (type passive))
        (pin (num 11) (name CKS) (type power_in))
        (pin (num 12) (name CK-) (type passive))
        (pin (num 13) (name CEC) (type BiDi))
        (pin (num 14) (name UTILITY) (type passive))
        (pin (num 15) (name SCL) (type passive))
        (pin (num 16) (name SDA) (type BiDi))
        (pin (num 17) (name GND) (type power_in))
        (pin (num 18) (name +5V) (type power_in))
        (pin (num 19) (name HPD) (type passive))
        (pin (num SH) (name SH) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x07_Odd_Even)
      (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x07_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead_Small)
      (description "Ferrite bead, small symbol")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part LED_ALT)
      (description "Light emitting diode, filled shape")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_ALT))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Power_Management) (part TPS2041B)
      (description "Single power-distribution switcher")
      (docs http://www.ti.com/lit/ds/symlink/tps2041.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS2041B)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name OUT) (type power_out))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name ~OC) (type openCol))
        (pin (num 4) (name ~EN) (type input))
        (pin (num 5) (name IN) (type power_in))))
    (libpart (lib Power_Protection) (part SN65220)
      (description "USB port transient suppressors")
      (docs http://www.ti.com/lit/ds/symlink/sn65220.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) SN65220)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name ~) (type NotConnected))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name ~) (type NotConnected))
        (pin (num 4) (name B) (type passive))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name A) (type passive))))
    (libpart (lib TPD12S016PWR) (part TPD12S016PWR)
      (fields
        (field (name Reference) U)
        (field (name Value) TPD12S016PWR)
        (field (name Footprint) SOP65P640X120-24N)
        (field (name MAXIMUM_PACKAGE_HEIGHT) "1.2 mm")
        (field (name MANUFACTURER) "Texas Instruments")
        (field (name PARTREV) F)
        (field (name STANDARD) "IPC 7351B"))
      (pins
        (pin (num 1) (name CEC_A) (type BiDi))
        (pin (num 2) (name SCL_A) (type BiDi))
        (pin (num 3) (name SDA_A) (type BiDi))
        (pin (num 4) (name HPD_A) (type output))
        (pin (num 5) (name LS_OE) (type input))
        (pin (num 6) (name GND_6) (type power_in))
        (pin (num 7) (name CEC_B) (type BiDi))
        (pin (num 8) (name SCL_B) (type BiDi))
        (pin (num 9) (name SDA_B) (type BiDi))
        (pin (num 10) (name HPD_B) (type input))
        (pin (num 11) (name VCC5V) (type input))
        (pin (num 12) (name CT_HPD) (type input))
        (pin (num 13) (name 5V_OUT) (type output))
        (pin (num 14) (name GND_14) (type power_in))
        (pin (num 15) (name CLK-) (type BiDi))
        (pin (num 16) (name CLK+) (type BiDi))
        (pin (num 17) (name D0-) (type BiDi))
        (pin (num 18) (name D0+) (type BiDi))
        (pin (num 19) (name GND_19) (type power_in))
        (pin (num 20) (name D1-) (type BiDi))
        (pin (num 21) (name D1+) (type BiDi))
        (pin (num 22) (name D2-) (type BiDi))
        (pin (num 23) (name D2+) (type BiDi))
        (pin (num 24) (name VCCA) (type power_in))))
    (libpart (lib ad1580) (part AD1580)
      (footprints
        (fp SOT-23-3))
      (fields
        (field (name Reference) U)
        (field (name Value) AD1580))
      (pins
        (pin (num 1) (name V+) (type input))
        (pin (num 2) (name V-) (type output))
        (pin (num 3) (name NC) (type passive))))
    (libpart (lib ztex_AB) (part ZTEX_AB)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) ZTEX_AB))
      (pins
        (pin (num 1) (name VIN) (type passive))
        (pin (num 2) (name VIN) (type passive))
        (pin (num 3) (name GND) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name K16~IO_25_15) (type passive))
        (pin (num 6) (name J18~IO_L23N_T3_FWE_B_15) (type passive))
        (pin (num 7) (name K15~IO_L24P_T3_RS1_15) (type passive))
        (pin (num 8) (name J17~IO_L23P_T3_FOE_B_15) (type passive))
        (pin (num 9) (name J15~IO_L24N_T3_RS0_15) (type passive))
        (pin (num 10) (name K13~IO_L17P_T2_A26_15) (type passive))
        (pin (num 11) (name H15~IO_L19N_T3_A21_VREF_15) (type passive))
        (pin (num 12) (name J13~IO_L17N_T2_A25_15) (type passive))
        (pin (num 13) (name J14~IO_L19P_T3_A22_15) (type passive))
        (pin (num 14) (name H14~IO_L15P_T2_DQS_15) (type passive))
        (pin (num 15) (name H17~IO_L18P_T2_A24_15) (type passive))
        (pin (num 16) (name G14~IO_L15N_T2_DQS_ADV_B_15) (type passive))
        (pin (num 17) (name G17~IO_L18N_T2_A23_15) (type passive))
        (pin (num 18) (name G16~IO_L13N_T2_MRCC_15) (type passive))
        (pin (num 19) (name G18~IO_L22P_T3_A17_15) (type passive))
        (pin (num 20) (name H16~IO_L13P_T2_MRCC_15) (type passive))
        (pin (num 21) (name F18~IO_L22N_T3_A16_15) (type passive))
        (pin (num 22) (name F16~IO_L14N_T2_SRCC_15) (type passive))
        (pin (num 23) (name E18~IO_L21P_T3_DQS_15) (type passive))
        (pin (num 24) (name F15~IO_L14P_T2_SRCC_15) (type passive))
        (pin (num 25) (name D18~IO_L21N_T3_DQS_A18_15) (type passive))
        (pin (num 26) (name E17~IO_L16P_T2_A28_15) (type passive))
        (pin (num 27) (name G13~IO_0_15) (type passive))
        (pin (num 28) (name D17~IO_L16N_T2_A27_15) (type passive))
        (pin (num 29) (name 3.3V) (type passive))
        (pin (num 30) (name 3.3V) (type passive))
        (pin (num 31) (name GND) (type passive))
        (pin (num 32) (name GND) (type passive))
        (pin (num 33) (name VCCO_AB) (type passive))
        (pin (num 34) (name VCCO_AB) (type passive))
        (pin (num 35) (name F13~IO_L5P_T0_AD9P_15) (type passive))
        (pin (num 36) (name F14~IO_L5N_T0_AD9N_15) (type passive))
        (pin (num 37) (name E16~IO_L11N_T1_SRCC_15) (type passive))
        (pin (num 38) (name E15~IO_L11P_T1_SRCC_15) (type passive))
        (pin (num 39) (name C17~IO_L20N_T3_A19_15) (type passive))
        (pin (num 40) (name C16~IO_L20P_T3_A20_15) (type passive))
        (pin (num 41) (name A18~IO_L10N_T1_AD11N_15) (type passive))
        (pin (num 42) (name B18~IO_L10P_T1_AD11P_15) (type passive))
        (pin (num 43) (name C15~IO_L12N_T1_MRCC_15) (type passive))
        (pin (num 44) (name D15~IO_L12P_T1_MRCC_15) (type passive))
        (pin (num 45) (name B17~IO_L7N_T1_AD2N_15) (type passive))
        (pin (num 46) (name B16~IO_L7P_T1_AD2P_15) (type passive))
        (pin (num 47) (name C14~IO_L1N_T0_AD0N_15) (type passive))
        (pin (num 48) (name D14~IO_L1P_T0_AD0P_15) (type passive))
        (pin (num 49) (name D13~IO_L6N_T0_VREF_15) (type passive))
        (pin (num 50) (name D12~IO_L6P_T0_15) (type passive))
        (pin (num 51) (name A16~IO_L8N_T1_AD10N_15) (type passive))
        (pin (num 52) (name A15~IO_L8P_T1_AD10P_15) (type passive))
        (pin (num 53) (name B14~IO_L2N_T0_AD8N_15) (type passive))
        (pin (num 54) (name B13~IO_L2P_T0_AD8P_15) (type passive))
        (pin (num 55) (name B12~IO_L3N_T0_DQS_AD1N_15) (type passive))
        (pin (num 56) (name C12~IO_L3P_T0_DQS_AD1P_15) (type passive))
        (pin (num 57) (name A14~IO_L9N_T1_DQS_AD3N_15) (type passive))
        (pin (num 58) (name A13~IO_L9P_T1_DQS_AD3P_15) (type passive))
        (pin (num 59) (name B11~IO_L4P_T0_15) (type passive))
        (pin (num 60) (name A11~IO_L4N_T0_15) (type passive))
        (pin (num 61) (name JTAG_TDI) (type passive))
        (pin (num 62) (name JTAG_TCK) (type passive))
        (pin (num 63) (name JTAG_VIO) (type passive))
        (pin (num 64) (name GND) (type passive))))
    (libpart (lib ztex_CD) (part ZTEX_CD)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) ZTEX_CD))
      (pins
        (pin (num 1) (name USB_5V) (type passive))
        (pin (num 2) (name RESET#) (type passive))
        (pin (num 3) (name GND) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name U9~IO_L21P_T3_DQS_34) (type passive))
        (pin (num 6) (name V9~IO_L21N_T3_DQS_34) (type passive))
        (pin (num 7) (name U8~IO_25_34) (type passive))
        (pin (num 8) (name V7~IO_L20P_T3_34) (type passive))
        (pin (num 9) (name U7~IO_L22P_T3_34) (type passive))
        (pin (num 10) (name V6~IO_L20N_T3_34) (type passive))
        (pin (num 11) (name U6~IO_L22N_T3_34) (type passive))
        (pin (num 12) (name V5~IO_L10P_T1_34) (type passive))
        (pin (num 13) (name T8~IO_L24N_T3_34) (type passive))
        (pin (num 14) (name V4~IO_L10N_T1_34) (type passive))
        (pin (num 15) (name R8~IO_L24P_T3_34) (type passive))
        (pin (num 16) (name T5~IO_L12P_T1_MRCC_34) (type passive))
        (pin (num 17) (name R7~IO_L23P_T3_34) (type passive))
        (pin (num 18) (name T4~IO_L12N_T1_MRCC_34) (type passive))
        (pin (num 19) (name T6~IO_L23N_T3_34) (type passive))
        (pin (num 20) (name U4~IO_L8P_T1_34) (type passive))
        (pin (num 21) (name R6~IO_L19P_T3_34) (type passive))
        (pin (num 22) (name U3~IO_L8N_T1_34) (type passive))
        (pin (num 23) (name R5~IO_L19N_T3_VREF_34) (type passive))
        (pin (num 24) (name V1~IO_L7N_T1_34) (type passive))
        (pin (num 25) (name V2~IO_L9N_T1_DQS_34) (type passive))
        (pin (num 26) (name U1~IO_L7P_T1_34) (type passive))
        (pin (num 27) (name U2~IO_L9P_T1_DQS_34) (type passive))
        (pin (num 28) (name T3~IO_L11N_T1_SRCC_34) (type passive))
        (pin (num 29) (name K6~IO_0_34) (type passive))
        (pin (num 30) (name R3~IO_L11P_T1_SRCC_34) (type passive))
        (pin (num 31) (name VCCO_CD) (type passive))
        (pin (num 32) (name VCCO_CD) (type passive))
        (pin (num 33) (name GND) (type passive))
        (pin (num 34) (name GND) (type passive))
        (pin (num 35) (name 3.3V) (type passive))
        (pin (num 36) (name 3.3V) (type passive))
        (pin (num 37) (name N6~IO_L18N_T2_34) (type passive))
        (pin (num 38) (name P5~IO_L13N_T2_MRCC_34) (type passive))
        (pin (num 39) (name M6~IO_L18P_T2_34) (type passive))
        (pin (num 40) (name N5~IO_L13P_T2_MRCC_34) (type passive))
        (pin (num 41) (name L6~IO_L6P_T0_34) (type passive))
        (pin (num 42) (name P4~IO_L14P_T2_SRCC_34) (type passive))
        (pin (num 43) (name L5~IO_L6N_T0_VREF_34) (type passive))
        (pin (num 44) (name P3~IO_L14N_T2_SRCC_34) (type passive))
        (pin (num 45) (name N4~IO_L16N_T2_34) (type passive))
        (pin (num 46) (name T1~IO_L17N_T2_34) (type passive))
        (pin (num 47) (name M4~IO_L16P_T2_34) (type passive))
        (pin (num 48) (name R1~IO_L17P_T2_34) (type passive))
        (pin (num 49) (name M3~IO_L4P_T0_34) (type passive))
        (pin (num 50) (name R2~IO_L15N_T2_DQS_34) (type passive))
        (pin (num 51) (name M2~IO_L4N_T0_34) (type passive))
        (pin (num 52) (name P2~IO_L15P_T2_DQS_34) (type passive))
        (pin (num 53) (name K5~IO_L5P_T0_34) (type passive))
        (pin (num 54) (name N2~IO_L3P_T0_DQS_34) (type passive))
        (pin (num 55) (name L4~IO_L5N_T0_34) (type passive))
        (pin (num 56) (name N1~IO_L3N_T0_DQS_34) (type passive))
        (pin (num 57) (name L3~IO_L2N_T0_34) (type passive))
        (pin (num 58) (name M1~IO_L1N_T0_34) (type passive))
        (pin (num 59) (name K3~IO_L2P_T0_34) (type passive))
        (pin (num 60) (name L1~IO_L1P_T0_34) (type passive))
        (pin (num 61) (name JTAG_TDO) (type passive))
        (pin (num 62) (name JTAG_TMS) (type passive))
        (pin (num 63) (name GND) (type passive))
        (pin (num 64) (name GND) (type passive)))))
  (libraries
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical ADV7125-lqfp48)
      (uri /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/ADV7125-lqfp48.lib))
    (library (logical C96ABC)
      (uri /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/NuBus/C96ABC.lib))
    (library (logical CPLD_Xilinx)
      (uri /usr/share/kicad/library/CPLD_Xilinx.lib))
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Power_Management)
      (uri /usr/share/kicad/library/Power_Management.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical TPD12S016PWR)
      (uri /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/TPD12S016PWR.lib))
    (library (logical ad1580)
      (uri /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/ad1580.lib))
    (library (logical ztex_AB)
      (uri /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/ztex_AB.lib))
    (library (logical ztex_CD)
      (uri /home/dolbeau/MAC/NuBusFPGA/nubus-to-ztex/ztex_CD.lib)))
  (nets
    (net (code 1) (name /B2B/TX)
      (node (ref J3) (pin 5))
      (node (ref JCD1) (pin 6)))
    (net (code 2) (name +3V3)
      (node (ref JAB1) (pin 33))
      (node (ref R37) (pin 1))
      (node (ref JAB1) (pin 29))
      (node (ref R36) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref C32) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref U6) (pin 20))
      (node (ref U12) (pin 29))
      (node (ref JAB1) (pin 30))
      (node (ref C14) (pin 1))
      (node (ref JAB1) (pin 34))
      (node (ref U3) (pin 14))
      (node (ref C4) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref U5) (pin 20))
      (node (ref C31) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref U9) (pin 24))
      (node (ref U9) (pin 5))
      (node (ref U9) (pin 12))
      (node (ref C9) (pin 1))
      (node (ref JCD1) (pin 31))
      (node (ref JCD1) (pin 35))
      (node (ref C11) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref JCD1) (pin 32))
      (node (ref JCD1) (pin 36))
      (node (ref U12) (pin 11))
      (node (ref R29) (pin 1))
      (node (ref U12) (pin 13))
      (node (ref C13) (pin 1))
      (node (ref C33) (pin 1))
      (node (ref U12) (pin 30))
      (node (ref U8) (pin 20))
      (node (ref R14) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref C30) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref R21) (pin 1))
      (node (ref U4) (pin 37))
      (node (ref U12) (pin 38))
      (node (ref U4) (pin 3))
      (node (ref U1) (pin 14))
      (node (ref R15) (pin 1))
      (node (ref R44) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref U4) (pin 55))
      (node (ref U4) (pin 26))
      (node (ref R16) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref C20) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref R39) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref R40) (pin 1))
      (node (ref R41) (pin 1))
      (node (ref R38) (pin 1))
      (node (ref R42) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref R43) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref U2) (pin 13))
      (node (ref J8) (pin 1))
      (node (ref U2) (pin 14))
      (node (ref C5) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref R45) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U7) (pin 20)))
    (net (code 3) (name "Net-(J2-Pad12)")
      (node (ref J2) (pin 12)))
    (net (code 4) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14)))
    (net (code 5) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 6) (name "Net-(J1-Pad14)")
      (node (ref J1) (pin 14)))
    (net (code 7) (name CPLD_JTAG_TDO)
      (node (ref U4) (pin 53))
      (node (ref J2) (pin 8)))
    (net (code 8) (name CPLD_JTAG_TCK)
      (node (ref J2) (pin 6))
      (node (ref U4) (pin 30)))
    (net (code 9) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref R3) (pin 2)))
    (net (code 10) (name CPLD_JTAG_TMS)
      (node (ref U4) (pin 29))
      (node (ref J2) (pin 4)))
    (net (code 11) (name "Net-(D2-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 12) (name "Net-(D1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 13) (name CPLD_JTAG_TDI)
      (node (ref U4) (pin 28))
      (node (ref J2) (pin 10)))
    (net (code 14) (name ~AD31_3V3)
      (node (ref U5) (pin 18))
      (node (ref JAB1) (pin 19)))
    (net (code 15) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3)))
    (net (code 16) (name HDMI_CLK-)
      (node (ref JCD1) (pin 23))
      (node (ref U9) (pin 15))
      (node (ref J5) (pin 12)))
    (net (code 17) (name HDMI_CLK+)
      (node (ref J5) (pin 10))
      (node (ref JCD1) (pin 21))
      (node (ref U9) (pin 16)))
    (net (code 18) (name HDMI_CEC_A)
      (node (ref JCD1) (pin 19))
      (node (ref U9) (pin 1)))
    (net (code 19) (name "Net-(JCD1-Pad1)")
      (node (ref JCD1) (pin 1)))
    (net (code 20) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6)))
    (net (code 21) (name HDMI_D1-)
      (node (ref J5) (pin 6))
      (node (ref JCD1) (pin 25))
      (node (ref U9) (pin 20)))
    (net (code 22) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2)))
    (net (code 23) (name NUBUS_AD_DIR)
      (node (ref U8) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref JAB1) (pin 18))
      (node (ref U6) (pin 1)))
    (net (code 24) (name fpga_to_cpld_signal_2)
      (node (ref U4) (pin 50))
      (node (ref JAB1) (pin 16)))
    (net (code 25) (name fpga_to_cpld_clk)
      (node (ref JAB1) (pin 14))
      (node (ref U4) (pin 15)))
    (net (code 26) (name ARB)
      (node (ref JAB1) (pin 12))
      (node (ref D4) (pin 1))
      (node (ref U4) (pin 52)))
    (net (code 27) (name ~ACK_3V3)
      (node (ref JAB1) (pin 10))
      (node (ref D8) (pin 1))
      (node (ref U4) (pin 2)))
    (net (code 28) (name ~TM1_3V3)
      (node (ref U4) (pin 62))
      (node (ref D6) (pin 1))
      (node (ref JAB1) (pin 8)))
    (net (code 29) (name FPGA_B0)
      (node (ref U12) (pin 16))
      (node (ref JCD1) (pin 51)))
    (net (code 30) (name HDMI_SCL_A)
      (node (ref U9) (pin 2))
      (node (ref JCD1) (pin 17)))
    (net (code 31) (name HDMI_SDA_A)
      (node (ref U9) (pin 3))
      (node (ref JCD1) (pin 15)))
    (net (code 32) (name HDMI_HPD_A)
      (node (ref U9) (pin 4))
      (node (ref JCD1) (pin 13)))
    (net (code 33) (name tmoen)
      (node (ref JCD1) (pin 11))
      (node (ref U4) (pin 51)))
    (net (code 34) (name ~ID0_3V3)
      (node (ref U4) (pin 59))
      (node (ref JCD1) (pin 9))
      (node (ref D11) (pin 1)))
    (net (code 35) (name ~ID3_3V3)
      (node (ref U4) (pin 1))
      (node (ref D14) (pin 1))
      (node (ref JCD1) (pin 7)))
    (net (code 36) (name FPGA_JTAG_TDO)
      (node (ref JCD1) (pin 61))
      (node (ref J1) (pin 8)))
    (net (code 37) (name FPGA_G4)
      (node (ref JCD1) (pin 59))
      (node (ref U12) (pin 7)))
    (net (code 38) (name /B2B/RX)
      (node (ref J3) (pin 4))
      (node (ref JCD1) (pin 5)))
    (net (code 39) (name FPGA_G5)
      (node (ref JCD1) (pin 57))
      (node (ref U12) (pin 8)))
    (net (code 40) (name FPGA_G6)
      (node (ref U12) (pin 9))
      (node (ref JCD1) (pin 55)))
    (net (code 41) (name FPGA_G7)
      (node (ref U12) (pin 10))
      (node (ref JCD1) (pin 53)))
    (net (code 42) (name FPGA_B1)
      (node (ref U12) (pin 17))
      (node (ref JCD1) (pin 49)))
    (net (code 43) (name FPGA_B2)
      (node (ref U12) (pin 18))
      (node (ref JCD1) (pin 47)))
    (net (code 44) (name FPGA_B3)
      (node (ref U12) (pin 19))
      (node (ref JCD1) (pin 45)))
    (net (code 45) (name FPGA_B4)
      (node (ref U12) (pin 20))
      (node (ref JCD1) (pin 43)))
    (net (code 46) (name FPGA_B5)
      (node (ref U12) (pin 21))
      (node (ref JCD1) (pin 41)))
    (net (code 47) (name FPGA_B6)
      (node (ref U12) (pin 22))
      (node (ref JCD1) (pin 39)))
    (net (code 48) (name FPGA_B7)
      (node (ref U12) (pin 23))
      (node (ref JCD1) (pin 37)))
    (net (code 49) (name FPGA_VGA_CLK)
      (node (ref JCD1) (pin 29))
      (node (ref U12) (pin 24)))
    (net (code 50) (name HDMI_D1+)
      (node (ref J5) (pin 4))
      (node (ref U9) (pin 21))
      (node (ref JCD1) (pin 27)))
    (net (code 51) (name ~AD15_3V3)
      (node (ref JAB1) (pin 43))
      (node (ref U7) (pin 17)))
    (net (code 52) (name GRANT)
      (node (ref JAB1) (pin 11))
      (node (ref U4) (pin 56))
      (node (ref D5) (pin 1)))
    (net (code 53) (name ~START_3V3)
      (node (ref JAB1) (pin 9))
      (node (ref U4) (pin 4))
      (node (ref D9) (pin 1)))
    (net (code 54) (name ~TM0_3V3)
      (node (ref D7) (pin 1))
      (node (ref U4) (pin 61))
      (node (ref JAB1) (pin 7)))
    (net (code 55) (name /B2B/JTAG_VIO)
      (node (ref JAB1) (pin 63)))
    (net (code 56) (name USBH0_D+)
      (node (ref JAB1) (pin 59))
      (node (ref R22) (pin 2)))
    (net (code 57) (name ~RQST_3V3)
      (node (ref U4) (pin 64))
      (node (ref JAB1) (pin 5)))
    (net (code 58) (name ~AD1_3V3)
      (node (ref JAB1) (pin 57))
      (node (ref D15) (pin 1))
      (node (ref U8) (pin 11)))
    (net (code 59) (name ~AD3_3V3)
      (node (ref U8) (pin 13))
      (node (ref JAB1) (pin 55)))
    (net (code 60) (name ~AD5_3V3)
      (node (ref U8) (pin 15))
      (node (ref JAB1) (pin 53)))
    (net (code 61) (name ~AD7_3V3)
      (node (ref JAB1) (pin 51))
      (node (ref U8) (pin 17)))
    (net (code 62) (name ~AD9_3V3)
      (node (ref JAB1) (pin 49))
      (node (ref U7) (pin 11)))
    (net (code 63) (name ~AD11_3V3)
      (node (ref JAB1) (pin 47))
      (node (ref U7) (pin 13)))
    (net (code 64) (name ~AD13_3V3)
      (node (ref JAB1) (pin 45))
      (node (ref U7) (pin 15)))
    (net (code 65) (name fpga_to_cpld_signal)
      (node (ref U4) (pin 23))
      (node (ref JAB1) (pin 13)))
    (net (code 66) (name ~AD17_3V3)
      (node (ref U6) (pin 11))
      (node (ref JAB1) (pin 41)))
    (net (code 67) (name ~AD19_3V3)
      (node (ref JAB1) (pin 39))
      (node (ref U6) (pin 13)))
    (net (code 68) (name ~AD21_3V3)
      (node (ref JAB1) (pin 37))
      (node (ref U6) (pin 15)))
    (net (code 69) (name ~AD23_3V3)
      (node (ref U6) (pin 17))
      (node (ref JAB1) (pin 35)))
    (net (code 70) (name NUBUS_OE)
      (node (ref U5) (pin 19))
      (node (ref R4) (pin 2))
      (node (ref U7) (pin 19))
      (node (ref U8) (pin 19))
      (node (ref JAB1) (pin 27))
      (node (ref U6) (pin 19))
      (node (ref U4) (pin 45)))
    (net (code 71) (name ~AD25_3V3)
      (node (ref JAB1) (pin 25))
      (node (ref U5) (pin 12)))
    (net (code 72) (name ~AD27_3V3)
      (node (ref JAB1) (pin 23))
      (node (ref U5) (pin 14)))
    (net (code 73) (name ~AD29_3V3)
      (node (ref JAB1) (pin 21))
      (node (ref U5) (pin 16)))
    (net (code 74) (name FPGA_JTAG_TCK)
      (node (ref JAB1) (pin 62))
      (node (ref J1) (pin 6)))
    (net (code 75) (name USBH0_D-)
      (node (ref JAB1) (pin 60))
      (node (ref R23) (pin 2)))
    (net (code 76) (name ~NMRQ_3V3)
      (node (ref U1) (pin 1))
      (node (ref JAB1) (pin 6))
      (node (ref R36) (pin 2)))
    (net (code 77) (name ~AD0_3V3)
      (node (ref JAB1) (pin 58))
      (node (ref D16) (pin 1))
      (node (ref U8) (pin 12)))
    (net (code 78) (name ~AD2_3V3)
      (node (ref U8) (pin 14))
      (node (ref JAB1) (pin 56)))
    (net (code 79) (name ~AD4_3V3)
      (node (ref JAB1) (pin 54))
      (node (ref U8) (pin 16)))
    (net (code 80) (name ~AD6_3V3)
      (node (ref JAB1) (pin 52))
      (node (ref U8) (pin 18)))
    (net (code 81) (name ~AD8_3V3)
      (node (ref JAB1) (pin 50))
      (node (ref U7) (pin 12)))
    (net (code 82) (name ~AD10_3V3)
      (node (ref JAB1) (pin 48))
      (node (ref U7) (pin 14)))
    (net (code 83) (name ~AD12_3V3)
      (node (ref JAB1) (pin 46))
      (node (ref U7) (pin 16)))
    (net (code 84) (name ~AD14_3V3)
      (node (ref JAB1) (pin 44))
      (node (ref U7) (pin 18)))
    (net (code 85) (name ~AD16_3V3)
      (node (ref JAB1) (pin 42))
      (node (ref U6) (pin 12)))
    (net (code 86) (name ~AD18_3V3)
      (node (ref JAB1) (pin 40))
      (node (ref U6) (pin 14)))
    (net (code 87) (name ~AD20_3V3)
      (node (ref U6) (pin 16))
      (node (ref JAB1) (pin 38)))
    (net (code 88) (name ~AD22_3V3)
      (node (ref U6) (pin 18))
      (node (ref JAB1) (pin 36)))
    (net (code 89) (name ~AD24_3V3)
      (node (ref U5) (pin 11))
      (node (ref JAB1) (pin 28)))
    (net (code 90) (name ~AD26_3V3)
      (node (ref U5) (pin 13))
      (node (ref JAB1) (pin 26)))
    (net (code 91) (name ~AD28_3V3)
      (node (ref U5) (pin 15))
      (node (ref JAB1) (pin 24)))
    (net (code 92) (name ~AD30_3V3)
      (node (ref U5) (pin 17))
      (node (ref JAB1) (pin 22)))
    (net (code 93) (name ~CLK_3V3)
      (node (ref JAB1) (pin 20))
      (node (ref U4) (pin 47)))
    (net (code 94) (name ~RESET_3V3)
      (node (ref JAB1) (pin 17))
      (node (ref D10) (pin 1))
      (node (ref U4) (pin 48)))
    (net (code 95) (name NUBUS_MASTER_DIR)
      (node (ref JAB1) (pin 15))
      (node (ref U4) (pin 49)))
    (net (code 96) (name "Net-(JCD1-Pad2)")
      (node (ref JCD1) (pin 2)))
    (net (code 97) (name FPGA_VGA_HS)
      (node (ref JCD1) (pin 20))
      (node (ref R34) (pin 1)))
    (net (code 98) (name GND)
      (node (ref C18) (pin 2))
      (node (ref U8) (pin 10))
      (node (ref U7) (pin 10))
      (node (ref J4) (pin b18))
      (node (ref J4) (pin a22))
      (node (ref J4) (pin a23))
      (node (ref J4) (pin b12))
      (node (ref J4) (pin c22))
      (node (ref J4) (pin b13))
      (node (ref J4) (pin b14))
      (node (ref C14) (pin 2))
      (node (ref J4) (pin b15))
      (node (ref J4) (pin b16))
      (node (ref J4) (pin b17))
      (node (ref C19) (pin 2))
      (node (ref J4) (pin b19))
      (node (ref J4) (pin b31))
      (node (ref J4) (pin b30))
      (node (ref J4) (pin b3))
      (node (ref J4) (pin b23))
      (node (ref J4) (pin b22))
      (node (ref J4) (pin b21))
      (node (ref J4) (pin b20))
      (node (ref J4) (pin b2))
      (node (ref U5) (pin 10))
      (node (ref J4) (pin c31))
      (node (ref R24) (pin 1))
      (node (ref J6) (pin 5))
      (node (ref U11) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref U12) (pin 33))
      (node (ref U12) (pin 12))
      (node (ref U12) (pin 31))
      (node (ref U12) (pin 40))
      (node (ref U12) (pin 2))
      (node (ref U12) (pin 1))
      (node (ref R25) (pin 2))
      (node (ref U9) (pin 19))
      (node (ref C26) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref U10) (pin 2))
      (node (ref U10) (pin 5))
      (node (ref J5) (pin 17))
      (node (ref J5) (pin 8))
      (node (ref J5) (pin 5))
      (node (ref J5) (pin 2))
      (node (ref J8) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref J5) (pin 11))
      (node (ref C29) (pin 2))
      (node (ref J7) (pin 3))
      (node (ref J7) (pin 1))
      (node (ref U9) (pin 14))
      (node (ref U9) (pin 6))
      (node (ref U12) (pin 14))
      (node (ref C21) (pin 2))
      (node (ref C20) (pin 2))
      (node (ref J9) (pin 6))
      (node (ref C32) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref J9) (pin 8))
      (node (ref J9) (pin 7))
      (node (ref C36) (pin 2))
      (node (ref J9) (pin 5))
      (node (ref J9) (pin 10))
      (node (ref R28) (pin 2))
      (node (ref U12) (pin 39))
      (node (ref R30) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref R32) (pin 1))
      (node (ref U6) (pin 10))
      (node (ref C7) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref R33) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref U13) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref U12) (pin 27))
      (node (ref U12) (pin 26))
      (node (ref U12) (pin 25))
      (node (ref C38) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref U12) (pin 15))
      (node (ref J1) (pin 13))
      (node (ref J1) (pin 9))
      (node (ref J1) (pin 7))
      (node (ref J1) (pin 5))
      (node (ref J1) (pin 1))
      (node (ref J1) (pin 11))
      (node (ref JCD1) (pin 34))
      (node (ref J1) (pin 3))
      (node (ref C13) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref U3) (pin 5))
      (node (ref U3) (pin 9))
      (node (ref U3) (pin 12))
      (node (ref U3) (pin 7))
      (node (ref U4) (pin 41))
      (node (ref U4) (pin 21))
      (node (ref JCD1) (pin 64))
      (node (ref JCD1) (pin 4))
      (node (ref U1) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 7))
      (node (ref C4) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U4) (pin 54))
      (node (ref U4) (pin 14))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 7))
      (node (ref C5) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref J2) (pin 9))
      (node (ref J2) (pin 7))
      (node (ref J2) (pin 5))
      (node (ref C3) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref J2) (pin 3))
      (node (ref JAB1) (pin 32))
      (node (ref J2) (pin 13))
      (node (ref J3) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref J2) (pin 11))
      (node (ref JCD1) (pin 63))
      (node (ref JAB1) (pin 64))
      (node (ref JCD1) (pin 3))
      (node (ref JCD1) (pin 33))
      (node (ref JAB1) (pin 3))
      (node (ref JAB1) (pin 31))
      (node (ref JAB1) (pin 4)))
    (net (code 99) (name FPGA_R3)
      (node (ref U12) (pin 44))
      (node (ref JCD1) (pin 44)))
    (net (code 100) (name ~ID1_3V3)
      (node (ref U4) (pin 60))
      (node (ref D12) (pin 1))
      (node (ref JCD1) (pin 10)))
    (net (code 101) (name ~ID2_3V3)
      (node (ref U4) (pin 63))
      (node (ref D13) (pin 1))
      (node (ref JCD1) (pin 8)))
    (net (code 102) (name FPGA_JTAG_TMS)
      (node (ref J1) (pin 4))
      (node (ref JCD1) (pin 62)))
    (net (code 103) (name FPGA_G3)
      (node (ref JCD1) (pin 60))
      (node (ref U12) (pin 6)))
    (net (code 104) (name FPGA_G2)
      (node (ref U12) (pin 5))
      (node (ref JCD1) (pin 58)))
    (net (code 105) (name FPGA_G1)
      (node (ref U12) (pin 4))
      (node (ref JCD1) (pin 56)))
    (net (code 106) (name FPGA_G0)
      (node (ref JCD1) (pin 54))
      (node (ref U12) (pin 3)))
    (net (code 107) (name FPGA_R7)
      (node (ref U12) (pin 48))
      (node (ref JCD1) (pin 52)))
    (net (code 108) (name FPGA_R6)
      (node (ref U12) (pin 47))
      (node (ref JCD1) (pin 50)))
    (net (code 109) (name FPGA_R5)
      (node (ref JCD1) (pin 48))
      (node (ref U12) (pin 46)))
    (net (code 110) (name FPGA_R4)
      (node (ref U12) (pin 45))
      (node (ref JCD1) (pin 46)))
    (net (code 111) (name FPGA_R2)
      (node (ref U12) (pin 43))
      (node (ref JCD1) (pin 42)))
    (net (code 112) (name FPGA_R1)
      (node (ref U12) (pin 42))
      (node (ref JCD1) (pin 40)))
    (net (code 113) (name FPGA_R0)
      (node (ref U12) (pin 41))
      (node (ref JCD1) (pin 38)))
    (net (code 114) (name HDMI_D2+)
      (node (ref JCD1) (pin 30))
      (node (ref U9) (pin 23))
      (node (ref J5) (pin 1)))
    (net (code 115) (name HDMI_D2-)
      (node (ref JCD1) (pin 28))
      (node (ref U9) (pin 22))
      (node (ref J5) (pin 3)))
    (net (code 116) (name HDMI_D0+)
      (node (ref U9) (pin 18))
      (node (ref J5) (pin 7))
      (node (ref JCD1) (pin 26)))
    (net (code 117) (name HDMI_D0-)
      (node (ref JCD1) (pin 24))
      (node (ref J5) (pin 9))
      (node (ref U9) (pin 17)))
    (net (code 118) (name FPGA_VGA_VS)
      (node (ref JCD1) (pin 22))
      (node (ref R35) (pin 1)))
    (net (code 119) (name LED1)
      (node (ref JCD1) (pin 14))
      (node (ref R2) (pin 1)))
    (net (code 120) (name LED0)
      (node (ref R1) (pin 1))
      (node (ref JCD1) (pin 12)))
    (net (code 121) (name ~CLK2X_3V3)
      (node (ref U4) (pin 58))
      (node (ref JCD1) (pin 16)))
    (net (code 122) (name ~TM2_3V3)
      (node (ref JCD1) (pin 18))
      (node (ref U4) (pin 57)))
    (net (code 123) (name FPGA_JTAG_TDI)
      (node (ref J1) (pin 10))
      (node (ref JAB1) (pin 61)))
    (net (code 124) (name /B2B/JTAG_VIO)
      (node (ref J1) (pin 2)))
    (net (code 125) (name "Net-(D5-Pad2)")
      (node (ref D5) (pin 2))
      (node (ref R10) (pin 2)))
    (net (code 126) (name "Net-(D4-Pad2)")
      (node (ref R9) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 127) (name "Net-(D8-Pad2)")
      (node (ref D8) (pin 2))
      (node (ref R13) (pin 2)))
    (net (code 128) (name "Net-(D9-Pad2)")
      (node (ref R14) (pin 2))
      (node (ref D9) (pin 2)))
    (net (code 129) (name "Net-(D15-Pad2)")
      (node (ref R20) (pin 2))
      (node (ref D15) (pin 2)))
    (net (code 130) (name "Net-(D16-Pad2)")
      (node (ref D16) (pin 2))
      (node (ref R21) (pin 2)))
    (net (code 131) (name ~ARB0_5V)
      (node (ref U4) (pin 34))
      (node (ref J4) (pin c24))
      (node (ref U3) (pin 3)))
    (net (code 132) (name ~ARB1_5V)
      (node (ref J4) (pin a24))
      (node (ref U4) (pin 36))
      (node (ref U3) (pin 6)))
    (net (code 133) (name ~ARB3_5V)
      (node (ref U4) (pin 32))
      (node (ref U3) (pin 8))
      (node (ref J4) (pin a25)))
    (net (code 134) (name ~ARB2_5V)
      (node (ref U4) (pin 27))
      (node (ref U3) (pin 11))
      (node (ref J4) (pin c25)))
    (net (code 135) (name "Net-(D6-Pad2)")
      (node (ref R11) (pin 2))
      (node (ref D6) (pin 2)))
    (net (code 136) (name "Net-(D7-Pad2)")
      (node (ref R12) (pin 2))
      (node (ref D7) (pin 2)))
    (net (code 137) (name "Net-(D11-Pad2)")
      (node (ref D11) (pin 2))
      (node (ref R16) (pin 2)))
    (net (code 138) (name "Net-(D12-Pad2)")
      (node (ref R17) (pin 2))
      (node (ref D12) (pin 2)))
    (net (code 139) (name "Net-(D13-Pad2)")
      (node (ref D13) (pin 2))
      (node (ref R18) (pin 2)))
    (net (code 140) (name "Net-(D14-Pad2)")
      (node (ref R19) (pin 2))
      (node (ref D14) (pin 2)))
    (net (code 141) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 142) (name TM0_n_o)
      (node (ref U2) (pin 5))
      (node (ref U4) (pin 42)))
    (net (code 143) (name ~TM1_5V)
      (node (ref U4) (pin 38))
      (node (ref J4) (pin a5))
      (node (ref U2) (pin 3)))
    (net (code 144) (name ~TM0_5V)
      (node (ref J4) (pin c5))
      (node (ref U2) (pin 6))
      (node (ref U4) (pin 39)))
    (net (code 145) (name TMx_oe_n)
      (node (ref R40) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 1))
      (node (ref U4) (pin 43)))
    (net (code 146) (name TM1_n_o)
      (node (ref U4) (pin 40))
      (node (ref U2) (pin 2)))
    (net (code 147) (name ~TM2_5V)
      (node (ref J4) (pin b8))
      (node (ref U4) (pin 22))
      (node (ref U2) (pin 8)))
    (net (code 148) (name "Net-(D10-Pad2)")
      (node (ref D10) (pin 2))
      (node (ref R15) (pin 2)))
    (net (code 149) (name ~NMRQ_5V)
      (node (ref J4) (pin a31))
      (node (ref U1) (pin 3)))
    (net (code 150) (name ~RQST_5V)
      (node (ref U1) (pin 6))
      (node (ref U4) (pin 6))
      (node (ref J4) (pin a30)))
    (net (code 151) (name START_oe_n)
      (node (ref U1) (pin 10))
      (node (ref U4) (pin 11))
      (node (ref R38) (pin 2)))
    (net (code 152) (name ~START_5V)
      (node (ref U4) (pin 13))
      (node (ref U1) (pin 8))
      (node (ref J4) (pin c28)))
    (net (code 153) (name START_o_n)
      (node (ref U1) (pin 9))
      (node (ref U4) (pin 12)))
    (net (code 154) (name ~ACK_5V)
      (node (ref U4) (pin 10))
      (node (ref J4) (pin a28))
      (node (ref U1) (pin 11)))
    (net (code 155) (name ACK_o_n)
      (node (ref U4) (pin 9))
      (node (ref U1) (pin 12)))
    (net (code 156) (name ACK_oe_n)
      (node (ref R39) (pin 2))
      (node (ref U4) (pin 8))
      (node (ref U1) (pin 13)))
    (net (code 157) (name ARB0_o_n)
      (node (ref U3) (pin 1))
      (node (ref R42) (pin 2))
      (node (ref U4) (pin 33)))
    (net (code 158) (name TM2_oe_n)
      (node (ref U2) (pin 10))
      (node (ref U4) (pin 24))
      (node (ref R41) (pin 2)))
    (net (code 159) (name ARB2_o_n)
      (node (ref U4) (pin 25))
      (node (ref U3) (pin 13))
      (node (ref R44) (pin 2)))
    (net (code 160) (name ARB1_o_n)
      (node (ref U4) (pin 35))
      (node (ref R43) (pin 2))
      (node (ref U3) (pin 4)))
    (net (code 161) (name ~CLK_5V)
      (node (ref J4) (pin c32))
      (node (ref U4) (pin 16)))
    (net (code 162) (name TM2_o_n)
      (node (ref U4) (pin 46))
      (node (ref U2) (pin 9)))
    (net (code 163) (name RQST_o_n)
      (node (ref U1) (pin 4))
      (node (ref R37) (pin 2))
      (node (ref U4) (pin 5)))
    (net (code 164) (name ARB3_o_n)
      (node (ref U4) (pin 31))
      (node (ref U3) (pin 10))
      (node (ref R45) (pin 2)))
    (net (code 165) (name +12V)
      (node (ref J4) (pin a32))
      (node (ref J4) (pin b32)))
    (net (code 166) (name ~AD31_5V)
      (node (ref U5) (pin 2))
      (node (ref J4) (pin a21)))
    (net (code 167) (name ~ID1_5V)
      (node (ref U4) (pin 19))
      (node (ref J4) (pin a26))
      (node (ref R6) (pin 2)))
    (net (code 168) (name ~ID3_5V)
      (node (ref J4) (pin a27))
      (node (ref R8) (pin 1))
      (node (ref U4) (pin 7)))
    (net (code 169) (name ~SPV_5V)
      (node (ref J4) (pin a3)))
    (net (code 170) (name ~SP_5V)
      (node (ref J4) (pin a4)))
    (net (code 171) (name ~AD29_5V)
      (node (ref J4) (pin a20))
      (node (ref U5) (pin 4)))
    (net (code 172) (name ~AD1_5V)
      (node (ref U8) (pin 9))
      (node (ref J4) (pin a6)))
    (net (code 173) (name ~AD3_5V)
      (node (ref J4) (pin a7))
      (node (ref U8) (pin 7)))
    (net (code 174) (name ~AD5_5V)
      (node (ref J4) (pin a8))
      (node (ref U8) (pin 5)))
    (net (code 175) (name ~AD7_5V)
      (node (ref J4) (pin a9))
      (node (ref U8) (pin 3)))
    (net (code 176) (name ~CM1_5V)
      (node (ref J4) (pin b10)))
    (net (code 177) (name ~CM2_5V)
      (node (ref J4) (pin b11)))
    (net (code 178) (name -12V)
      (node (ref J4) (pin b1))
      (node (ref J4) (pin a1)))
    (net (code 179) (name ~AD9_5V)
      (node (ref U7) (pin 9))
      (node (ref J4) (pin a10)))
    (net (code 180) (name ~AD11_5V)
      (node (ref U7) (pin 7))
      (node (ref J4) (pin a11)))
    (net (code 181) (name ~AD13_5V)
      (node (ref U7) (pin 5))
      (node (ref J4) (pin a12)))
    (net (code 182) (name ~AD15_5V)
      (node (ref J4) (pin a13))
      (node (ref U7) (pin 3)))
    (net (code 183) (name ~AD17_5V)
      (node (ref J4) (pin a14))
      (node (ref U6) (pin 9)))
    (net (code 184) (name ~AD19_5V)
      (node (ref J4) (pin a15))
      (node (ref U6) (pin 7)))
    (net (code 185) (name ~AD21_5V)
      (node (ref J4) (pin a16))
      (node (ref U6) (pin 5)))
    (net (code 186) (name ~AD23_5V)
      (node (ref J4) (pin a17))
      (node (ref U6) (pin 3)))
    (net (code 187) (name ~AD25_5V)
      (node (ref J4) (pin a18))
      (node (ref U5) (pin 8)))
    (net (code 188) (name ~AD27_5V)
      (node (ref U5) (pin 6))
      (node (ref J4) (pin a19)))
    (net (code 189) (name SB0_5V)
      (node (ref J4) (pin a2)))
    (net (code 190) (name ~AD24_5V)
      (node (ref J4) (pin c18))
      (node (ref U5) (pin 9)))
    (net (code 191) (name ~AD26_5V)
      (node (ref J4) (pin c19))
      (node (ref U5) (pin 7)))
    (net (code 192) (name SB1_5V)
      (node (ref J4) (pin c2)))
    (net (code 193) (name ~AD28_5V)
      (node (ref U5) (pin 5))
      (node (ref J4) (pin c20)))
    (net (code 194) (name ~AD30_5V)
      (node (ref U5) (pin 3))
      (node (ref J4) (pin c21)))
    (net (code 195) (name ~PFW_5V)
      (node (ref J4) (pin c23)))
    (net (code 196) (name ~ID0_5V)
      (node (ref U4) (pin 20))
      (node (ref R5) (pin 2))
      (node (ref J4) (pin c26)))
    (net (code 197) (name ~ID2_5V)
      (node (ref R7) (pin 2))
      (node (ref J4) (pin c27))
      (node (ref U4) (pin 18)))
    (net (code 198) (name ~AD22_5V)
      (node (ref U6) (pin 2))
      (node (ref J4) (pin c17)))
    (net (code 199) (name ~AD0_5V)
      (node (ref J4) (pin c6))
      (node (ref U8) (pin 8)))
    (net (code 200) (name ~AD2_5V)
      (node (ref U8) (pin 6))
      (node (ref J4) (pin c7)))
    (net (code 201) (name ~AD4_5V)
      (node (ref J4) (pin c8))
      (node (ref U8) (pin 4)))
    (net (code 202) (name ~AD6_5V)
      (node (ref U8) (pin 2))
      (node (ref J4) (pin c9)))
    (net (code 203) (name ~CLK2X_5V)
      (node (ref U4) (pin 17))
      (node (ref J4) (pin b24)))
    (net (code 204) (name STDBYPWR)
      (node (ref J4) (pin b25)))
    (net (code 205) (name ~CLK2XEN_5V)
      (node (ref J4) (pin b26)))
    (net (code 206) (name ~CBUSY_5V)
      (node (ref J4) (pin b27)))
    (net (code 207) (name ~CM0_5V)
      (node (ref J4) (pin b9)))
    (net (code 208) (name ~RESET_5V)
      (node (ref U4) (pin 44))
      (node (ref J4) (pin c1)))
    (net (code 209) (name ~AD8_5V)
      (node (ref J4) (pin c10))
      (node (ref U7) (pin 8)))
    (net (code 210) (name ~AD10_5V)
      (node (ref U7) (pin 6))
      (node (ref J4) (pin c11)))
    (net (code 211) (name ~AD12_5V)
      (node (ref U7) (pin 4))
      (node (ref J4) (pin c12)))
    (net (code 212) (name ~AD14_5V)
      (node (ref U7) (pin 2))
      (node (ref J4) (pin c13)))
    (net (code 213) (name ~AD16_5V)
      (node (ref J4) (pin c14))
      (node (ref U6) (pin 8)))
    (net (code 214) (name ~AD18_5V)
      (node (ref J4) (pin c15))
      (node (ref U6) (pin 6)))
    (net (code 215) (name ~AD20_5V)
      (node (ref U6) (pin 4))
      (node (ref J4) (pin c16)))
    (net (code 216) (name /vga/VGA_HS)
      (node (ref R34) (pin 2)))
    (net (code 217) (name /vga/VGA_VS)
      (node (ref R35) (pin 2)))
    (net (code 218) (name SHIELD)
      (node (ref J6) (pin 6))
      (node (ref J5) (pin SH))
      (node (ref J9) (pin 0))
      (node (ref R33) (pin 1))
      (node (ref C39) (pin 1)))
    (net (code 219) (name "Net-(J9-Pad11)")
      (node (ref J9) (pin 11)))
    (net (code 220) (name "Net-(J9-Pad12)")
      (node (ref J9) (pin 12)))
    (net (code 221) (name "Net-(J9-Pad15)")
      (node (ref J9) (pin 15)))
    (net (code 222) (name "Net-(J9-Pad4)")
      (node (ref J9) (pin 4)))
    (net (code 223) (name "Net-(J9-Pad9)")
      (node (ref J9) (pin 9)))
    (net (code 224) (name /vga/comp)
      (node (ref U12) (pin 35))
      (node (ref C31) (pin 1)))
    (net (code 225) (name /vga/VGA_B)
      (node (ref J9) (pin 3)))
    (net (code 226) (name /vga/VGA_G)
      (node (ref J9) (pin 2)))
    (net (code 227) (name /vga/VGA_VS)
      (node (ref J9) (pin 14)))
    (net (code 228) (name /vga/VGA_HS)
      (node (ref J9) (pin 13)))
    (net (code 229) (name /vga/VGA_R)
      (node (ref J9) (pin 1)))
    (net (code 230) (name /vga/rset)
      (node (ref R28) (pin 1))
      (node (ref U12) (pin 37)))
    (net (code 231) (name /vga/VGA_R)
      (node (ref R30) (pin 2)))
    (net (code 232) (name /vga/VGA_G)
      (node (ref R31) (pin 2)))
    (net (code 233) (name /vga/VGA_B)
      (node (ref R32) (pin 2)))
    (net (code 234) (name /vga/vref)
      (node (ref R29) (pin 2))
      (node (ref C37) (pin 1))
      (node (ref U12) (pin 36))
      (node (ref U13) (pin 1)))
    (net (code 235) (name /vga/VGA_B)
      (node (ref U12) (pin 28)))
    (net (code 236) (name "Net-(U13-Pad3)")
      (node (ref U13) (pin 3)))
    (net (code 237) (name /vga/VGA_R)
      (node (ref U12) (pin 34)))
    (net (code 238) (name /vga/VGA_G)
      (node (ref U12) (pin 32)))
    (net (code 239) (name /usb/USB_D-)
      (node (ref U10) (pin 6))
      (node (ref R25) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 240) (name +5V)
      (node (ref J4) (pin b28))
      (node (ref J4) (pin b29))
      (node (ref J4) (pin c4))
      (node (ref J4) (pin c3))
      (node (ref J4) (pin c29))
      (node (ref JAB1) (pin 1))
      (node (ref J4) (pin b6))
      (node (ref J4) (pin c30))
      (node (ref C3) (pin 1))
      (node (ref R27) (pin 2))
      (node (ref C28) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref J7) (pin 2))
      (node (ref J4) (pin b4))
      (node (ref J4) (pin b5))
      (node (ref J4) (pin b7))
      (node (ref R8) (pin 2))
      (node (ref U9) (pin 11))
      (node (ref U11) (pin 5))
      (node (ref R26) (pin 2))
      (node (ref C23) (pin 1))
      (node (ref JAB1) (pin 2))
      (node (ref J4) (pin a29))
      (node (ref C26) (pin 1)))
    (net (code 241) (name /usb/USB_D+)
      (node (ref J6) (pin 3))
      (node (ref U10) (pin 4))
      (node (ref R22) (pin 1))
      (node (ref R24) (pin 2)))
    (net (code 242) (name "Net-(U10-Pad1)")
      (node (ref U10) (pin 1)))
    (net (code 243) (name "Net-(U10-Pad3)")
      (node (ref U10) (pin 3)))
    (net (code 244) (name "Net-(J6-Pad4)")
      (node (ref J6) (pin 4)))
    (net (code 245) (name /usb/USB_EN)
      (node (ref R26) (pin 1))
      (node (ref U11) (pin 4)))
    (net (code 246) (name /usb/USB_FLT)
      (node (ref R27) (pin 1))
      (node (ref U11) (pin 3)))
    (net (code 247) (name /usb/VBus)
      (node (ref FB1) (pin 1))
      (node (ref U11) (pin 1))
      (node (ref C27) (pin 1)))
    (net (code 248) (name /usb/VBus_USB0)
      (node (ref C25) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref FB1) (pin 2)))
    (net (code 249) (name /hdmi/scl_b)
      (node (ref U9) (pin 8))
      (node (ref J5) (pin 15)))
    (net (code 250) (name /hdmi/sda_b)
      (node (ref U9) (pin 9))
      (node (ref J5) (pin 16)))
    (net (code 251) (name /hdmi/cec_b)
      (node (ref J5) (pin 13))
      (node (ref U9) (pin 7)))
    (net (code 252) (name /hdmi/hpd_b)
      (node (ref U9) (pin 10))
      (node (ref J5) (pin 19)))
    (net (code 253) (name HDMI_5V)
      (node (ref C24) (pin 1))
      (node (ref U9) (pin 13))
      (node (ref J5) (pin 18)))
    (net (code 254) (name "Net-(J5-Pad14)")
      (node (ref J5) (pin 14)))))