(export (version D)
  (design
    (source /home/dolbeau/SPARC/SBusFPGA/VGA222-PMOD/VGA222-PMOD.sch)
    (date "Sun Sep 12 12:31:19 2021")
    (tool "Eeschema 5.0.2+dfsg1-1~bpo9+1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source VGA222-PMOD.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J2)
      (value Conn_02x06_Odd_Even)
      (footprint Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name MPN) A2541WR-2x6P))
      (libsource (lib Connector_Generic) (part Conn_02x06_Odd_Even) (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0BFDF9))
    (comp (ref J1)
      (value DB15_Female_HighDensity_MountingHoles)
      (footprint For_SeeedStudio:L77HDE15SD1CH4RHNVGA)
      (datasheet " ~")
      (fields
        (field (name MPN) L77HDE15SD1CH4RHNVGA)
        (field (name URL) https://www.mouser.fr/ProductDetail/Amphenol-Commercial-Products/L77HDE15SD1CH4RHNVGA?qs=f9yNj16SXrKPVxRw%2FcVQYg==))
      (libsource (lib Connector) (part DB15_Female_HighDensity_MountingHoles) (description "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole"))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E1796))
    (comp (ref R12)
      (value 510)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR-25FTE52-510R))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E31B9))
    (comp (ref R13)
      (value 1k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR-25FTE52-1K))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E3877))
    (comp (ref R18)
      (value 510)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR-25FTE52-510R))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E5CB1))
    (comp (ref R19)
      (value 1k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR-25FTE52-1K))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E5CC1))
    (comp (ref R24)
      (value 510)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR-25FTE52-510R))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E5EC0))
    (comp (ref R25)
      (value 1k)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR-25FTE52-1K))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E5ED0))
    (comp (ref R10)
      (value 100)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) "MFR-25FTE52-100R "))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E8BD6))
    (comp (ref R11)
      (value 100)
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) "MFR-25FTE52-100R "))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613E90B1))
    (comp (ref R9)
      (value "1M (5% .25W)")
      (footprint Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) MFR50SFTE52-1M)
        (field (name URL) https://www.lcsc.com/product-detail/Chip-Resistor-Surface-Mount_UNI-ROYAL-Uniroyal-Elec-AS03W4J0105T5E_C966202.html))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 613DBDAB))
    (comp (ref C3)
      (value "1nF (250V)")
      (footprint Capacitor_THT:CP_Radial_D6.3mm_P2.50mm)
      (datasheet ~)
      (fields
        (field (name MPN) 860021373002))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 613DBE4A)))
  (libparts
    (libpart (lib Connector) (part DB15_Female_HighDensity_MountingHoles)
      (description "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole")
      (docs " ~")
      (footprints
        (fp DSUB*Female*))
      (fields
        (field (name Reference) J)
        (field (name Value) DB15_Female_HighDensity_MountingHoles))
      (pins
        (pin (num 0) (name ~) (type passive))
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num 13) (name ~) (type passive))
        (pin (num 14) (name ~) (type passive))
        (pin (num 15) (name ~) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref J1) (pin 8))
      (node (ref J1) (pin 10))
      (node (ref R9) (pin 2))
      (node (ref J1) (pin 5))
      (node (ref J1) (pin 7))
      (node (ref C3) (pin 2))
      (node (ref J1) (pin 6))
      (node (ref J2) (pin 3))
      (node (ref J2) (pin 4)))
    (net (code 2) (name "Net-(J1-Pad15)")
      (node (ref J1) (pin 15)))
    (net (code 3) (name "Net-(J1-Pad12)")
      (node (ref J1) (pin 12)))
    (net (code 4) (name "Net-(J1-Pad11)")
      (node (ref J1) (pin 11)))
    (net (code 5) (name "Net-(J1-Pad9)")
      (node (ref J1) (pin 9)))
    (net (code 6) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 7) (name B2)
      (node (ref J2) (pin 8))
      (node (ref R25) (pin 2)))
    (net (code 8) (name B3)
      (node (ref J2) (pin 7))
      (node (ref R24) (pin 2)))
    (net (code 9) (name VGA_B)
      (node (ref R24) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref R25) (pin 1)))
    (net (code 10) (name G2)
      (node (ref J2) (pin 10))
      (node (ref R19) (pin 2)))
    (net (code 11) (name "Net-(C3-Pad1)")
      (node (ref J1) (pin 0))
      (node (ref C3) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 12) (name G3)
      (node (ref R18) (pin 2))
      (node (ref J2) (pin 9)))
    (net (code 13) (name HS)
      (node (ref R11) (pin 1))
      (node (ref J2) (pin 6)))
    (net (code 14) (name VS)
      (node (ref J2) (pin 5))
      (node (ref R10) (pin 1)))
    (net (code 15) (name +3V3)
      (node (ref J2) (pin 2))
      (node (ref J2) (pin 1)))
    (net (code 16) (name R2)
      (node (ref J2) (pin 12))
      (node (ref R13) (pin 2)))
    (net (code 17) (name R3)
      (node (ref R12) (pin 2))
      (node (ref J2) (pin 11)))
    (net (code 18) (name VGA_G)
      (node (ref J1) (pin 2))
      (node (ref R19) (pin 1))
      (node (ref R18) (pin 1)))
    (net (code 19) (name VGA_VS)
      (node (ref J1) (pin 14))
      (node (ref R11) (pin 2)))
    (net (code 20) (name VGA_HS)
      (node (ref J1) (pin 13))
      (node (ref R10) (pin 2)))
    (net (code 21) (name VGA_R)
      (node (ref R12) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref J1) (pin 1)))))