(export (version D)
  (design
    (source /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/sbus-to-ztex.sch)
    (date "Sat Aug 28 17:38:05 2021")
    (tool "Eeschema 5.0.2+dfsg1-1~bpo9+1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "sbus-to-ztex root")
        (company)
        (rev)
        (date)
        (source sbus-to-ztex.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /sbus/) (tstamps /5F679B53/)
      (title_block
        (title "sbus-to-ztex SBus connection & level shifting")
        (company)
        (rev)
        (date)
        (source sbus.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /B2B/) (tstamps /5F67E4B9/)
      (title_block
        (title "sbus-to-ztex B2B connector")
        (company)
        (rev)
        (date)
        (source B2B.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /blinkey/) (tstamps /5F6B165A/)
      (title_block
        (title "sbus-to-ztex blinkey stuff")
        (company)
        (rev)
        (date)
        (source blinkey.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /sdcard.sch/) (tstamps /5F69F4EF/)
      (title_block
        (title "sbus-to-ztex sdcard")
        (company)
        (rev)
        (date)
        (source sdcard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /USB/) (tstamps /60D72F2C/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source usb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref SBus1)
      (value SBus)
      (footprint FCN-234P096-GY:FCN-234P096-GY)
      (datasheet https://www.mouser.com/datasheet/2/164/fcn230-3978.pdf)
      (fields
        (field (name MPN) FCN-234P096-G/Y)
        (field (name Mouser) "817-FCN-234P096-G/Y ")
        (field (name URL) https://www2.mouser.com/ProductDetail/Fujitsu/FCN-234P096-G-Y?qs=%2Fha2pyFadugZ9WCm2lJ8CZdXc85UARoDXS81raJopvR1w4UDuaXlcQ%3D%3D)
        (field (name bom_link) https://www2.mouser.com/ProductDetail/Fujitsu/FCN-234P096-G-Y?qs=uqct%252BzVq%2FBfM88%2F7KmJJ2Q%3D%3D))
      (libsource (lib SBUS) (part SBus) (description ""))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F5F6249))
    (comp (ref C31)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F78E71D))
    (comp (ref R30)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F741B09))
    (comp (ref R31)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F74D6C5))
    (comp (ref U_INT1)
      (value 74LVC2G07)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet https://www.diodes.com/assets/Datasheets/74LVC2G07.pdf)
      (fields
        (field (name MPN) SN74LVC2G07DBVR))
      (libsource (lib 74xGxx) (part 74AUC2G07) (description "Dual Buffer w/ Open Drain, Low-Voltage CMOS"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F74F1CF))
    (comp (ref C10)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F815217))
    (comp (ref U1)
      (value SN74CB3T16211DGGR)
      (footprint For_SeeedStudio:TSSOP-56_6.1x14mm_P0.5mm_For_SeeedStudio)
      (datasheet https://www.ti.com/lit/ds/symlink/sn74cb3t16211.pdf)
      (fields
        (field (name MPN) SN74CB3T16211DGGR))
      (libsource (lib ul_SN74CB3T16211DGGR) (part SN74CB3T16211DGGR) (description ""))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F80E30A))
    (comp (ref C11)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F8CA5C6))
    (comp (ref U2)
      (value SN74CB3T16211DGGR)
      (footprint For_SeeedStudio:TSSOP-56_6.1x14mm_P0.5mm_For_SeeedStudio)
      (fields
        (field (name MPN) SN74CB3T16211DGGR))
      (libsource (lib ul_SN74CB3T16211DGGR) (part SN74CB3T16211DGGR) (description ""))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F8CA5E7))
    (comp (ref C12)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC60KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F8F42D1))
    (comp (ref U3)
      (value SN74CB3T16211DGGR)
      (footprint For_SeeedStudio:TSSOP-56_6.1x14mm_P0.5mm_For_SeeedStudio)
      (fields
        (field (name MPN) SN74CB3T16211DGGR)
        (field (name URL) https://lcsc.com/product-detail/Signal-Switches-Encoders-Decoders-Multiplexers_Texas-Instruments-SN74CB3T16211DGGR_C2653275.html)
        (field (name URL-alt) https://www.mouser.fr/ProductDetail/Texas-Instruments/SN74CB3T16211DGGR?qs=%2Fha2pyFadujLgV8PJqueL5aUGpX9%252BbECTuUAq6EU8VAiPml4qcD9lw%3D%3D))
      (libsource (lib ul_SN74CB3T16211DGGR) (part SN74CB3T16211DGGR) (description ""))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F8F42F3))
    (comp (ref C13)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F91A4F0))
    (comp (ref R13)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F93CF72))
    (comp (ref U4)
      (value SN74CB3T3125PW)
      (footprint Package_SO:TSSOP-14_4.4x5mm_P0.65mm)
      (datasheet https://www.ti.com/lit/ds/symlink/sn74cb3t3125.pdf)
      (fields
        (field (name MPN) SN74CB3T3125PW))
      (libsource (lib ul_SN74CB3T3125PW) (part SN74CB3T3125PW) (description ""))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 5F9151C4))
    (comp (ref C4)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 60DE399B))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 60DE39A4))
    (comp (ref R2)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 60DE39AC))
    (comp (ref U_INT2)
      (value 74LVC2G07)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet https://www.diodes.com/assets/Datasheets/74LVC2G07.pdf)
      (fields
        (field (name MPN) SN74LVC2G07DBVR))
      (libsource (lib 74xGxx) (part 74AUC2G07) (description "Dual Buffer w/ Open Drain, Low-Voltage CMOS"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 60DE39C3))
    (comp (ref C7)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 612A6155))
    (comp (ref R5)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 612A615E))
    (comp (ref R6)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 612A6166))
    (comp (ref U_INT3)
      (value 74LVC2G07)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet https://www.diodes.com/assets/Datasheets/74LVC2G07.pdf)
      (fields
        (field (name MPN) SN74LVC2G07DBVR))
      (libsource (lib 74xGxx) (part 74AUC2G07) (description "Dual Buffer w/ Open Drain, Low-Voltage CMOS"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 612A617C))
    (comp (ref C8)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sbus/) (tstamps /5F679B53/))
      (tstamp 612BD908))
    (comp (ref JAB1)
      (value ZTEX_AB-ztex_AB)
      (footprint For_SeeedStudio:PinHeader_2x32_P2.54mm_Vertical_For_SeeedStudio)
      (fields
        (field (name MPN) 10-89-7642)
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/10-89-7642?qs=%2Fha2pyFadugCxzQFZUdvioDcljDVidgd4vXrOFuSRYM%3D))
      (libsource (lib ztex_AB) (part ZTEX_AB) (description ""))
      (sheetpath (names /B2B/) (tstamps /5F67E4B9/))
      (tstamp 5F676E85))
    (comp (ref ROE1)
      (value 549)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF5490T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /B2B/) (tstamps /5F67E4B9/))
      (tstamp 5F6BAF48))
    (comp (ref DOE1)
      (value RED)
      (footprint LED_SMD:LED_0805_2012Metric)
      (datasheet https://optoelectronics.liteon.com/upload/download/DS-22-99-0150/LTST-C170KRKT.pdf)
      (fields
        (field (name Digikey) 160-1415-1-ND)
        (field (name Koncar) FV007)
        (field (name LCSC) C94868)
        (field (name MNF1_URL) www.liteon.com)
        (field (name MPN) LTST-C170KRKT)
        (field (name Mouse_r2) 743-IN-S85ATR)
        (field (name Mouser) 859-LTST-C170KRKT)
        (field (name Side) TB)
        (field (name price400_LCSC) 0.0195$))
      (libsource (lib Device) (part LED_ALT) (description "Light emitting diode, filled shape"))
      (sheetpath (names /B2B/) (tstamps /5F67E4B9/))
      (tstamp 5F6BAF59))
    (comp (ref J1)
      (value Conn_01x06_Male)
      (footprint For_SeeedStudio:PinHeader_1x06_P2.54mm_Horizontal_For_SeeedStudio)
      (datasheet ~)
      (fields
        (field (name MPN) PZ254R-11-06P)
        (field (name MPN-ALT) 22-28-8060)
        (field (name URL) https://lcsc.com/product-detail/Pin-Header-Female-Header_XFCN-PZ254R-11-06P_C492414.html)
        (field (name URL-ALT) https://www2.mouser.com/ProductDetail/Molex/22-28-8060?qs=4XSMV6Twtb2rYD%2F%2F316gfQ==))
      (libsource (lib Connector) (part Conn_01x06_Male) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /B2B/) (tstamps /5F67E4B9/))
      (tstamp 5F69129B))
    (comp (ref JCD1)
      (value ZTEX_CD-ztex_CD)
      (footprint For_SeeedStudio:PinHeader_2x32_P2.54mm_Vertical_For_SeeedStudio)
      (fields
        (field (name MPN) 10-89-7642)
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/10-89-7642?qs=%2Fha2pyFadugCxzQFZUdvioDcljDVidgd4vXrOFuSRYM%3D))
      (libsource (lib ztex_CD) (part ZTEX_CD) (description ""))
      (sheetpath (names /B2B/) (tstamps /5F67E4B9/))
      (tstamp 5F676F65))
    (comp (ref J3)
      (value Conn_02x07_Odd_Even)
      (footprint For_SeeedStudio:PinHeader_2x07_P2.00mm_Horizontal_For_SeeedStudio)
      (datasheet https://www.molex.com/pdm_docs/sd/878331420_sd.pdf)
      (fields
        (field (name MPN) 87833-1420)
        (field (name MPN-ALT) A2005WR-N-2X7P-B)
        (field (name URL) https://www2.mouser.com/ProductDetail/Molex/87833-1420?qs=%2Fha2pyFadujYFYCIYI1IvFCvLi7no9WQYzIL%2FpYxKhg%3D))
      (libsource (lib Connector_Generic) (part Conn_02x07_Odd_Even) (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /B2B/) (tstamps /5F67E4B9/))
      (tstamp 5F749BE1))
    (comp (ref J5)
      (value Conn_02x06_Odd_Even)
      (footprint For_SeeedStudio:PinSocket_2x06_P2.54mm_Horizontal_For_SeeedStudio)
      (datasheet ~)
      (fields
        (field (name MPN) A2541HWR-2x6P)
        (field (name URL) https://lcsc.com/product-detail/Pin-Header-Female-Header_Changjiang-Connectors-A2541HWR-2x6P_C239357.html))
      (libsource (lib Connector_Generic) (part Conn_02x06_Odd_Even) (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /blinkey/) (tstamps /5F6B165A/))
      (tstamp 60D925D5))
    (comp (ref J6)
      (value Conn_01x03_Male)
      (footprint Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name MPN) 640456-3)
        (field (name MPN-ALT) 22-27-2031)
        (field (name Manufacturer) "TE Connectivity")
        (field (name Manufacturer-ALT) Molex)
        (field (name URL-ALT) https://www.mouser.fr/ProductDetail/Molex/22-27-2031?qs=%2Fha2pyFadugXOaGYK9vaczm7nZ04txhJn3OGcnGWT3U=))
      (libsource (lib Connector) (part Conn_01x03_Male) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /blinkey/) (tstamps /5F6B165A/))
      (tstamp 60E1E49E))
    (comp (ref C6)
      (value 47uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (fields
        (field (name MPN) GRM21BR60J476ME15L))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /blinkey/) (tstamps /5F6B165A/))
      (tstamp 60E24715))
    (comp (ref C9)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /blinkey/) (tstamps /5F6B165A/))
      (tstamp 612C3C5C))
    (comp (ref C1)
      (value 47uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (fields
        (field (name MPN) GRM21BR60J476ME15L))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sdcard.sch/) (tstamps /5F69F4EF/))
      (tstamp 590C7447))
    (comp (ref J2)
      (value 47219-2001)
      (footprint MOLEX_47219-2001:MOLEX_47219-2001)
      (datasheet https://www.molex.com/webdocs/datasheets/pdf/en-us/0472192001_MEMORY_CARD_SOCKET.pdf)
      (fields
        (field (name MPN) 47219-2001))
      (libsource (lib 47219-2001) (part 47219-2001) (description ""))
      (sheetpath (names /sdcard.sch/) (tstamps /5F69F4EF/))
      (tstamp 5F6F557B))
    (comp (ref C2)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /sdcard.sch/) (tstamps /5F69F4EF/))
      (tstamp 60D77AD6))
    (comp (ref J4)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_Molex-105017-0001)
      (datasheet https://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
      (fields
        (field (name Description) "CONN RCPT USB2.0 MICRO B SMD R/A")
        (field (name Digi-Key_PN) WM1399CT-ND)
        (field (name MPN) 1050170001)
        (field (name Manufacturer) Molex)
        (field (name URL) https://eu.mouser.com/ProductDetail/Molex/105017-0001?qs=hlXxxvYE36k7QcsR97GUKA%3D%3D))
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A6A3))
    (comp (ref R19)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A6C2))
    (comp (ref R18)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1002T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A6CD))
    (comp (ref C5)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A6E1))
    (comp (ref U5)
      (value SN65220)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet http://www.ti.com/lit/ds/symlink/sn65220.pdf)
      (fields
        (field (name MPN) SN65220DBVR))
      (libsource (lib Power_Protection) (part SN65220) (description "USB port transient suppressors"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A6FD))
    (comp (ref R14)
      (value 15k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1502T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A70F))
    (comp (ref R15)
      (value 15k)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF1502T5E))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A717))
    (comp (ref R9)
      (value 27)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF270JT5E)
        (field (name MPN-ALT) ERJ-3EKF27R0V))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A72D))
    (comp (ref R10)
      (value 27)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name MPN) 0603WAF270JT5E)
        (field (name MPN-ALT) ERJ-3EKF27R0V))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A735))
    (comp (ref C3)
      (value 150uF)
      (footprint Capacitor_SMD:C_1206_3216Metric)
      (datasheet ~)
      (fields
        (field (name MPN) GRM31CR60J157ME11L))
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A750))
    (comp (ref FB1)
      (value Ferrite_Bead_Small)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (datasheet ~)
      (fields
        (field (name MPN) PZ2012U221-2R0TF)
        (field (name MPN-ALT) 742792022))
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A758))
    (comp (ref C14)
      (value 100nF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (fields
        (field (name Digikey) ?)
        (field (name Koncar) ?)
        (field (name LCSC) ?)
        (field (name MNF1_URL) www.yageo.com)
        (field (name MPN) CC0603KRX7R8BB104)
        (field (name Mouser) 603-CC603KRX7R8BB104)
        (field (name Side) TB))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 612D3A06))
    (comp (ref U7)
      (value TPS2051C)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (fields
        (field (name MPN) TPS2051CDBVR)
        (field (name "Mouser No") 595-TPS2051CDBVR)
        (field (name URL) https://www.mouser.fr/ProductDetail/Texas-Instruments/TPS2051CDBVR?qs=PF3AD18CSE5vi2HeWLJCmw%3D%3D))
      (libsource (lib Power_Management) (part TPS2041B) (description "Single power-distribution switcher"))
      (sheetpath (names /USB/) (tstamps /60D72F2C/))
      (tstamp 60D9A6AC)))
  (libparts
    (libpart (lib 47219-2001) (part 47219-2001)
      (fields
        (field (name Reference) J)
        (field (name Value) 47219-2001)
        (field (name Footprint) MOLEX_47219-2001)
        (field (name Datasheet) MOLEX))
      (pins
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name CD/DAT3) (type BiDi))
        (pin (num 3) (name CMD) (type BiDi))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type BiDi))
        (pin (num 8) (name DAT1) (type BiDi))
        (pin (num G1) (name GND@1) (type power_in))
        (pin (num G2) (name GND@2) (type power_in))
        (pin (num G3) (name GND@3) (type power_in))
        (pin (num G4) (name GND@4) (type power_in))))
    (libpart (lib 74xGxx) (part 74LVC2G07)
      (aliases
        (alias 74AUC2G07))
      (description "Dual Buffer w/ Open Drain, Low-Voltage CMOS")
      (docs http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf)
      (footprints
        (fp SG-*)
        (fp SOT*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LVC2G07))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type openCol))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name ~) (type openCol))))
    (libpart (lib Connector) (part Conn_01x03_Male)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector) (part Conn_01x06_Male)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x06_Odd_Even)
      (description "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x06_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x07_Odd_Even)
      (description "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x07_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead_Small)
      (description "Ferrite bead, small symbol")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part LED_ALT)
      (description "Light emitting diode, filled shape")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_ALT))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Power_Management) (part TPS2041B)
      (description "Single power-distribution switcher")
      (docs http://www.ti.com/lit/ds/symlink/tps2041.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS2041B)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name OUT) (type power_out))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name ~OC) (type openCol))
        (pin (num 4) (name ~EN) (type input))
        (pin (num 5) (name IN) (type power_in))))
    (libpart (lib Power_Protection) (part SN65220)
      (description "USB port transient suppressors")
      (docs http://www.ti.com/lit/ds/symlink/sn65220.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) SN65220)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name ~) (type NotConnected))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name ~) (type NotConnected))
        (pin (num 4) (name B) (type passive))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name A) (type passive))))
    (libpart (lib SBUS) (part SBus)
      (footprints
        (fp FCN-234P096-GY))
      (fields
        (field (name Reference) SBus)
        (field (name Value) SBus))
      (pins
        (pin (num 01) (name GND) (type passive))
        (pin (num 02) (name BR*) (type BiDi))
        (pin (num 03) (name SEL*) (type BiDi))
        (pin (num 04) (name INT[1]*) (type BiDi))
        (pin (num 05) (name D[00]) (type BiDi))
        (pin (num 06) (name D[02]) (type BiDi))
        (pin (num 07) (name D[04]) (type BiDi))
        (pin (num 08) (name INT[2]*) (type BiDi))
        (pin (num 09) (name D[06]) (type BiDi))
        (pin (num 10) (name D[08]) (type BiDi))
        (pin (num 11) (name D[10]) (type BiDi))
        (pin (num 12) (name INT[3]*) (type BiDi))
        (pin (num 13) (name D[12]) (type BiDi))
        (pin (num 14) (name D[14]) (type BiDi))
        (pin (num 15) (name D[16]) (type BiDi))
        (pin (num 16) (name INT[4]*) (type BiDi))
        (pin (num 17) (name D[19]) (type BiDi))
        (pin (num 18) (name D[21]) (type BiDi))
        (pin (num 19) (name D[23]) (type BiDi))
        (pin (num 20) (name INT[5]*) (type BiDi))
        (pin (num 21) (name D[25]) (type BiDi))
        (pin (num 22) (name D[27]) (type BiDi))
        (pin (num 23) (name D[29]) (type BiDi))
        (pin (num 24) (name INT[6]*) (type BiDi))
        (pin (num 25) (name D[31]) (type BiDi))
        (pin (num 26) (name SIZ[0]) (type BiDi))
        (pin (num 27) (name SIZ[2]) (type BiDi))
        (pin (num 28) (name INT[7]*) (type BiDi))
        (pin (num 29) (name PA[00]) (type BiDi))
        (pin (num 30) (name PA[02]) (type BiDi))
        (pin (num 31) (name PA[04]) (type BiDi))
        (pin (num 32) (name EER*) (type BiDi))
        (pin (num 33) (name PA[06]) (type BiDi))
        (pin (num 34) (name PA[08]) (type BiDi))
        (pin (num 35) (name PA[10]) (type BiDi))
        (pin (num 36) (name ACK[0]*) (type BiDi))
        (pin (num 37) (name PA[12]) (type BiDi))
        (pin (num 38) (name PA[14]) (type BiDi))
        (pin (num 39) (name PA[16]) (type BiDi))
        (pin (num 40) (name ACK[1]*) (type BiDi))
        (pin (num 41) (name PA[18]) (type BiDi))
        (pin (num 42) (name PA[20]) (type BiDi))
        (pin (num 43) (name PA[22]) (type BiDi))
        (pin (num 44) (name ACK[2]*) (type BiDi))
        (pin (num 45) (name PA[24]) (type BiDi))
        (pin (num 46) (name PA[26]) (type BiDi))
        (pin (num 47) (name DP) (type BiDi))
        (pin (num 48) (name -12V) (type power_in))
        (pin (num 49) (name CLK) (type BiDi))
        (pin (num 50) (name BG*) (type BiDi))
        (pin (num 51) (name AS*) (type BiDi))
        (pin (num 52) (name GND) (type passive))
        (pin (num 53) (name D[01]) (type BiDi))
        (pin (num 54) (name D[03]) (type BiDi))
        (pin (num 55) (name D[05]) (type BiDi))
        (pin (num 56) (name +5V) (type power_in))
        (pin (num 57) (name D[07]) (type BiDi))
        (pin (num 58) (name D[09]) (type BiDi))
        (pin (num 59) (name D[11]) (type BiDi))
        (pin (num 60) (name GND) (type passive))
        (pin (num 61) (name D[13]) (type BiDi))
        (pin (num 62) (name D[15]) (type BiDi))
        (pin (num 63) (name D[17]) (type BiDi))
        (pin (num 64) (name +5V) (type power_in))
        (pin (num 65) (name D[18]) (type BiDi))
        (pin (num 66) (name D[20]) (type BiDi))
        (pin (num 67) (name D[22]) (type BiDi))
        (pin (num 68) (name GND) (type passive))
        (pin (num 69) (name D[24]) (type BiDi))
        (pin (num 70) (name D[26]) (type BiDi))
        (pin (num 71) (name D[28]) (type BiDi))
        (pin (num 72) (name +5V) (type power_in))
        (pin (num 73) (name D[30]) (type BiDi))
        (pin (num 74) (name SIZ[1]) (type BiDi))
        (pin (num 75) (name PPRD) (type BiDi))
        (pin (num 76) (name GND) (type passive))
        (pin (num 77) (name PA[01]) (type BiDi))
        (pin (num 78) (name PA[03]) (type BiDi))
        (pin (num 79) (name PA[05]) (type BiDi))
        (pin (num 80) (name +5V) (type power_in))
        (pin (num 81) (name PA[07]) (type BiDi))
        (pin (num 82) (name PA[09]) (type BiDi))
        (pin (num 83) (name PA[11]) (type BiDi))
        (pin (num 84) (name GND) (type passive))
        (pin (num 85) (name PA[13]) (type BiDi))
        (pin (num 86) (name PA[15]) (type BiDi))
        (pin (num 87) (name PA[17]) (type BiDi))
        (pin (num 88) (name +5V) (type power_in))
        (pin (num 89) (name PA[19]) (type BiDi))
        (pin (num 90) (name PA[21]) (type BiDi))
        (pin (num 91) (name PA[23]) (type BiDi))
        (pin (num 92) (name GND) (type passive))
        (pin (num 93) (name PA[25]) (type BiDi))
        (pin (num 94) (name PA[27]) (type BiDi))
        (pin (num 95) (name RST*) (type BiDi))
        (pin (num 96) (name +12V) (type power_in))))
    (libpart (lib ul_SN74CB3T16211DGGR) (part SN74CB3T16211DGGR)
      (fields
        (field (name Reference) U)
        (field (name Value) SN74CB3T16211DGGR))
      (pins
        (pin (num 1) (name NC) (type unspc))
        (pin (num 2) (name 1A1) (type BiDi))
        (pin (num 3) (name 1A2) (type BiDi))
        (pin (num 4) (name 1A3) (type BiDi))
        (pin (num 5) (name 1A4) (type BiDi))
        (pin (num 6) (name 1A5) (type BiDi))
        (pin (num 7) (name 1A6) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name 1A7) (type BiDi))
        (pin (num 10) (name 1A8) (type BiDi))
        (pin (num 11) (name 1A9) (type BiDi))
        (pin (num 12) (name 1A10) (type BiDi))
        (pin (num 13) (name 1A11) (type BiDi))
        (pin (num 14) (name 1A12) (type BiDi))
        (pin (num 15) (name 2A1) (type power_in))
        (pin (num 16) (name 2A2) (type BiDi))
        (pin (num 17) (name VCC) (type power_in))
        (pin (num 18) (name 2A3) (type BiDi))
        (pin (num 19) (name GND) (type power_in))
        (pin (num 20) (name 2A4) (type BiDi))
        (pin (num 21) (name 2A5) (type BiDi))
        (pin (num 22) (name 2A6) (type BiDi))
        (pin (num 23) (name 2A7) (type BiDi))
        (pin (num 24) (name 2A8) (type BiDi))
        (pin (num 25) (name 2A9) (type BiDi))
        (pin (num 26) (name 2A10) (type BiDi))
        (pin (num 27) (name 2A11) (type BiDi))
        (pin (num 28) (name 2A12) (type BiDi))
        (pin (num 29) (name 2B12) (type BiDi))
        (pin (num 30) (name 2B11) (type BiDi))
        (pin (num 31) (name 2B10) (type BiDi))
        (pin (num 32) (name 2B9) (type BiDi))
        (pin (num 33) (name 2B8) (type BiDi))
        (pin (num 34) (name 2B7) (type BiDi))
        (pin (num 35) (name 2B6) (type BiDi))
        (pin (num 36) (name 2B5) (type BiDi))
        (pin (num 37) (name 2B4) (type BiDi))
        (pin (num 38) (name GND) (type power_in))
        (pin (num 39) (name 2B3) (type BiDi))
        (pin (num 40) (name 2B2) (type BiDi))
        (pin (num 41) (name 2B1) (type BiDi))
        (pin (num 42) (name 1B12) (type BiDi))
        (pin (num 43) (name 1B11) (type BiDi))
        (pin (num 44) (name 1B10) (type BiDi))
        (pin (num 45) (name 1B9) (type BiDi))
        (pin (num 46) (name 1B8) (type BiDi))
        (pin (num 47) (name 1B7) (type BiDi))
        (pin (num 48) (name 1B6) (type BiDi))
        (pin (num 49) (name GND) (type power_in))
        (pin (num 50) (name 1B5) (type BiDi))
        (pin (num 51) (name 1B4) (type BiDi))
        (pin (num 52) (name 1B3) (type BiDi))
        (pin (num 53) (name 1B2) (type BiDi))
        (pin (num 54) (name 1B1) (type BiDi))
        (pin (num 55) (name *2OE) (type input))
        (pin (num 56) (name *1OE) (type input))))
    (libpart (lib ul_SN74CB3T3125PW) (part SN74CB3T3125PW)
      (footprints
        (fp PW14)
        (fp PW14-M)
        (fp PW14-L))
      (fields
        (field (name Reference) U)
        (field (name Value) SN74CB3T3125PW)
        (field (name Footprint) PW14))
      (pins
        (pin (num 1) (name *1OE) (type input))
        (pin (num 2) (name 1A) (type input))
        (pin (num 3) (name 1B) (type input))
        (pin (num 4) (name *2OE) (type input))
        (pin (num 5) (name 2A) (type input))
        (pin (num 6) (name 2B) (type input))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name 3B) (type input))
        (pin (num 9) (name 3A) (type input))
        (pin (num 10) (name *3OE) (type input))
        (pin (num 11) (name 4B) (type input))
        (pin (num 12) (name 4A) (type input))
        (pin (num 13) (name *4OE) (type input))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib ztex_AB) (part ZTEX_AB)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) ZTEX_AB))
      (pins
        (pin (num 1) (name VIN) (type passive))
        (pin (num 2) (name VIN) (type passive))
        (pin (num 3) (name GND) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name K16~IO_25_15) (type passive))
        (pin (num 6) (name J18~IO_L23N_T3_FWE_B_15) (type passive))
        (pin (num 7) (name K15~IO_L24P_T3_RS1_15) (type passive))
        (pin (num 8) (name J17~IO_L23P_T3_FOE_B_15) (type passive))
        (pin (num 9) (name J15~IO_L24N_T3_RS0_15) (type passive))
        (pin (num 10) (name K13~IO_L17P_T2_A26_15) (type passive))
        (pin (num 11) (name H15~IO_L19N_T3_A21_VREF_15) (type passive))
        (pin (num 12) (name J13~IO_L17N_T2_A25_15) (type passive))
        (pin (num 13) (name J14~IO_L19P_T3_A22_15) (type passive))
        (pin (num 14) (name H14~IO_L15P_T2_DQS_15) (type passive))
        (pin (num 15) (name H17~IO_L18P_T2_A24_15) (type passive))
        (pin (num 16) (name G14~IO_L15N_T2_DQS_ADV_B_15) (type passive))
        (pin (num 17) (name G17~IO_L18N_T2_A23_15) (type passive))
        (pin (num 18) (name G16~IO_L13N_T2_MRCC_15) (type passive))
        (pin (num 19) (name G18~IO_L22P_T3_A17_15) (type passive))
        (pin (num 20) (name H16~IO_L13P_T2_MRCC_15) (type passive))
        (pin (num 21) (name F18~IO_L22N_T3_A16_15) (type passive))
        (pin (num 22) (name F16~IO_L14N_T2_SRCC_15) (type passive))
        (pin (num 23) (name E18~IO_L21P_T3_DQS_15) (type passive))
        (pin (num 24) (name F15~IO_L14P_T2_SRCC_15) (type passive))
        (pin (num 25) (name D18~IO_L21N_T3_DQS_A18_15) (type passive))
        (pin (num 26) (name E17~IO_L16P_T2_A28_15) (type passive))
        (pin (num 27) (name G13~IO_0_15) (type passive))
        (pin (num 28) (name D17~IO_L16N_T2_A27_15) (type passive))
        (pin (num 29) (name 3.3V) (type passive))
        (pin (num 30) (name 3.3V) (type passive))
        (pin (num 31) (name GND) (type passive))
        (pin (num 32) (name GND) (type passive))
        (pin (num 33) (name VCCO_AB) (type passive))
        (pin (num 34) (name VCCO_AB) (type passive))
        (pin (num 35) (name F13~IO_L5P_T0_AD9P_15) (type passive))
        (pin (num 36) (name F14~IO_L5N_T0_AD9N_15) (type passive))
        (pin (num 37) (name E16~IO_L11N_T1_SRCC_15) (type passive))
        (pin (num 38) (name E15~IO_L11P_T1_SRCC_15) (type passive))
        (pin (num 39) (name C17~IO_L20N_T3_A19_15) (type passive))
        (pin (num 40) (name C16~IO_L20P_T3_A20_15) (type passive))
        (pin (num 41) (name A18~IO_L10N_T1_AD11N_15) (type passive))
        (pin (num 42) (name B18~IO_L10P_T1_AD11P_15) (type passive))
        (pin (num 43) (name C15~IO_L12N_T1_MRCC_15) (type passive))
        (pin (num 44) (name D15~IO_L12P_T1_MRCC_15) (type passive))
        (pin (num 45) (name B17~IO_L7N_T1_AD2N_15) (type passive))
        (pin (num 46) (name B16~IO_L7P_T1_AD2P_15) (type passive))
        (pin (num 47) (name C14~IO_L1N_T0_AD0N_15) (type passive))
        (pin (num 48) (name D14~IO_L1P_T0_AD0P_15) (type passive))
        (pin (num 49) (name D13~IO_L6N_T0_VREF_15) (type passive))
        (pin (num 50) (name D12~IO_L6P_T0_15) (type passive))
        (pin (num 51) (name A16~IO_L8N_T1_AD10N_15) (type passive))
        (pin (num 52) (name A15~IO_L8P_T1_AD10P_15) (type passive))
        (pin (num 53) (name B14~IO_L2N_T0_AD8N_15) (type passive))
        (pin (num 54) (name B13~IO_L2P_T0_AD8P_15) (type passive))
        (pin (num 55) (name B12~IO_L3N_T0_DQS_AD1N_15) (type passive))
        (pin (num 56) (name C12~IO_L3P_T0_DQS_AD1P_15) (type passive))
        (pin (num 57) (name A14~IO_L9N_T1_DQS_AD3N_15) (type passive))
        (pin (num 58) (name A13~IO_L9P_T1_DQS_AD3P_15) (type passive))
        (pin (num 59) (name B11~IO_L4P_T0_15) (type passive))
        (pin (num 60) (name A11~IO_L4N_T0_15) (type passive))
        (pin (num 61) (name JTAG_TDI) (type passive))
        (pin (num 62) (name JTAG_TCK) (type passive))
        (pin (num 63) (name JTAG_VIO) (type passive))
        (pin (num 64) (name GND) (type passive))))
    (libpart (lib ztex_CD) (part ZTEX_CD)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) ZTEX_CD))
      (pins
        (pin (num 1) (name USB_5V) (type passive))
        (pin (num 2) (name RESET#) (type passive))
        (pin (num 3) (name GND) (type passive))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name U9~IO_L21P_T3_DQS_34) (type passive))
        (pin (num 6) (name V9~IO_L21N_T3_DQS_34) (type passive))
        (pin (num 7) (name U8~IO_25_34) (type passive))
        (pin (num 8) (name V7~IO_L20P_T3_34) (type passive))
        (pin (num 9) (name U7~IO_L22P_T3_34) (type passive))
        (pin (num 10) (name V6~IO_L20N_T3_34) (type passive))
        (pin (num 11) (name U6~IO_L22N_T3_34) (type passive))
        (pin (num 12) (name V5~IO_L10P_T1_34) (type passive))
        (pin (num 13) (name T8~IO_L24N_T3_34) (type passive))
        (pin (num 14) (name V4~IO_L10N_T1_34) (type passive))
        (pin (num 15) (name R8~IO_L24P_T3_34) (type passive))
        (pin (num 16) (name T5~IO_L12P_T1_MRCC_34) (type passive))
        (pin (num 17) (name R7~IO_L23P_T3_34) (type passive))
        (pin (num 18) (name T4~IO_L12N_T1_MRCC_34) (type passive))
        (pin (num 19) (name T6~IO_L23N_T3_34) (type passive))
        (pin (num 20) (name U4~IO_L8P_T1_34) (type passive))
        (pin (num 21) (name R6~IO_L19P_T3_34) (type passive))
        (pin (num 22) (name U3~IO_L8N_T1_34) (type passive))
        (pin (num 23) (name R5~IO_L19N_T3_VREF_34) (type passive))
        (pin (num 24) (name V1~IO_L7N_T1_34) (type passive))
        (pin (num 25) (name V2~IO_L9N_T1_DQS_34) (type passive))
        (pin (num 26) (name U1~IO_L7P_T1_34) (type passive))
        (pin (num 27) (name U2~IO_L9P_T1_DQS_34) (type passive))
        (pin (num 28) (name T3~IO_L11N_T1_SRCC_34) (type passive))
        (pin (num 29) (name K6~IO_0_34) (type passive))
        (pin (num 30) (name R3~IO_L11P_T1_SRCC_34) (type passive))
        (pin (num 31) (name VCCO_CD) (type passive))
        (pin (num 32) (name VCCO_CD) (type passive))
        (pin (num 33) (name GND) (type passive))
        (pin (num 34) (name GND) (type passive))
        (pin (num 35) (name 3.3V) (type passive))
        (pin (num 36) (name 3.3V) (type passive))
        (pin (num 37) (name N6~IO_L18N_T2_34) (type passive))
        (pin (num 38) (name P5~IO_L13N_T2_MRCC_34) (type passive))
        (pin (num 39) (name M6~IO_L18P_T2_34) (type passive))
        (pin (num 40) (name N5~IO_L13P_T2_MRCC_34) (type passive))
        (pin (num 41) (name L6~IO_L6P_T0_34) (type passive))
        (pin (num 42) (name P4~IO_L14P_T2_SRCC_34) (type passive))
        (pin (num 43) (name L5~IO_L6N_T0_VREF_34) (type passive))
        (pin (num 44) (name P3~IO_L14N_T2_SRCC_34) (type passive))
        (pin (num 45) (name N4~IO_L16N_T2_34) (type passive))
        (pin (num 46) (name T1~IO_L17N_T2_34) (type passive))
        (pin (num 47) (name M4~IO_L16P_T2_34) (type passive))
        (pin (num 48) (name R1~IO_L17P_T2_34) (type passive))
        (pin (num 49) (name M3~IO_L4P_T0_34) (type passive))
        (pin (num 50) (name R2~IO_L15N_T2_DQS_34) (type passive))
        (pin (num 51) (name M2~IO_L4N_T0_34) (type passive))
        (pin (num 52) (name P2~IO_L15P_T2_DQS_34) (type passive))
        (pin (num 53) (name K5~IO_L5P_T0_34) (type passive))
        (pin (num 54) (name N2~IO_L3P_T0_DQS_34) (type passive))
        (pin (num 55) (name L4~IO_L5N_T0_34) (type passive))
        (pin (num 56) (name N1~IO_L3N_T0_DQS_34) (type passive))
        (pin (num 57) (name L3~IO_L2N_T0_34) (type passive))
        (pin (num 58) (name M1~IO_L1N_T0_34) (type passive))
        (pin (num 59) (name K3~IO_L2P_T0_34) (type passive))
        (pin (num 60) (name L1~IO_L1P_T0_34) (type passive))
        (pin (num 61) (name JTAG_TDO) (type passive))
        (pin (num 62) (name JTAG_TMS) (type passive))
        (pin (num 63) (name GND) (type passive))
        (pin (num 64) (name GND) (type passive)))))
  (libraries
    (library (logical 47219-2001)
      (uri /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/SBus/47219-2001.lib))
    (library (logical 74xGxx)
      (uri /usr/share/kicad/library/74xGxx.lib))
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Power_Management)
      (uri /usr/share/kicad/library/Power_Management.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical SBUS)
      (uri /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/SBus/SBUS.lib))
    (library (logical ul_SN74CB3T16211DGGR)
      (uri /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/SBus/ul_SN74CB3T16211DGGR.lib))
    (library (logical ul_SN74CB3T3125PW)
      (uri /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/SBus/ul_SN74CB3T3125PW.lib))
    (library (logical ztex_AB)
      (uri /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/ztex_AB.lib))
    (library (logical ztex_CD)
      (uri /home/dolbeau/SPARC/SBusFPGA/sbus-to-ztex/ztex_CD.lib)))
  (nets
    (net (code 1) (name SBUS_3V3_PA[07])
      (node (ref U2) (pin 29))
      (node (ref JAB1) (pin 53)))
    (net (code 2) (name SBUS_3V3_PA[06])
      (node (ref JAB1) (pin 52))
      (node (ref U2) (pin 30)))
    (net (code 3) (name SBUS_3V3_EER*)
      (node (ref JAB1) (pin 49))
      (node (ref U1) (pin 54)))
    (net (code 4) (name SBUS_OE)
      (node (ref U2) (pin 56))
      (node (ref R13) (pin 2))
      (node (ref JCD1) (pin 38))
      (node (ref U4) (pin 10))
      (node (ref U4) (pin 1))
      (node (ref U2) (pin 55))
      (node (ref U3) (pin 55))
      (node (ref U3) (pin 56))
      (node (ref U1) (pin 56))
      (node (ref U1) (pin 55)))
    (net (code 5) (name GND)
      (node (ref DOE1) (pin 1))
      (node (ref U3) (pin 38))
      (node (ref J1) (pin 1))
      (node (ref U_INT2) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref JAB1) (pin 32))
      (node (ref JAB1) (pin 4))
      (node (ref JCD1) (pin 64))
      (node (ref JCD1) (pin 3))
      (node (ref U3) (pin 49))
      (node (ref JCD1) (pin 63))
      (node (ref U_INT3) (pin 2))
      (node (ref J3) (pin 5))
      (node (ref J3) (pin 3))
      (node (ref J3) (pin 13))
      (node (ref U_INT3) (pin 2))
      (node (ref J3) (pin 11))
      (node (ref J3) (pin 1))
      (node (ref JAB1) (pin 31))
      (node (ref J3) (pin 7))
      (node (ref JAB1) (pin 3))
      (node (ref C4) (pin 2))
      (node (ref U_INT2) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref J3) (pin 9))
      (node (ref SBus1) (pin 92))
      (node (ref C9) (pin 2))
      (node (ref SBus1) (pin 76))
      (node (ref J5) (pin 3))
      (node (ref J2) (pin G3))
      (node (ref J2) (pin G2))
      (node (ref J2) (pin G1))
      (node (ref J2) (pin 6))
      (node (ref C1) (pin 2))
      (node (ref SBus1) (pin 52))
      (node (ref J2) (pin G4))
      (node (ref SBus1) (pin 60))
      (node (ref SBus1) (pin 68))
      (node (ref C2) (pin 2))
      (node (ref SBus1) (pin 84))
      (node (ref J5) (pin 4))
      (node (ref JCD1) (pin 33))
      (node (ref J6) (pin 1))
      (node (ref J6) (pin 3))
      (node (ref U3) (pin 19))
      (node (ref SBus1) (pin 01))
      (node (ref C31) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 7))
      (node (ref U4) (pin 6))
      (node (ref U4) (pin 5))
      (node (ref U_INT1) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref JCD1) (pin 4))
      (node (ref U_INT1) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref U2) (pin 49))
      (node (ref C11) (pin 2))
      (node (ref U2) (pin 38))
      (node (ref U3) (pin 8))
      (node (ref JAB1) (pin 64))
      (node (ref C14) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref U7) (pin 2))
      (node (ref U1) (pin 49))
      (node (ref R15) (pin 2))
      (node (ref J4) (pin 5))
      (node (ref J4) (pin 6))
      (node (ref U1) (pin 38))
      (node (ref U1) (pin 19))
      (node (ref U2) (pin 19))
      (node (ref C3) (pin 2))
      (node (ref JCD1) (pin 34))
      (node (ref U2) (pin 8))
      (node (ref C5) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref U5) (pin 5)))
    (net (code 6) (name SBUS_3V3_PA[05])
      (node (ref U2) (pin 31))
      (node (ref JAB1) (pin 51)))
    (net (code 7) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 8) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 9) (name SBUS_3V3_D[29])
      (node (ref U2) (pin 44))
      (node (ref JAB1) (pin 41)))
    (net (code 10) (name SBUS_3V3_PA[04])
      (node (ref U2) (pin 32))
      (node (ref JAB1) (pin 50)))
    (net (code 11) (name SBUS_3V3_PA[03])
      (node (ref JAB1) (pin 47))
      (node (ref U2) (pin 33)))
    (net (code 12) (name SBUS_3V3_PA[02])
      (node (ref U2) (pin 34))
      (node (ref JAB1) (pin 48)))
    (net (code 13) (name SBUS_3V3_PA[01])
      (node (ref JAB1) (pin 45))
      (node (ref U2) (pin 35)))
    (net (code 14) (name SBUS_3V3_PA[00])
      (node (ref U2) (pin 36))
      (node (ref JAB1) (pin 46)))
    (net (code 15) (name SBUS_3V3_PPRD)
      (node (ref JCD1) (pin 37))
      (node (ref U2) (pin 37)))
    (net (code 16) (name SBUS_3V3_SIZ[2])
      (node (ref JCD1) (pin 24))
      (node (ref U2) (pin 39)))
    (net (code 17) (name SBUS_3V3_SIZ[1])
      (node (ref JCD1) (pin 22))
      (node (ref U2) (pin 40)))
    (net (code 18) (name SBUS_3V3_SIZ[0])
      (node (ref U2) (pin 41))
      (node (ref JCD1) (pin 19)))
    (net (code 19) (name SBUS_3V3_D[31])
      (node (ref U2) (pin 42))
      (node (ref JAB1) (pin 43)))
    (net (code 20) (name SBUS_3V3_D[30])
      (node (ref U2) (pin 43))
      (node (ref JAB1) (pin 42)))
    (net (code 21) (name SBUS_3V3_PA[08])
      (node (ref JAB1) (pin 54))
      (node (ref U1) (pin 53)))
    (net (code 22) (name SBUS_3V3_D[28])
      (node (ref JAB1) (pin 40))
      (node (ref U2) (pin 45)))
    (net (code 23) (name SBUS_3V3_D[27])
      (node (ref JAB1) (pin 39))
      (node (ref U2) (pin 46)))
    (net (code 24) (name SBUS_3V3_D[26])
      (node (ref U2) (pin 47))
      (node (ref JAB1) (pin 38)))
    (net (code 25) (name SBUS_3V3_D[25])
      (node (ref U2) (pin 48))
      (node (ref JAB1) (pin 37)))
    (net (code 26) (name SBUS_3V3_D[24])
      (node (ref JAB1) (pin 36))
      (node (ref U2) (pin 50)))
    (net (code 27) (name SBUS_3V3_D[23])
      (node (ref U2) (pin 51))
      (node (ref JAB1) (pin 35)))
    (net (code 28) (name SBUS_3V3_D[22])
      (node (ref JAB1) (pin 28))
      (node (ref U2) (pin 52)))
    (net (code 29) (name SBUS_3V3_D[21])
      (node (ref U2) (pin 53))
      (node (ref JAB1) (pin 27)))
    (net (code 30) (name SBUS_3V3_D[20])
      (node (ref JAB1) (pin 26))
      (node (ref U2) (pin 54)))
    (net (code 31) (name +3V3)
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref JAB1) (pin 33))
      (node (ref JCD1) (pin 32))
      (node (ref JCD1) (pin 36))
      (node (ref JCD1) (pin 31))
      (node (ref J2) (pin 4))
      (node (ref C31) (pin 1))
      (node (ref JCD1) (pin 35))
      (node (ref JAB1) (pin 30))
      (node (ref JAB1) (pin 34))
      (node (ref JAB1) (pin 29))
      (node (ref U4) (pin 4))
      (node (ref U_INT3) (pin 5))
      (node (ref C8) (pin 1))
      (node (ref U4) (pin 13))
      (node (ref U4) (pin 14))
      (node (ref R13) (pin 1))
      (node (ref U1) (pin 17))
      (node (ref U_INT1) (pin 5))
      (node (ref R1) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref U3) (pin 17))
      (node (ref U_INT2) (pin 5))
      (node (ref C13) (pin 1))
      (node (ref U_INT3) (pin 5))
      (node (ref U_INT2) (pin 5))
      (node (ref R2) (pin 1))
      (node (ref U2) (pin 17))
      (node (ref C11) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref U_INT1) (pin 5))
      (node (ref C10) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref R30) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref J5) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 32) (name SBUS_5V_INT[4]*)
      (node (ref SBus1) (pin 16))
      (node (ref U_INT1) (pin 4)))
    (net (code 33) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 34) (name SBUS_3V3_INT[4]*)
      (node (ref U_INT1) (pin 3))
      (node (ref JCD1) (pin 40))
      (node (ref R31) (pin 2)))
    (net (code 35) (name SBUS_3V3_INT[3]*)
      (node (ref R30) (pin 2))
      (node (ref JCD1) (pin 30))
      (node (ref U_INT1) (pin 1)))
    (net (code 36) (name SBUS_5V_INT[3]*)
      (node (ref SBus1) (pin 12))
      (node (ref U_INT1) (pin 6)))
    (net (code 37) (name SBUS_3V3_PA[16])
      (node (ref U1) (pin 41))
      (node (ref JCD1) (pin 50)))
    (net (code 38) (name SBUS_3V3_PA[26])
      (node (ref U1) (pin 29))
      (node (ref JCD1) (pin 60)))
    (net (code 39) (name SBUS_3V3_PA[27])
      (node (ref JCD1) (pin 59))
      (node (ref U1) (pin 30)))
    (net (code 40) (name SBUS_3V3_PA[25])
      (node (ref U1) (pin 31))
      (node (ref JCD1) (pin 57)))
    (net (code 41) (name SBUS_3V3_PA[24])
      (node (ref JCD1) (pin 58))
      (node (ref U1) (pin 32)))
    (net (code 42) (name SBUS_3V3_PA[23])
      (node (ref U1) (pin 33))
      (node (ref JCD1) (pin 55)))
    (net (code 43) (name SBUS_3V3_PA[22])
      (node (ref JCD1) (pin 56))
      (node (ref U1) (pin 34)))
    (net (code 44) (name SBUS_3V3_PA[21])
      (node (ref JCD1) (pin 53))
      (node (ref U1) (pin 35)))
    (net (code 45) (name SBUS_3V3_PA[20])
      (node (ref U1) (pin 36))
      (node (ref JCD1) (pin 54)))
    (net (code 46) (name SBUS_3V3_PA[19])
      (node (ref JCD1) (pin 51))
      (node (ref U1) (pin 37)))
    (net (code 47) (name SBUS_3V3_PA[18])
      (node (ref U1) (pin 39))
      (node (ref JCD1) (pin 52)))
    (net (code 48) (name SBUS_3V3_PA[17])
      (node (ref JCD1) (pin 49))
      (node (ref U1) (pin 40)))
    (net (code 49) (name SBUS_3V3_ACK[2]*)
      (node (ref U1) (pin 42))
      (node (ref JCD1) (pin 45)))
    (net (code 50) (name SBUS_3V3_PA[15])
      (node (ref U1) (pin 43))
      (node (ref JCD1) (pin 47)))
    (net (code 51) (name SBUS_3V3_PA[14])
      (node (ref U1) (pin 44))
      (node (ref JAB1) (pin 60)))
    (net (code 52) (name SBUS_3V3_PA[13])
      (node (ref JAB1) (pin 59))
      (node (ref U1) (pin 45)))
    (net (code 53) (name SBUS_3V3_ACK[1]*)
      (node (ref JCD1) (pin 41))
      (node (ref U1) (pin 46)))
    (net (code 54) (name SBUS_3V3_PA[12])
      (node (ref JAB1) (pin 58))
      (node (ref U1) (pin 47)))
    (net (code 55) (name SBUS_3V3_PA[11])
      (node (ref U1) (pin 48))
      (node (ref JAB1) (pin 57)))
    (net (code 56) (name SBUS_3V3_PA[10])
      (node (ref JAB1) (pin 56))
      (node (ref U1) (pin 50)))
    (net (code 57) (name SBUS_3V3_ACK[0]*)
      (node (ref U1) (pin 51))
      (node (ref JCD1) (pin 39)))
    (net (code 58) (name SBUS_3V3_PA[09])
      (node (ref U1) (pin 52))
      (node (ref JAB1) (pin 55)))
    (net (code 59) (name SBUS_3V3_INT[1]*)
      (node (ref JCD1) (pin 23))
      (node (ref R2) (pin 2))
      (node (ref U_INT2) (pin 3)))
    (net (code 60) (name SBUS_3V3_INT[2]*)
      (node (ref JAB1) (pin 11))
      (node (ref R1) (pin 2))
      (node (ref U_INT2) (pin 1)))
    (net (code 61) (name SBUS_5V_INT[2]*)
      (node (ref SBus1) (pin 08))
      (node (ref U_INT2) (pin 6)))
    (net (code 62) (name SBUS_5V_INT[6]*)
      (node (ref U_INT3) (pin 6))
      (node (ref SBus1) (pin 24)))
    (net (code 63) (name SBUS_5V_INT[5]*)
      (node (ref U_INT3) (pin 4))
      (node (ref SBus1) (pin 20)))
    (net (code 64) (name SBUS_5V_INT[1]*)
      (node (ref SBus1) (pin 04))
      (node (ref U_INT2) (pin 4)))
    (net (code 65) (name SBUS_3V3_INT[5]*)
      (node (ref R6) (pin 2))
      (node (ref JCD1) (pin 43))
      (node (ref U_INT3) (pin 3)))
    (net (code 66) (name SBUS_3V3_INT[6]*)
      (node (ref R5) (pin 2))
      (node (ref JCD1) (pin 25))
      (node (ref U_INT3) (pin 1)))
    (net (code 67) (name SBUS_3V3_D[03])
      (node (ref JAB1) (pin 7))
      (node (ref U3) (pin 47)))
    (net (code 68) (name SBUS_3V3_D[13])
      (node (ref JAB1) (pin 19))
      (node (ref U3) (pin 35)))
    (net (code 69) (name SBUS_3V3_D[12])
      (node (ref JAB1) (pin 18))
      (node (ref U3) (pin 36)))
    (net (code 70) (name SBUS_3V3_D[11])
      (node (ref JAB1) (pin 17))
      (node (ref U3) (pin 37)))
    (net (code 71) (name SBUS_3V3_D[10])
      (node (ref U3) (pin 39))
      (node (ref JAB1) (pin 16)))
    (net (code 72) (name SBUS_3V3_D[09])
      (node (ref U3) (pin 40))
      (node (ref JAB1) (pin 15)))
    (net (code 73) (name SBUS_3V3_D[08])
      (node (ref JAB1) (pin 14))
      (node (ref U3) (pin 41)))
    (net (code 74) (name SBUS_3V3_D[07])
      (node (ref JAB1) (pin 13))
      (node (ref U3) (pin 42)))
    (net (code 75) (name SBUS_3V3_D[06])
      (node (ref U3) (pin 43))
      (node (ref JAB1) (pin 12)))
    (net (code 76) (name SBUS_3V3_D[04])
      (node (ref U3) (pin 44))
      (node (ref JAB1) (pin 10)))
    (net (code 77) (name SBUS_3V3_D[05])
      (node (ref U3) (pin 45))
      (node (ref JAB1) (pin 9)))
    (net (code 78) (name SBUS_3V3_D[02])
      (node (ref JAB1) (pin 8))
      (node (ref U3) (pin 46)))
    (net (code 79) (name SBUS_3V3_D[14])
      (node (ref U3) (pin 34))
      (node (ref JAB1) (pin 20)))
    (net (code 80) (name SBUS_3V3_D[00])
      (node (ref U3) (pin 48))
      (node (ref JAB1) (pin 6)))
    (net (code 81) (name SBUS_3V3_D[01])
      (node (ref U3) (pin 50))
      (node (ref JAB1) (pin 5)))
    (net (code 82) (name SBUS_3V3_CLK)
      (node (ref JAB1) (pin 44))
      (node (ref U3) (pin 51)))
    (net (code 83) (name SBUS_3V3_AS*)
      (node (ref JCD1) (pin 18))
      (node (ref U3) (pin 52)))
    (net (code 84) (name SBUS_3V3_SEL*)
      (node (ref JCD1) (pin 29))
      (node (ref U3) (pin 53)))
    (net (code 85) (name SBUS_3V3_RST*)
      (node (ref U3) (pin 54))
      (node (ref JCD1) (pin 27)))
    (net (code 86) (name SBUS_3V3_D[19])
      (node (ref JAB1) (pin 25))
      (node (ref U3) (pin 29)))
    (net (code 87) (name SBUS_3V3_D[18])
      (node (ref JAB1) (pin 24))
      (node (ref U3) (pin 30)))
    (net (code 88) (name SBUS_3V3_D[17])
      (node (ref U3) (pin 31))
      (node (ref JAB1) (pin 23)))
    (net (code 89) (name SBUS_3V3_D[16])
      (node (ref JAB1) (pin 22))
      (node (ref U3) (pin 32)))
    (net (code 90) (name SBUS_3V3_D[15])
      (node (ref JAB1) (pin 21))
      (node (ref U3) (pin 33)))
    (net (code 91) (name SBUS_3V3_BR*)
      (node (ref JCD1) (pin 21))
      (node (ref U4) (pin 3)))
    (net (code 92) (name SBUS_3V3_BG*)
      (node (ref JCD1) (pin 17))
      (node (ref U4) (pin 8)))
    (net (code 93) (name SBUS_5V_PA[20])
      (node (ref SBus1) (pin 42))
      (node (ref U1) (pin 21)))
    (net (code 94) (name SBUS_5V_PA[02])
      (node (ref SBus1) (pin 30))
      (node (ref U2) (pin 23)))
    (net (code 95) (name SBUS_5V_PA[04])
      (node (ref U2) (pin 25))
      (node (ref SBus1) (pin 31)))
    (net (code 96) (name SBUS_5V_EER*)
      (node (ref SBus1) (pin 32))
      (node (ref U1) (pin 2)))
    (net (code 97) (name SBUS_5V_PA[06])
      (node (ref U2) (pin 27))
      (node (ref SBus1) (pin 33)))
    (net (code 98) (name SBUS_5V_PA[08])
      (node (ref SBus1) (pin 34))
      (node (ref U1) (pin 3)))
    (net (code 99) (name SBUS_5V_PA[10])
      (node (ref U1) (pin 6))
      (node (ref SBus1) (pin 35)))
    (net (code 100) (name SBUS_5V_ACK[0]*)
      (node (ref SBus1) (pin 36))
      (node (ref U1) (pin 5)))
    (net (code 101) (name SBUS_5V_PA[12])
      (node (ref U1) (pin 9))
      (node (ref SBus1) (pin 37)))
    (net (code 102) (name SBUS_5V_PA[14])
      (node (ref SBus1) (pin 38))
      (node (ref U1) (pin 12)))
    (net (code 103) (name SBUS_5V_PA[16])
      (node (ref SBus1) (pin 39))
      (node (ref U1) (pin 15)))
    (net (code 104) (name SBUS_5V_ACK[1]*)
      (node (ref U1) (pin 10))
      (node (ref SBus1) (pin 40)))
    (net (code 105) (name SBUS_5V_PA[18])
      (node (ref SBus1) (pin 41))
      (node (ref U1) (pin 18)))
    (net (code 106) (name SBUS_5V_PA[00])
      (node (ref U2) (pin 21))
      (node (ref SBus1) (pin 29)))
    (net (code 107) (name SBUS_5V_PA[22])
      (node (ref U1) (pin 23))
      (node (ref SBus1) (pin 43)))
    (net (code 108) (name SBUS_5V_ACK[2]*)
      (node (ref SBus1) (pin 44))
      (node (ref U1) (pin 14)))
    (net (code 109) (name SBUS_5V_PA[24])
      (node (ref SBus1) (pin 45))
      (node (ref U1) (pin 25)))
    (net (code 110) (name SBUS_5V_PA[26])
      (node (ref U1) (pin 28))
      (node (ref SBus1) (pin 46)))
    (net (code 111) (name SBUS_5V_DP)
      (node (ref SBus1) (pin 47)))
    (net (code 112) (name SBUS_5V_-12V)
      (node (ref SBus1) (pin 48)))
    (net (code 113) (name SBUS_5V_CLK)
      (node (ref U3) (pin 5))
      (node (ref SBus1) (pin 49)))
    (net (code 114) (name SBUS_5V_BG*)
      (node (ref SBus1) (pin 50))
      (node (ref U4) (pin 9)))
    (net (code 115) (name SBUS_5V_AS*)
      (node (ref SBus1) (pin 51))
      (node (ref U3) (pin 4)))
    (net (code 116) (name SBUS_5V_D[01])
      (node (ref U3) (pin 6))
      (node (ref SBus1) (pin 53)))
    (net (code 117) (name SBUS_5V_D[19])
      (node (ref U3) (pin 28))
      (node (ref SBus1) (pin 17)))
    (net (code 118) (name SBUS_5V_D[00])
      (node (ref SBus1) (pin 05))
      (node (ref U3) (pin 7)))
    (net (code 119) (name SBUS_5V_D[02])
      (node (ref U3) (pin 10))
      (node (ref SBus1) (pin 06)))
    (net (code 120) (name SBUS_5V_D[04])
      (node (ref U3) (pin 12))
      (node (ref SBus1) (pin 07)))
    (net (code 121) (name SBUS_5V_D[06])
      (node (ref U3) (pin 13))
      (node (ref SBus1) (pin 09)))
    (net (code 122) (name SBUS_5V_D[08])
      (node (ref SBus1) (pin 10))
      (node (ref U3) (pin 15)))
    (net (code 123) (name SBUS_5V_D[10])
      (node (ref SBus1) (pin 11))
      (node (ref U3) (pin 18)))
    (net (code 124) (name SBUS_5V_D[12])
      (node (ref U3) (pin 21))
      (node (ref SBus1) (pin 13)))
    (net (code 125) (name SBUS_5V_D[14])
      (node (ref U3) (pin 23))
      (node (ref SBus1) (pin 14)))
    (net (code 126) (name SBUS_5V_D[16])
      (node (ref U3) (pin 25))
      (node (ref SBus1) (pin 15)))
    (net (code 127) (name SBUS_5V_D[03])
      (node (ref U3) (pin 9))
      (node (ref SBus1) (pin 54)))
    (net (code 128) (name SBUS_5V_D[21])
      (node (ref SBus1) (pin 18))
      (node (ref U2) (pin 3)))
    (net (code 129) (name SBUS_5V_D[23])
      (node (ref SBus1) (pin 19))
      (node (ref U2) (pin 5)))
    (net (code 130) (name SBUS_5V_D[25])
      (node (ref U2) (pin 7))
      (node (ref SBus1) (pin 21)))
    (net (code 131) (name SBUS_5V_D[27])
      (node (ref U2) (pin 10))
      (node (ref SBus1) (pin 22)))
    (net (code 132) (name SBUS_5V_D[29])
      (node (ref SBus1) (pin 23))
      (node (ref U2) (pin 12)))
    (net (code 133) (name SBUS_5V_D[31])
      (node (ref U2) (pin 14))
      (node (ref SBus1) (pin 25)))
    (net (code 134) (name SBUS_5V_SIZ[0])
      (node (ref SBus1) (pin 26))
      (node (ref U2) (pin 15)))
    (net (code 135) (name SBUS_5V_SIZ[2])
      (node (ref U2) (pin 18))
      (node (ref SBus1) (pin 27)))
    (net (code 136) (name SBUS_5V_PA[07])
      (node (ref SBus1) (pin 81))
      (node (ref U2) (pin 28)))
    (net (code 137) (name SBUS_5V_PA[09])
      (node (ref U1) (pin 4))
      (node (ref SBus1) (pin 82)))
    (net (code 138) (name SBUS_5V_PA[11])
      (node (ref U1) (pin 7))
      (node (ref SBus1) (pin 83)))
    (net (code 139) (name SBUS_5V_PA[13])
      (node (ref SBus1) (pin 85))
      (node (ref U1) (pin 11)))
    (net (code 140) (name SBUS_5V_PA[15])
      (node (ref SBus1) (pin 86))
      (node (ref U1) (pin 13)))
    (net (code 141) (name SBUS_5V_PA[17])
      (node (ref U1) (pin 16))
      (node (ref SBus1) (pin 87)))
    (net (code 142) (name SBUS_5V_PA[19])
      (node (ref U1) (pin 20))
      (node (ref SBus1) (pin 89)))
    (net (code 143) (name SBUS_5V_PA[21])
      (node (ref U1) (pin 22))
      (node (ref SBus1) (pin 90)))
    (net (code 144) (name SBUS_5V_PA[23])
      (node (ref U1) (pin 24))
      (node (ref SBus1) (pin 91)))
    (net (code 145) (name SBUS_5V_PA[05])
      (node (ref U2) (pin 26))
      (node (ref SBus1) (pin 79)))
    (net (code 146) (name SBUS_5V_PA[25])
      (node (ref SBus1) (pin 93))
      (node (ref U1) (pin 26)))
    (net (code 147) (name SBUS_5V_PA[27])
      (node (ref U1) (pin 27))
      (node (ref SBus1) (pin 94)))
    (net (code 148) (name SBUS_5V_RST*)
      (node (ref SBus1) (pin 95))
      (node (ref U3) (pin 2)))
    (net (code 149) (name SBUS_5V_+12V)
      (node (ref SBus1) (pin 96)))
    (net (code 150) (name SBUS_5V_INT[7]*)
      (node (ref SBus1) (pin 28)))
    (net (code 151) (name SBUS_5V_D[22])
      (node (ref SBus1) (pin 67))
      (node (ref U2) (pin 4)))
    (net (code 152) (name SBUS_5V_D[05])
      (node (ref U3) (pin 11))
      (node (ref SBus1) (pin 55)))
    (net (code 153) (name SBUS_5V_D[07])
      (node (ref SBus1) (pin 57))
      (node (ref U3) (pin 14)))
    (net (code 154) (name SBUS_5V_D[09])
      (node (ref U3) (pin 16))
      (node (ref SBus1) (pin 58)))
    (net (code 155) (name SBUS_5V_D[11])
      (node (ref U3) (pin 20))
      (node (ref SBus1) (pin 59)))
    (net (code 156) (name SBUS_5V_D[13])
      (node (ref U3) (pin 22))
      (node (ref SBus1) (pin 61)))
    (net (code 157) (name SBUS_5V_D[15])
      (node (ref SBus1) (pin 62))
      (node (ref U3) (pin 24)))
    (net (code 158) (name SBUS_5V_D[17])
      (node (ref U3) (pin 26))
      (node (ref SBus1) (pin 63)))
    (net (code 159) (name SBUS_5V_D[18])
      (node (ref U3) (pin 27))
      (node (ref SBus1) (pin 65)))
    (net (code 160) (name SBUS_5V_D[20])
      (node (ref U2) (pin 2))
      (node (ref SBus1) (pin 66)))
    (net (code 161) (name SBUS_5V_D[24])
      (node (ref SBus1) (pin 69))
      (node (ref U2) (pin 6)))
    (net (code 162) (name SBUS_5V_D[26])
      (node (ref SBus1) (pin 70))
      (node (ref U2) (pin 9)))
    (net (code 163) (name SBUS_5V_D[28])
      (node (ref U2) (pin 11))
      (node (ref SBus1) (pin 71)))
    (net (code 164) (name SBUS_5V_D[30])
      (node (ref U2) (pin 13))
      (node (ref SBus1) (pin 73)))
    (net (code 165) (name SBUS_5V_SIZ[1])
      (node (ref SBus1) (pin 74))
      (node (ref U2) (pin 16)))
    (net (code 166) (name SBUS_5V_PPRD)
      (node (ref SBus1) (pin 75))
      (node (ref U2) (pin 20)))
    (net (code 167) (name SBUS_5V_PA[01])
      (node (ref SBus1) (pin 77))
      (node (ref U2) (pin 22)))
    (net (code 168) (name SBUS_5V_PA[03])
      (node (ref U2) (pin 24))
      (node (ref SBus1) (pin 78)))
    (net (code 169) (name SBUS_5V_BR*)
      (node (ref U4) (pin 2))
      (node (ref SBus1) (pin 02)))
    (net (code 170) (name SBUS_5V_SEL*)
      (node (ref SBus1) (pin 03))
      (node (ref U3) (pin 3)))
    (net (code 172) (name +5V)
      (node (ref SBus1) (pin 64))
      (node (ref SBus1) (pin 80))
      (node (ref R18) (pin 2))
      (node (ref JAB1) (pin 2))
      (node (ref SBus1) (pin 56))
      (node (ref JAB1) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref SBus1) (pin 88))
      (node (ref SBus1) (pin 72))
      (node (ref J6) (pin 2))
      (node (ref U7) (pin 5))
      (node (ref R19) (pin 2))
      (node (ref C5) (pin 1)))
    (net (code 174) (name /B2B/JTAG_TDO)
      (node (ref J3) (pin 8)))
    (net (code 175) (name /B2B/JTAG_TCK)
      (node (ref J3) (pin 6)))
    (net (code 176) (name /B2B/JTAG_TMS)
      (node (ref J3) (pin 4)))
    (net (code 177) (name /B2B/JTAG_VIO)
      (node (ref J3) (pin 2)))
    (net (code 178) (name "Net-(J3-Pad14)")
      (node (ref J3) (pin 14)))
    (net (code 179) (name "Net-(J3-Pad12)")
      (node (ref J3) (pin 12)))
    (net (code 180) (name /B2B/JTAG_TDI)
      (node (ref J3) (pin 10)))
    (net (code 181) (name SD_CMD)
      (node (ref JCD1) (pin 16))
      (node (ref J2) (pin 3)))
    (net (code 182) (name SD_D1)
      (node (ref JCD1) (pin 14))
      (node (ref J2) (pin 8)))
    (net (code 183) (name SD_D0)
      (node (ref JCD1) (pin 12))
      (node (ref J2) (pin 7)))
    (net (code 184) (name SD_D3)
      (node (ref J2) (pin 2))
      (node (ref JCD1) (pin 10)))
    (net (code 185) (name /B2B/RX)
      (node (ref JCD1) (pin 5))
      (node (ref J1) (pin 4)))
    (net (code 186) (name PMOD-8)
      (node (ref JCD1) (pin 20))
      (node (ref J5) (pin 8)))
    (net (code 187) (name "Net-(JCD1-Pad2)")
      (node (ref JCD1) (pin 2)))
    (net (code 188) (name SD_CLK)
      (node (ref JCD1) (pin 15))
      (node (ref J2) (pin 5)))
    (net (code 189) (name PMOD-11)
      (node (ref J5) (pin 11))
      (node (ref JCD1) (pin 13)))
    (net (code 190) (name PMOD-12)
      (node (ref JCD1) (pin 11))
      (node (ref J5) (pin 12)))
    (net (code 191) (name USBH0_D-)
      (node (ref R10) (pin 2))
      (node (ref JCD1) (pin 9)))
    (net (code 192) (name USBH0_D+)
      (node (ref R9) (pin 2))
      (node (ref JCD1) (pin 7)))
    (net (code 193) (name /B2B/JTAG_TDO)
      (node (ref JCD1) (pin 61)))
    (net (code 194) (name PMOD-9)
      (node (ref J5) (pin 9))
      (node (ref JCD1) (pin 44)))
    (net (code 195) (name /B2B/JTAG_TMS)
      (node (ref JCD1) (pin 62)))
    (net (code 196) (name /B2B/TX)
      (node (ref J1) (pin 5))
      (node (ref JCD1) (pin 6)))
    (net (code 197) (name PMOD-5)
      (node (ref J5) (pin 5))
      (node (ref JCD1) (pin 48)))
    (net (code 198) (name PMOD-7)
      (node (ref J5) (pin 7))
      (node (ref JCD1) (pin 46)))
    (net (code 199) (name SD_D2)
      (node (ref J2) (pin 1))
      (node (ref JCD1) (pin 8)))
    (net (code 200) (name PMOD-10)
      (node (ref J5) (pin 10))
      (node (ref JCD1) (pin 42)))
    (net (code 201) (name PMOD-6)
      (node (ref JCD1) (pin 28))
      (node (ref J5) (pin 6)))
    (net (code 202) (name SBUS_DATA_OE_LED)
      (node (ref JCD1) (pin 26))
      (node (ref ROE1) (pin 1)))
    (net (code 205) (name /B2B/JTAG_TCK)
      (node (ref JAB1) (pin 62)))
    (net (code 206) (name /B2B/JTAG_VIO)
      (node (ref JAB1) (pin 63)))
    (net (code 207) (name /B2B/JTAG_TDI)
      (node (ref JAB1) (pin 61)))
    (net (code 208) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 209) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 210) (name /B2B/DATA_OE_LED)
      (node (ref DOE1) (pin 2))
      (node (ref ROE1) (pin 2)))
    (net (code 211) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 212) (name "Net-(JCD1-Pad1)")
      (node (ref JCD1) (pin 1)))
    (net (code 213) (name /USB/USB_D+)
      (node (ref R9) (pin 1))
      (node (ref J4) (pin 3))
      (node (ref U5) (pin 4))
      (node (ref R14) (pin 2)))
    (net (code 214) (name /USB/USB_D-)
      (node (ref J4) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref U5) (pin 6)))
    (net (code 215) (name /USB/USB_EN)
      (node (ref U7) (pin 4))
      (node (ref R18) (pin 1)))
    (net (code 216) (name /USB/USB_FLT)
      (node (ref U7) (pin 3))
      (node (ref R19) (pin 1)))
    (net (code 217) (name /USB/VBus)
      (node (ref FB1) (pin 1))
      (node (ref U7) (pin 1))
      (node (ref C14) (pin 1)))
    (net (code 218) (name /USB/VBus_USB0)
      (node (ref C3) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref FB1) (pin 2)))
    (net (code 219) (name "Net-(J4-Pad4)")
      (node (ref J4) (pin 4)))
    (net (code 220) (name "Net-(U5-Pad3)")
      (node (ref U5) (pin 3)))
    (net (code 221) (name "Net-(U5-Pad1)")
      (node (ref U5) (pin 1)))))